For 1990-2009 cars

### Removal Procedure

1. Disable the SIR System. Refer to Disabling the SIR System in SIR.
2. Remove the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
3. Remove the park brake lever cover.
4. Remove the park brake adjuster nut.
5. Remove the park brake cables from the equalizer assembly.
6. Pull the park brake lever to the highest position.
7. Lift the equalizer cable over the park brake indicator switch and swing it forward. Pull the cable down and out of the park brake lever.

### Installation Procedure

1. Slide the equalizer cable into the park brake lever. Hand start the adjuster nut.
2. Swing the equalizer cable rearward and lift over the park brake indicator switch.
3. Release and lower the park brake lever fully.
4. Install the rear park brake cables into the equalizer.
5. Adjust the park brake. Refer to Park Brake Adjustment .
6. Install the park brake cover.
7. Install the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
8. Enable SIR System. Refer to Enabling the SIR System in SIR.