For 1990-2009 cars

## Rear Wheelhouse Trim Finish Panel Replacement Wagon

### Removal Procedure

1. Remove the rear wheelhouse trim finish panel by pulling up at the clip locations to disengage the clips. Remove the trim panel.
2. Slip the shoulder belt out of the trim finish panel at the slit in the trim panel.

### Installation Procedure

1. Route the shoulder belt into the rear wheelhouse trim finish panel at the slit.
2. Position the trim finish panel to the vehicle. Push at the clip locations to engage the clips.
3. Check to make sure the shoulder belt is not twisted and operates properly.