For 1990-2009 cars

### General Information

The Saturn Security System provides an anti-theft feature for you vehicle. You will have the ability to lock and unlock your doors or release your trunk (liftgate for the wagon) when approaching or leaving your vehicle.

This feature will work from a distance of up to 26 ft. (8 m) using your key chain remote transmitter supplied with the Saturn Security System.

Additional features of the Saturn Security System include active security system arming, passive security system arming (programmed in by the retailer) and illuminated entry.

The Saturn Security System consists of a receiver, which is located in your vehicle, and two transmitters. The receiver can be programmed with up to four transmitters. Additional transmitters can be purchased at your vehicle retailer.

Your Saturn Security System operates on a radio frequency subject to Federal Communications Commission (FCC) Rules and with Industry Canada.

This device complies with Part 15 of the FCC Rules. Operation is subject to the following two conditions:

1. This device may not cause interference, and;
2. This device must accept any interference received, including interference that may cause undesired operation.

This device complies with RSS-210 of Industry Canada. Operation is subject to the following two conditions:

1. This device may not cause interference, and;
2. This device must accept any interference received, including interference that may cause undesired operation of the device.

Changes or modifications to this system by other than an authorized service facility could void authorization to use this equipment.