For 1990-2009 cars

### Removal Procedure

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

1. Raise the vehicle on hoist.
2. Remove the wheel and tire assembly.
3. Disconnect the brake hose from the caliper or wheel cylinder. Plug the opening in the caliper or wheel cylinder to avoid fluid loss and contamination.
4. Disconnect the brake hose from the brake pipe. Plug the opening in the brake pipe to avoid fluid loss and contamination.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the brake hose to the brake pipe.

Tighten
Tighten the fastener to 15 N·m (11 lb ft).

2. Install the brake hose to the caliper or wheel cylinder with new washers.

Tighten
Tighten the washers to 49 N·m (36 lb ft).

3. Bleed the brakes. Refer to Hydraulic Brake System Bleeding .
4. Check the connections for fluid leaks.

Notice: Before installing wheels, remove rust or corrosion from wheel mounting surfaces and brake rotors/drums. Failure to do so can cause wheel nuts to loosen in service.

5. Position the wheel onto the hub.
6. Install the wheel nuts and tighten in a crisscross pattern. Repeat the tightening pattern to be sure the torque is correct.

Tighten
Tighten the wheel nuts to 140 N·m (103 lb ft).

7. Lower the vehicle from the hoist.