For 1990-2009 cars

### Removal Procedure

1. Remove the driver's seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the seat back pad and seat cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .

### Installation Procedure

1. Position the seat back foam pad to the lumbar adjustment and frame assembly.
2. Install the seat back pad and cover to the frame and install the seat back to the seat bottom. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Install the driver's seat into the vehicle. Refer to Front Seat Replacement - Bucket .