For 1990-2009 cars

1. Turn the steering wheel so that the vehicle's wheels are pointed straight ahead.
2. Turn the ignition switch to the LOCK position and remove the key.
3. Connect the left and right curtain inflator module (YEL 2-way) connectors.

Notice: Be careful not to damage the VIN plate when removing or replacing the upper trim panel.

Important: Be sure the upper trim panel seal is correctly seated on the forward edge before installing the upper trim panel.

Important: LHD illustration shown, RHD similar.

4. Install the instrument panel upper trim panel.

4.1. | Ensure the hook-and-loop fastener attachments on the upper trim panel are correctly inserted.

4.2. | Position the upper trim panel on the retainer assembly.

4.3. | Align the tabs on the sides the of upper trim panel with the openings in the windshield garnish molding.

4.4. | Align the clips with the clip locations.

4.5. | Firmly snap in the clips at the clip locations.

Notice: Refer to Fastener Notice in the Preface section.

4.6. | Install the screws on underside of upper trim panel on passenger side of vehicle.

Tighten
Tighten the upper I/P trim panel fasteners to 6 N·m (53 lb in)

5. Connect the passenger (YEL 2-way) connector.
6. Attach the connector clip to the metal brace near the HVAC fan.

Important: LHD illustration shown, RHD similar.

7. Connect the driver (YEL 2-way) connector and clip to the steering column brace.
8. Install the AIR BAG fuse in IPFB.
9. Turn the ignition ON and verify the AIR BAG telltale operates properly.