For 1990-2009 cars

Caution: Failing to follow the following procedures could result in serious personal injury or property damage.

Always disconnect the negative battery (ground) lead when replacing components on a vehicle. Remove rings, watches and all other jewelry. When working around the battery, always shield your eyes. Avoid leaning over the battery if possible. Do not allow battery fluid to contact eyes, skin, fabrics or painted surfaces; battery fluid is a corrosive acid. Flush any contacted area with water immediately and thoroughly, and get medical help. Be careful that metal tools or jumper cables do not contact the positive battery terminal (or metal in contact with terminal) and any other metal on the vehicle; a short could occur. Do not expose a battery to open flames or sparks (including lit tobacco). Batteries produce a gas which is flammable and explosive. Never wear loose or baggy clothing around moving machinery. Remove ties and any hanging jewelry, and tie back long hair.