For 1990-2009 cars

### Removal Procedure

Important: LHD shown; RHD similar

1. Gently pry edges of ignition lock bezel with a blunt tool and separate from lower shroud.
2. Remove steering column shroud fasteners and remove steering column upper shroud.
3. Remove steering column lower shroud.

### Installation Procedure

1. Position steering column lower shroud to steering column.
2. Secure steering column upper and lower shrouds with shroud fasteners.

Tighten
Tighten Steering Column Shroud Fasteners 1.5 N·m (13 lbs in).

3. Install ignition bezel.

3.1. | Align peg of bezel with the cut-out in lower shroud.

3.2. | Snap into place.