For 1990-2009 cars

### Removal Procedure

1. Remove the compartment lid outer panel. Refer to Rear Compartment Lid Outer Panel .
2. Remove the retainer clip from the lock cylinder assembly.
3. Disconnect the lock rod from clip on the lock cylinder assembly. Remove the cylinder assembly.

### Installation Procedure

1. Attach the lock rod to the clip on the cylinder assembly. Position the lock cylinder assembly in the compartment lid.
2. Install the retainer clip, securing the lock cylinder assembly in place.
3. Install the compartment lid outer panel. Refer to Rear Compartment Lid Outer Panel .