For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Position the vehicle on the lift and raise the vehicle.
2. Disconnect the electrical connector from the speed sensor and remove the sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Inspect the O-ring for damage and replace if necessary.
2. Clean and lubricate the fastener with Saturn Transaxle Fluid. Wipe off the excess fluid and install.
3. Install the speed sensor.

Tighten
Tighten the vehicle speed sensor to 26 N·m (19 lb ft).

4. Connect the electrical connector to the speed sensor. Push in until a click is heard and pull back to confirm the positive engagement.
5. Lower the vehicle.
6. Check the transaxle fluid level. Refer to Transmission Fluid Check .