For 1990-2009 cars

### Removal Procedure

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

1. Position the vehicle on the hoist and ensure the ignition is OFF.

Notice: Refer to Vehicle Lifting Caution in the Preface section.

2. Raise the vehicle.

Important: Inspect the O-ring for damage and replace if necessary.

3. Disconnect the input speed sensor (ISS) harness connector and remove the sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Clean and lubricate the fastener with Saturn Transaxle Fluid. Wipe off excess fluid.

1. Install the ISS.

Tighten
Tighten the input speed sensor (ISS) to 26 N·m (19 lb ft).

2. Connect the ISS harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.
3. Lower the vehicle.
4. Inspect the transaxle fluid level.