For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door lower trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the rear side door inside handle fasteners and the handle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear side door inside handle and the fasteners.

Tighten
Tighten the inside rear handle screws (Coupe) to 5 N·m (44 lb in).

2. Install the rear side door lower trim panel. Refer to Rear Side Door Trim Panel Replacement .