For 1990-2009 cars

## Fascia Grille Replacement SL2/SW2

### Removal Procedure

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the fasteners from the fascia support brackets and energy absorber.
3. Remove the grille.

### Installation Procedure

1. Position the grille to the vehicle.
2. Install the fasteners to the fascia support brackets and energy absorber.
3. Install the front fascia. Refer to Front Bumper Fascia Replacement .