For 1990-2009 cars

## Quarter Window Garnish Molding Replacement Coupe Left Side 1st Design

### Removal Procedure

1. Remove the seat belt retractor cover by pulling.
2. Remove the coat hook. Refer to Coat Hook Replacement .
3. Remove the quarter window garnish upper molding by pulling. Refer to the following:

• | Quarter window garnish upper molding (1)

• | Interlock tab (2)

### Installation Procedure

1. Install the quarter window garnish upper molding. Refer to the following:

• | Quarter window garnish upper molding (1)

• | Interlock tab (2)

2. Install the seat belt retractor cover panel.
3. Install the coathook. Refer to Coat Hook Replacement .

## Quarter Window Garnish Molding Replacement Coupe Left Side 2nd Design

### Removal Procedure

Important: Before removing, note the position of the door weatherstrip over the edge of the quarter window garnish upper molding.

Remove the quarter window upper molding by pulling at the clip locations to disengage.

### Instatllation Procedure

1. Align the garnish molding clips and push to install.
2. Reposition the door weatherstrip over edge of the quarter window garnish upper molding.