For 1990-2009 cars

### Removal Procedure

1. Remove the steering column upper shroud.
2. Remove the ignition switch fasteners and switch.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical harness.
2. Position the ignition switch and install the fasteners.

Tighten
Tighten the ignition switch screws to 1.5 N·m (13.3 lb in).

3. Install the steering column upper shroud.