For 1990-2009 cars

### Removal Procedure

1. Remove the wheelhouse garnish molding. Refer to Garnish Molding Replacement - Wheelhouse in Interior Trim.
2. Remove the rear washer bottle fasteners.
3. Move the washer bottle away from the rear body and disconnect the washer pump connector.

Notice: Place a towel under washer pump to prevent washer fluid from spilling onto vehicle.

4. Remove the washer bottle from the vehicle.

### Installation Procedure

1. Transfer the washer pump to the new washer bottle. Refer to Washer Pump Replacement - Rear for the correct procedure.
2. Connect the washer fluid hose and the washer pump to the washer fluid bottle.
3. Install the washer bottle onto the studs in the rear body and install the fasteners.
4. Install the wheelhouse garnish molding. Refer to Garnish Molding Replacement - Wheelhouse in Interior Trim.