For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment floor trim and the rear compartment side wall trim.
2. Measure the following dimensions and mark the center of the mounting locations for the anchor bases. Remove the undercoating as necessary to ensure a clean surface for the anchor bases.

• | A from the rear end panel assembly, interior wall, of the rear compartment to the number 1 location.

• | B from the number 1 location to the number 2 location.

• | C from the rear end panel assembly to the number 2 location.

• | D from number 2 location to the number 3 location.

• | E from the bend in the quarter rear panel assembly, wheel housing, to the number 3 location.

• | F from the rear compartment floor to the number 4 location shock tower.

• | G from the number 4 to number 1 location.

Important: Mix part A and B of the adhesive according to the directions on the adhesive package. Each mixture of adhesive has enough adhesive for 4 anchor bases. Allow 24 hours cure time before installing the convenience nets into the base caps. Allow 48 hours before loading the convenience nets.

3. Apply the adhesive equally to each anchor base.
4. Install the anchor base at the anchor locations by pushing them into the surface and turning ½ turn.

Important: It is recommended that the anchor bases mounted on the vertical surfaces be temporarily secured with masking tape to prevent the anchor bases from creeping downward.

5. Allow the adhesive on the anchor bases to cure 1 hour at room temperature.
6. Using a razor knife, slit the rear compartment side wall trim to allow the studs on the mounting bases to pass through the rear compartment side wall trim. Install the rear compartment side wall trim.
7. Cut a small slit at the anchor bases on the rear compartment floor to allow the studs on the anchor bases to pass through the rear compartment floor trim. Install the rear compartment floor trim.
8. Install the anchor base caps onto the anchor bases. Tighten the caps finger tight.