For 1990-2009 cars

## Front Fog Lamp Replacement Coupe

### Removal Procedure

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement in Bumpers.
2. Remove the bulb.
3. Remove the retaining bolts from the front impact beam to the fog lamp bracket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the retaining bolts from the fog lamp bracket to the impact beam.

Tighten
Tighten the fog lamp bracket-to-impact beam bolts to 30 N·m (22 lb ft).

2. Install the bulb.
3. Install the front fascia. Refer to Front Bumper Fascia Replacement in Bumpers
4. Aim the fog lamp. Refer to "Fog Lamp Aiming" in Lighting Systems.

## Front Fog Lamp Replacement Sedan/Wagon

### Removal Procedure

1. Remove the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement in Lighting Systems.
2. Remove the nuts attaching the fog lamp bracket to the impact bar.
3. Remove the fog lamp assembly down through the bottom of the front fascia.

### Installation Procedure

1. Place the fog lamp assembly into position through the bottom of the front fascia.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts attaching the fog lamp bracket to the impact bar.

Tighten
Tighten the fog lamp bracket-to-impact bar attaching nuts to 30 N·m(22 lb ft).

3. Install the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement in Lighting Systems.
4. Aim the fog lamp. Refer to Fog Lamp Aiming in Lighting Systems.