For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Floor Console Refer to Front Floor Console Replacement .
2 | Center Console End Panel

#### Procedure

1. Using blunt trim tool release the retaining clips. Refer to Front Floor Console Side Trim Rear Panel Replacement .
2. Removing the end panel allows the removal of the air distribution duct (6).

3 | Side Impact Brace Screw (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
4 | Side Impact Brace
5 | Air Distribution Duct Screw (Qty: 3) Tighten 2 N·m (18 lb in)
6 | Air Distribution Duct
7 | Retainer Actuator Screw (Qty: 2) Tighten 1 N·m (9 lb in)
8 | Mode Actuator Connector
9 | Mode Actuator