For 1990-2009 cars

Important: Setting the camshaft timing is necessary whenever the camshaft drive system has been disturbed such that the relationship between any chain and sprocket has been lost. Even when only one sprocket is involved, multiple crankshaft rotations will not produce conditions where correct timing can be confirmed.

If necessary, follow the left bank secondary camshaft drive chain replacement procedures to reset the camshaft timing. Refer to Secondary Camshaft Drive Chain Replacement - Left Side.