For 1990-2009 cars

#### Universal Joint Noise (RWD)

Problem | Action
--- | ---
One or more of the universal joints are worn or damaged. | Replace the driveshaft complete.
One or more of the universal joints have lost lubricant. | Replace the driveshaft complete.
Rubber coupling bolts loose at transmission or axle flange. | Tighten the bolts to specifications. Refer to Fastener Tightening Specifications .
Bolts loose at driveshaft flange and coupling. | Tighten the bolts to specifications. Refer to Fastener Tightening Specifications .