For 1990-2009 cars

### Removal Procedure

1. Remove the overhead console. Refer to Roof Console Replacement .
2. Remove the screws (1) securing the sunroof switch to the overhead console.
3. Disconnect the electrical connector.

### Installation Procedure

1. Install the sunroof switch to the overhead console.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws (1) securing the sunroof switch to the overhead console.

Tighten
Tighten the screws to 1 N·m (2 lb in).

3. Connect the electrical connectors.
4. Install the overhead console. Refer to Roof Console Replacement .