For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Differential Case Shim Sizes | 3.5-4.4 mm | 0.14-0.17 in
Drive Pinion Housing Shim Sizes | 1.2-1.9 mm | 0.04-0.07 in
Drive Pinion Rotating Torque (w/Seals) | 2.5-4 N·m | 22-35 lb in
Ring Gear/Drive Pinion A1 Nominal Value - All Axles | 111.00 mm | 4.37 in
Ring Gear/Drive Pinion A2 Nominal Value - 3.42 Ratio Axles | 63.5 mm | 2.50 in
Ring Gear/Drive Pinion A2 Nominal Value - 2.73 Ration Axles | 63.5 mm | 2.50 in
Torsional Backlash

- 2.73 Ratio With 105 mm Flange

0.20-0.31 mm

0.007-0.012 in

- 3.42 Ratio With 105 mm Flange

0.24-0.38 mm

0.009-0.015 in