For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Vehicle stationary for at least 60 minutes/Tire pressures adjusted to recommended kPa/psi.
Battery Voltage | Data Display | Volts | 12.5
LF Pressure Sensor ID | Data Display | 8 digit number/Invalid | 8 digit number
LF Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/N/A | Stationary
LF Tire Pressure | Data Display | kPa/psi | Varies
LF Tire Pressure Sensor Status | Data Display | Valid/Invalid | Valid
LR Pressure Sensor ID | Data Display | 8 digit number/Invalid | 8 digit number
LR Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/N/A | Stationary
LR Tire Press | Data Display | kPa/psi | varies
LR Tire Pressure Sensor Status | Data Display | Valid/Invalid | Valid
RF Pressure Sensor ID | Data Display | 8 digit number/Invalid | 8 digit number
RF Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/N/A | Stationary
RF Tire Pressure | Data Display | kPa/psi | Varies
RF Tire Pressure Sensor Status | Data Display | Valid/Invalid | Valid
RR Pressure Sensor ID | Data Display | 8 digit number/Invalid | 8 digit number
RR Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/N/A | Stationary
RR Tire Pressure | Data Display | kPA/psi | Varies
RR Tire Pressure Sensor Status | Data Display | Valid/Invalid | Valid
Sensor Learn Mode | Data Display | Active/Inactive | Inactive
TPM System Enabled | Data Display | Yes/No | Yes
Vehicle Speed | Data Display | km/h or mph | 0