For 1990-2009 cars

### Removal Procedure

1. Remove the bridge console compartment. Refer to Front Floor Console Rear Compartment Replacement.
2. Remove the screw securing the cupholder from the rear of bridge console.
3. Remove the cupholder from the bridge console.

### Installation Procedure

1. Install the cupholder to the bridge console.
2. Install the bolts securing the cupholder to the bridge console.
3. Install the bridge console compartment. Refer to Front Floor Console Rear Compartment Replacement.