For 1990-2009 cars

### Removal Procedure

1. Remove the rear overhead console.
2. Remove screws securing the rear park assist tell tale module to the overhead console.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws securing the rear park assist tell tale module to the overhead console.

Tighten
Tighten the bolt (1) to 2 N·m (18 lb in).

3. Install the rear overhead console.