For 1990-2009 cars

### Remote Control Door Lock Receiver Programming and Setup

Each of the following service procedures requires programming or setup procedures to be performed on the theft deterrent control module.

### Remote Control Door Lock Receiver Replacement

If the remote control door lock receiver is replaced, the following procedures must be performed:

1. Keyless Entry Transmitter Programming--Method 1--Refer to Transmitter Programming.
2. Set up a new remote control door lock receiver
3. Theft Deterrent 10 Minute Relearn Procedure
4. Refer to Tire Pressure Indicator Sensor Learn.

### Replacing Keyless Entry Transmitters

If a keyless entry transmitter is replaced, the following procedure must be performed:

Keyless Entry Transmitter Programming--Refer to Transmitter Programming.