For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Side Door Lock Striker Replacement

1 | Striker Cover and Front Side Door Lock Striker Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 28 N·m (21 lb ft)
2 | Front Side Door Lock Striker Assembly Caution: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

Tip
Adjust striker as needed. Refer to Door Lock Striker Adjustment.