For 1990-2009 cars

Table 1: | Instrument Panel Cluster (IPC)
Table 2: | Engine Control Module (ECM) 4.6L (LH2), 3.6L (LY7)

#### Instrument Panel Cluster (IPC)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Display(s) Test | Output Controls | The IPC illuminates all of the display segments and sweeps all gage pointers when On is selected.

#### Engine Control Module (ECM) 4.6L (LH2), 3.6L (LY7)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
MIL | Engine Output Controls | The ECM commands the MIL indicator on and off.