For 1990-2009 cars
Active Antenna Authenticated: The scan tool displays Yes/No. The scan tool will display Yes when the active antenna has been successfully authenticated.
Active Antenna - Fob 1: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 1 has been detected by the active antenna.
Active Antenna - Fob 2: The scan tool displays Present/ Not Present. The scan tool will display Present when Fob 2 has been detected by the active antenna.
Active Antenna - Fob 3: The scan tool displays Present/ Not Present. The scan tool will display Present when Fob 3 has been detected by the active antenna.
Active Antenna - Fob 4: The scan tool displays Present/ Not Present. The scan tool will display Present when Fob 4 has been detected by the active antenna.
Battery Voltage Signal: The scan tool displays the battery voltage.
Console Antenna Authenticated: The scan tool displays Yes/No. The scan tool will display Yes when the console antenna has been successfully authenticated.
Console Antenna - Fob 1: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 1 has been detected by the console antenna.
Console Antenna - Fob 2: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 2 has been detected by the console antenna.
Console Antenna - Fob 3: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 3 has been detected by the console antenna.
Console Antenna - Fob 4: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 4 has been detected by the console antenna.
Door Ajar Switch: The scan tool displays Door Closed/Ajar. The scan tool displays Door Ajar when the respective door is ajar.
Door Lock Cylinder Switch: The scan tool displays Idle/Lock/Unlock/Invalid. The scan tool displays the status of the driver door cylinder switch.
Driver Door Handle Exterior: The scan tool displays Active/Inactive. The scan tool will display Active when the exterior driver door handle is pulled.
Passenger Door Handle Exterior: The scan tool displays Active/Inactive. The scan tool will display Active when the exterior passenger door handle is pulled.
Press the Fob 1 key: No Key Press/Lock/Unlock/Remote Start/Trunk/Panic The scan tool displays the last key pressed on the key fob 1.
Fob 1 Programmed: The scan tool displays Yes/No. Then scan tool will display Yes if a keyless entry transmitter is programmed in the Fob 1 slot.
Press the Fob 2 key: No Key Press/Lock/Unlock/Remote Start/Trunk/Panic The scan tool displays the last key pressed on the key fob 2.
Fob 2 Programmed: The scan tool displays Yes/No. Then scan tool will display Yes if a keyless entry transmitter is programmed in the Fob 2 slot.
Press the Fob 3 key: No Key Press/Lock/Unlock/Remote Start/Trunk/Panic The scan tool displays the last key pressed on the key fob 3.
Fob 3 Programmed: The scan tool displays Yes/No. Then scan tool will display Yes if a keyless entry transmitter is programmed in the Fob 3 slot.
Press the Fob 4 key: No Key Press/Lock/Unlock/Remote Start/Trunk/Panic The scan tool displays the last key pressed on the key fob 4.
Fob 4 Programmed: The scan tool displays Yes/No. Then scan tool will display Yes if a keyless entry transmitter is programmed in the Fob 4 slot.
Hood Closed Switch: The scan tool displays Active/Inactive. The scan tool will display Active when the hood is closed.
Hood Open Switch: The scan tool displays Active/Inactive. The scan tool will display Active when the hood is open.
Ignition Mode Switch: The scan tool displays Idle/Crank/Accy/Off. The scan tool displays the current status of the ignition mode switch.
Vehicle Remote Key: The scan tool displays None/Fob 1/Fob 2/Fob 3/Fob 4. The scan tool will display the respective fob located within the vehicle.
Last Remote Key Used: The scan tool displays Fob 1/ Fob 2/Fob 3/Fob 4. The scan tool will displays the last key fob used for any keyless entry function.
Left Door Handle Antenna Authenticated: The scan tool displays Yes/No. The scan tool will display Yes when the left door handle antenna has been successfully authenticated.
Left Door Handle Antenna Fob 1: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 1 has been detected by the left door handle antenna.
Left Door Handle Antenna Fob 2: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 2 has been detected by the left door handle antenna.
Left Door Handle Antenna Fob 3: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 3 has been detected by the left door handle antenna.
Left Door Handle Antenna Fob 4: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 4 has been detected by the left door handle antenna.
Key Code Number Programmed: The Scan tool displays 0/1/2/3/4. The scan tool will display the number of key fobs currently programmed to the vehicle.
Passive Door Unlock Status: The scan tool displays Disabled/Authenticated Dr./Driver+Passenger/All Door Unlock. The scan tool displays the personalization setting of the passive door lock.
Passive Door Unlock Trigger: The scan tool displays Enabled/Disabled. The scan tool will display Enabled when passive unlocking is turned on in personalization.
Rear Fascia Antenna Authenticated: The scan tool displays Yes/No. The scan tool will display Yes when the rear fascia antenna has been successfully authenticated.
Rear Fascia Antenna - Fob 1: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 1 has been detected by the rear fascia antenna.
Rear Fascia Antenna - Fob 2: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 2 has been detected by the rear fascia antenna.
Rear Fascia Antenna - Fob 3: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 3 has been detected by the rear fascia antenna.
Rear Fascia Antenna - Fob 4: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 4 has been detected by the rear fascia antenna.
Remote Start Activation: The scan tool displays the number of attempted remote starts.
Remote Start Equipped: The scan tool displays Enabled/Disabled. The scan tool will display Enabled when all criteria to allow a remote start event have been met.
Remote Starts Remaining: The scan tool displays the number of remaining remote starts that will be allowed.
Remote Start Request: The scan tool displays Yes/No. The scan tool will display Yes when a valid remote start request is received.
Right Door Handle Antenna Authenticated: The scan tool displays Yes/No. The scan tool will display Yes when the right door handle antenna has been successfully authenticated.
Right Door Handle Antenna Fob 1: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 1 has been detected by the right door handle antenna.
Right Door Handle Antenna Fob 2: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 2 has been detected by the right door handle antenna.
Right Door Handle Antenna Fob 3: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 3 has been detected by the right door handle antenna.
Right Door Handle Antenna Fob 4: The scan tool displays Present/Not Present. The scan tool will display Present when Fob 4 has been detected by the right door handle antenna.