For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result. Tip Clean and inspect all valve components and the valve body. The control valve lower body is replaceable only as an assembly.
1 | Clutch Piston Dam Feed Regulator Valve Train
2 | Clutch Select Solenoid Valve Train
3 | Clutch Select Solenoid Valve Train
4 | Manual Valve
5 | TCC Regulator Apply Valve Train