For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Compartment Caulking Panel Locator (Qty: 2)
2 | Radiator Bracket Shield Sight Cover Assembly
3 | Hood Primary and Secondary Latch Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
4 | Hood Primary and Secondary Latch Assembly Tip Remove the hood release cable from the latch.
5 | Hood Ajar Rivet
6 | Hood Ajar Switch