For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ignition Lock Cylinder Case Screws | 7 N·m | 22 lb ft
Intermediate Shaft Bolts | 33 N·m | 24 lb ft
Intermediate Shaft to the Steering Column Pinch Bolt | 48 N·m | 35 lb ft
Intermediate Shaft to the Steering Gear Pinch Bolt | 45 N·m | 33 lb ft
Steering Column Mounting Nuts | 25 N·m | 18 lb in
Steering Column Trim Cover Screws Lower | 3.5 N·m | 31 lb in
Steering Column Trim Cover Screws Upper | 1.5 N·m | 13 lb in
Steering Wheel Control Harness Retainer Screws | 2.3 N·m | 20 lb in
Steering Wheel Control Switch Screws | 2.3 N·m | 20 lb ft
Steering Wheel Nut | 40 N·m | 29 lb in
Turn Signal Multifunction Switch Screw Side | 7 N·m | 62 lb in
Turn Signal Multifunction Switch Screw Top | 3 N·m | 27 lb ft
Upper Intermediate shaft to Lower Intermediate Shaft Pinch bolt | 33 N·m | 24 lb in
Telescope Actuator Retainer Bolts | 5 N·m | 45 lb ft
Steering Column Bracket | 17 N·m | 13 lb in
Tilt Motor Mounting Screws | 1.5 N·m | 13 lb in