For 1990-2009 cars

Connector 1: | 16-Way Transmission Pass-Through

### 16-Way Transmission Pass-Through

#### Connector Part Information

- OEM: 15491328
- Service: 15131300
- Description: 16-Way F 1.5 Pin Housing (BK)

#### Terminal Part Information

- Terminal/Tray: 2 21 24 47220 0/12
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-28/J-35616-66 (YE)

#### 16-Way Transmission Pass-Through

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | OG/BK | 1786 | Park/Neutral Signal
4 | RD/WH | 2440 | Battery Positive Voltage
5 | BK/WH | 451 | Ground
6 | WH | 17 | Brake Pedal Apply Signal
7-8 | -- | -- | Not Used
9 | YE | 43 | Accessory Voltage Power
10 | TN/BK | 2500 | CAN Hi
11 | TN | 2501 | CAN Lo
12 | PK | 1339 | Run/Crank Voltage
13 | TN | 2501 | CAN Lo 2
14 | TN/BK | 2500 | CAN Hi 2
15-16 | -- | -- | Not Used