For 1990-2009 cars

Table 1: | Pinion Shim Calculation Table with an A1 Value Greater Than 111.00 mm (4.37 in)
Table 2: | Drive Pinion Shim Calculation Table with an A1 Value Less Than 111.00 mm (4.37 in)
Table 3: | Differential Case Right Side Shim Calculation Table with an A2 Value Greater Than 63.5 mm (2.5 in)
Table 4: | Differential Case Right Side Shim Calculation Table with an A2 Value Less Than 63.5 mm (2.5 in)

#### Pinion Shim Calculation Table with an A1 Value Greater Than 111.00 mm (4.37 in)

Calculations | Example Measurements | Actual Measurements
--- | --- | ---
| Metric | English | Metric | English
B Nominal Value | 5.00 mm | 0.197 in | 5.00 mm | 0.197 in
B1 Measured Value | 3.31 mm | 0.130 in | -- | --
B2 (B Nominal Value Minus B1 = B2) | 1.69 mm | 0.067 in | -- | --
A1 Value (Taken from Ring Gear) | 111.03 mm | 4.371 in | -- | --
A Nominal Value | 111.00 mm | 4.37 in | 111.00 mm | 4.37 in
B3 (A1 Value Minus A Nominal = B3) | 0.03 mm | 0.0012 in | -- | --
B2 | 1.69 mm | 0.0665 in | -- | --
B3 | 0.03 mm | 0.0012 in | -- | --
Pinion Shim Size (B2 Plus B3 = Pinion Shim) | 1.72 mm | 0.0677 in | -- | --

#### Drive Pinion Shim Calculation Table with an A1 Value Less Than 111.00 mm (4.37 in)

Calculations | Example Measurements | Actual Measurements
--- | --- | ---
| Metric | English | Metric | English
B Nominal Value | 5.00 mm | 0.197 in | 5.00 mm | 0.197 in
B1 Measured Value | 3.31 mm | 0.130 in | -- | --
B2 (B Nominal Value Minus B1 = B2) | 1.69 mm | 0.067 in | -- | --
A1 Value (Taken from Ring Gear) | 110.97 mm | 4.369 in | -- | --
A Nominal Value | 111.00 mm | 4.37 in | 111.00 mm | 4.37 in
B3 (A1 Value Minus A Nominal = B3) | -0.03 mm | -0.0011 in | -- | --
B2 | 1.69 mm | 0.067 in | -- | --
B3 | -0.03 mm | -0.0011 in | -- | --
Pinion Shim Size (B2 Plus B3 = Pinion Shim) | 1.66 mm | 0.0654 in | -- | --

#### Differential Case Right Side Shim Calculation Table with an A2 Value Greater Than 63.5 mm (2.5 in)

Calculations | Example Measurements | Actual Measurements
--- | --- | ---
| Metric | English | Metric | English
C Nominal Value for Differential Ratio of which is 3.42 | 5.00 mm | 0.197 in | 5.00 mm | 0.197 in
C Nominal Value for Differential Ratio of which is 2.73 | 10.5 mm | 0.413 in | 10.5 mm | 0.413 in
C1 Measured Value | 3.10 mm | 0.122 in | -- | --
C2 (C Nominal Value Minus C1 = C2) | 1.90 mm | 0.075 in | -- | --
A2 Value (Taken from Ring Gear) | 63.53 mm | 2.501 in | -- | --
D Nominal Value | 63.50 mm | 2.5 in | 63.5 mm | 2.5 in
C3 (A2 Value Minus D Nominal = C3) | 0.03 mm | 0.0012 in | -- | --
C2 | 1.90 mm | 0.0748 in | -- | --
C3 | 0.03 mm | 0.0012 in | -- | --
Right Side Case Shim (C2 Plus C3 = Right Side Shim) | 1.93 mm | 0.0736 in | -- | --

#### Differential Case Right Side Shim Calculation Table with an A2 Value Less Than 63.5 mm (2.5 in)

Calculations | Example Measurements | Actual Measurements
--- | --- | ---
| Metric | English | Metric | English
C Nominal Value for Differential Ratio of which is 3.42 | 5.00 mm | 0.197 in | 5.00 mm | 0.197 in
C Nominal Value for Differential Ratio of which is 2.73 | 10.5 mm | 0.413 in | 10.5 mm | 0.413 in
C1 Measured Value | 3.10 mm | 0.122 in | -- | --
C2 (C Nominal Value Minus C1 = C2) | 1.90 mm | 0.75 in | -- | --
A2 Value (Taken from Ring Gear) | 63.47 mm | 2.499 in | -- | --
D Nominal Value | 63.5 mm | 2.5 in | 63.5 mm | 2.50 in
C3 (A2 Value Minus D Nominal = C3) | -0.03 mm | -0.0012 in | -- | --
C2 | 1.90 mm | 0.0748 in | -- | --
C3 | -0.03 mm | -.0012 in | -- | --
Right Side Case Shim (C2 Plus C3 = Right Side Shim) | 1.87 mm | 0.0736 in | -- | --