For 1990-2009 cars

Connector 1: | C100 Body Harness to the Engine Harness (LH2)
Connector 2: | C101 Engine Harness to Body Harness
Connector 3: | C102 I/P to Engine Harness
Connector 4: | C104 Engine to Valley Jumper Harness (LH2)
Connector 5: | C105 Engine to Starter Harness (LH2)
Connector 6: | C106 Engine to POA Jumper Harness (LY7)
Connector 7: | C107 Left Repeater Lamp Harness to Forward Lamp
Connector 8: | C108 Right Repeater Lamp Harness to Forward Lamp
Connector 9: | C109 A/C Jumper Harness (LY7)
Connector 10: | C110 Engine Harness to Transmission
Connector 11: | C111 Forward Lamp to I/P Harness (K59, TT6)
Connector 12: | C112 I/P to Forward Lamp Harness
Connector 13: | C113 Engine to Forward Lamp Harness (LH2)
Connector 14: | C115 Fuel Injector Harness (LY7)
Connector 15: | C139 Engine to Even Bank Coil/Module Harness (LH2)
Connector 16: | C140 Engine to Odd Bank Coil/Module Harness (LH2)
Connector 17: | C200 Body to I/P Harness Right
Connector 18: | C201 Body to I/P Harness Right Center
Connector 19: | C202 I/P to Steering Column Harness
Connector 20: | C204 Body to I/P Harness Left Center
Connector 21: | C205 Body to I/P Harness Left
Connector 22: | C212 Body to Console Harness
Connector 23: | C213 Rear Console to Rear Seat Harness
Connector 24: | C214 HVAC Motor Assembly
Connector 25: | C217 Inflatable Restraint Module to Body Harness (Passenger)
Connector 26: | C218 Inflatable Restraint Steering Wheel Module to Body Harness (Driver)
Connector 27: | C276 Steering Column Harness
Connector 28: | C277 Steering Column Harness
Connector 29: | C300 Body to Driver Seat Harness
Connector 30: | C301 Body to Driver Seat Harness
Connector 31: | C302 Body to Rear Seat Harness
Connector 32: | C302 Body to Rear Seat Harness (w/o Heated Seats)
Connector 33: | C304 Console to I/P Harness
Connector 34: | C305 Headliner to Body Harness
Connector 35: | C306 Body to Front Passenger Seat
Connector 36: | C307 Body to Front Passenger Seat
Connector 37: | C308 Headliner to Body
Connector 38: | C309 Sunroof Jumper (CF5) to Headliner
Connector 39: | C310 Sunroof (CF5) to Body
Connector 40: | C312 Driver Lumbar to Driver Seat (AL2 w/o A45)
Connector 41: | C313 Passenger Lumbar to Passenger Seat (AL2)
Connector 42: | C317 Driver Seat Harness to Body Harness
Connector 43: | C318 Passenger Seat Harness to Body Harness
Connector 44: | C319 Lumbar Motor Position Sensor - Driver to Driver Seat Harness (A45)
Connector 45: | C320 Body to Rear I/P Harness
Connector 46: | C321 Left Rear Seat Cushion to Left Rear Seat Harness C1
Connector 47: | C321 Left Rear Seat Cushion to Left Rear Seat Harness (w/o Heated Seat)
Connector 48: | C322 Right Rear Seat Cushion to Right Rear Seat Harness (w/o Heated Seat)
Connector 49: | C322 Right Rear Seat Cushion to Right Rear Seat Harness C1
Connector 50: | C323 Left Rear Seat Cushion to Left Rear Seat Harness C2
Connector 51: | C324 Right Rear Seat Cushion to Right Rear Seat Harness C2
Connector 52: | C325 Rear Seat Harness to Rear Seatback C1
Connector 53: | C326 Rear Seat Harness to Rear Seatback C2
Connector 54: | C327 Left, Right Rear Seat Harness Connection
Connector 55: | C327 Left, Right Rear Seat Harness Connection
Connector 56: | C329 Rear Seatback Harness to Left Rear Massage Motor Sensor
Connector 57: | C330 Rear Seatback Harness to Massage Module C1
Connector 58: | C331 Rear Seatback Harness to Massage Module C2
Connector 59: | C400 Body Harness to Rear Fascia
Connector 60: | C401 Body Harness to Rear Fascia (UD7)
Connector 61: | C420 Fuel Tank Jumper to Body
Connector 62: | C500 Body to Left Front Door Harness
Connector 63: | C501 Left Front Door to Left Front Door Trim Harness
Connector 64: | C600 Body to Right Front Door Harness
Connector 65: | C601 Right Front Door to Right Front Door Trim Harness
Connector 66: | C700 Body to Left Front Door Harness
Connector 67: | C701 Left Rear Door to Left Rear Door Trim Harness
Connector 68: | C800 Body to Right Rear Door Harness
Connector 69: | C801 Right Front Door to Right Front Door Trim Harness

### C100 Body Harness to the Engine Harness (LH2)

#### Connector Part Information

- OEM: 13539911
- Service: NS
- Description: 8-Way F (BK)

#### Connector Part Information

- OEM: 15489219
- Service: NS
- Description: 8-Way M (BK)

#### C100 Body Harness to the Engine Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference | 1 | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference
2 | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference | 2 | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference
3 | TN/WH | 1207 | Left Front Strut Position Sensor Signal | 3 | TN/WH | 1207 | Left Front Strut Position Sensor Signal
4 | L-BU/BK | 1212 | Right Front Strut Position Sensor Low Reference | 4 | L-BU/BK | 1212 | Right Front Strut Position Sensor Low Reference
5 | PU/WH | 1211 | Right Front Strut Position Sensor Voltage Reference | 5 | PU/WH | 1211 | Right Front Strut Position Sensor Voltage Reference
6 | TN/WH | 1213 | Right Front Strut Position Sensor Signal | 6 | TN/WH | 1213 | Right Front Strut Position Sensor Signal
7 | OG/BK | 1448 | Left Front Strut Motor Increase Damping | 7 | OG/BK | 1448 | Left Front Strut Motor Increase Damping
8 | L-GN | 1005 | Left Front Strut Motor Decrease Damping Control | 8 | L-GN | 1005 | Left Front Strut Motor Decrease Damping Control

### C101 Engine Harness to Body Harness

#### Connector Part Information

- OEM: 15326084
- Service: 15306348
- Description: 16-Way F GT 150, 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Service: 15306122
- Description: 16-Way M GT 150, 280 Series Sealed 4.0 5.8 (BK)

#### C101 Engine Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN | 884 | Wheel Speed Sensor Signal Left Rear | A | BN | 884 | Wheel Speed Sensor Signal Left Rear
B | OG | 885 | Wheel Speed Sensor Low Reference Left Rear | B | OG | 885 | Wheel Speed Sensor Low Reference Left Rear
C | BN | 882 | Wheel Speed Sensor Signal Right Rear | C | BN | 882 | Wheel Speed Sensor Signal Right Rear
D | WH | 883 | Wheel Speed Sensor Low Reference Right Rear | D | WH | 883 | Wheel Speed Sensor Low Reference Right Rear
E | L-BU | 715 | Lateral Accelerometer Signal | E | L-BU | 715 | Lateral Accelerometer Signal
F | D-BU | 716 | Yaw Rate Sensor Signal (1) | F | D-BU | 716 | Yaw Rate Sensor Signal (1)
G-H | -- | -- | Not Used | G-H | -- | -- | Not Used
J | D-BU | 1936 | Primary Fuel Level Sensor Signal | J | D-BU | 1936 | Primary Fuel Level Sensor Signal
K | L-BU | 1937 | Secondary Fuel Level Sensor Signal | K | L-BU | 1937 | Secondary Fuel Level Sensor Signal
L | GY | 596 | Fuel Tank Pressure Sensor 5-Volt Reference (LH2) | L | GY | 596 | Fuel Tank Pressure Sensor 5-Volt Reference
M | D-GN | 890 | Fuel Tank Pressure Sensor Signal | M | D-GN | 890 | Fuel Tank Pressure Sensor Signal
N | BK | 452 | Fuel Tank Pressure Sensor Low Reference (LH2) | N | BK | 562 | Fuel Tank Pressure Sensor Low Reference
P | -- | -- | Not Used | P | -- | -- | Not Used
R | D-GN/WH | 465 | Fuel Pump Primary Relay Control | R | D-GN/WH | 465 | Fuel Pump Primary Relay Control
S | WH | 1310 | EVAP Canister Vent Solenoid Control | S | WH | 1310 | EVAP Canister Vent Solenoid Control

### C102 I/P to Engine Harness

#### Connector Part Information

- OEM: 13485711
- Service: N/A
- Description: 24-Way F

#### Connector Part Information

- OEM: 13485177
- Service: N/A
- Description: 24-Way M

#### C102 I/P to Engine Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WH | 17 | Stop Lamp Switch Signal | A1 | WH | 17 | Stop Lamp Switch Signal
A2 | BN/WH | 419 | Service Engine Indicator Control | A2 | BN/WH | 419 | Service Engine Indicator Control
A3 | BN | 818 | Vehicle Speed Signal | A3 | BN | 818 | Vehicle Speed Signal
A4 | -- | -- | -- | A4 | -- | -- | --
A5 | PK | 2039 | Run Ignition 3 Voltage | A5 | PK | 2039 | Run Ignition 3 Voltage
A6 | -- | -- | -- | A6 | -- | -- | --
A7 | L-GN/BK | 1338 | Yaw Rate Sensor Signal (2) | A7 | L-GN/BK | 1338 | Yaw Rate Sensor Signal (2)
A8 | GY/BK | 1337 | Yaw Rate Sensor Volt Reference | A8 | GY/BK | 1337 | Yaw Rate Sensor Volt Reference
B1 | YE/BK | 5728 | ECM/TCM Serial Data Wake Up | B1 | YE/BK | 5728 | ECM/TCM Serial Data Wake Up
B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) (TT7/TT8/K59) | B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) (TT7/TT8/K59)
B3 | TN | 2501 | High Speed GMLAN Serial Data (-) (1) (TT7/TT8/K59) | B3 | TN | 2501 | High Speed GMLAN Serial Data (-) (1) (TT7/TT8/K59)
B4 | YE | 5727 | High Speed GMLAN Serial Data Wake Up | B4 | YE | 5727 | High Speed GMLAN Serial Data Wake Up
B5 | PU | 5526 | Tap Up/Tap Down Switch Signal | B5 | PU | 5526 | Tap Up/Tap Down Switch Signal
B6 | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55) | B6 | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55)
B7 | TN/WH | 1207 | Left Front Strut Position Sensor Signal (w/TT7/TT8 w/o F55) | B7 | TN/WH | 1207 | Left Front Strut Position Sensor Signal (w/TT7/TT8 w/o F55)
B8 | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55) | B8 | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55)
C1 | PU | 1272 | Accelerator Pedal Position Low Reference (2) | C1 | PU | 1272 | Accelerator Pedal Position Low Reference (2)
C2 | L-BU | 1162 | Accelerator Pedal Position Signal (2) | C2 | L-BU | 1162 | Accelerator Pedal Position Signal (2)
C3 | TN | 1274 | Accelerator Pedal Position 5-Volt Reference (2) | C3 | TN | 1274 | Accelerator Pedal Position 5-Volt Reference (2)
C4 | L-GN | 1763 | Steering Wheel Position Signal A | C4 | L-GN | 1763 | Steering Wheel Position Signal A
C5 | L-BU | 1764 | Steering Wheel Position Signal B | C5 | L-BU | 1764 | Steering Wheel Position Signal B
C6 | WH/BK | 1164 | Accelerator Pedal Position 5-Volt Reference (1) | C6 | WH/BK | 1164 | Accelerator Pedal Position 5-Volt Reference (1)
C7 | D-BU | 1161 | Accelerator Pedal Position Signal (1) | C7 | D-BU | 1161 | Accelerator Pedal Position Signal (1)
C8 | BN | 1271 | Accelerator Pedal Position Low Reference (1) | C8 | BN | 1271 | Accelerator Pedal Position Low Reference (1)

### C104 Engine to Valley Jumper Harness (LH2)

#### Connector Part Information

- OEM: 15326863
- Service: 88986260
- Description: 16-Way F (BK)

#### Connector Part Information

- OEM: 15326854
- Service: NS
- Description: 16-Way M GT 150 Series Sealed 4.0 (BK)

#### C104 Engine to Valley Jumper Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY/BK | 6272 | Crankshaft Position Sensor Low Reference (1) | A | GY/BK | 6272 | Crankshaft Position Sensor Low Reference (1)
B | WH/BK | 6271 | Crankshaft Position Sensor Signal (1) | B | WH/BK | 6271 | Crankshaft Position Sensor Signal (1)
C | PU/WH | 6270 | Crankshaft Position Sensor 12-Volt Reference | C | PU/WH | 6270 | Crankshaft Position Sensor 12-Volt Reference
D | D-BU/WH | 6756 | Camshaft Phase Reset 1 | D | D-BU/WH | 6756 | Camshaft Phase Reset 1
E | WH/BK | 6396 | Camshaft Phaser Exhaust Solenoid (1) | E | WH/BK | 6396 | Camshaft Phaser Exhaust Solenoid (1)
F | PK/BK | 6395 | Camshaft Phaser Intake Solenoid (1) | F | PK/BK | 6395 | Camshaft Phaser Intake Solenoid (1)
G | D-BU | 496 | Knock Sensor Signal (1) | G | D-BU | 496 | Knock Sensor Signal (1)
H | GY | 1716 | Knock Sensor Low Reference (1) | H | GY | 1716 | Knock Sensor Low Reference (1)
J | L-BU/WH | 1876 | Knock Sensor Signal (2) | J | L-BU/WH | 1876 | Knock Sensor Signal (2)
K | GY | 2303 | Knock Sensor Low Reference (2) | K | GY | 2303 | Knock Sensor Low Reference (2)
L | TN/BK | 6397 | Camshaft Phaser Intake Solenoid (2) | L | TN/BK | 6397 | Camshaft Phaser Intake Solenoid (2)
M | GY/BK | 6394 | Camshaft Phaser Exhaust Solenoid (2) | M | GY/BK | 6394 | Camshaft Phaser Exhaust Solenoid (2)
N | D-BU | 6755 | Camshaft Phase Reset 4 | N | D-BU | 6755 | Camshaft Phase Reset 4
P | BN | 6753 | Camshaft Phase Reset 2 | P | BN | 6753 | Camshaft Phase Reset 2
R | BK/WH | 6754 | Camshaft Phase Reset 3 | R | BK/WH | 6754 | Camshaft Phase Reset 3
S | -- | -- | Not Used | S | -- | -- | Not Used

### C105 Engine to Starter Harness (LH2)

#### Connector Part Information

- OEM: 12065172
- Service: N/A
- Description: 1-Way F 280 Series Sealed (BK)

#### Connector Part Information

- OEM: 12065171
- Service: N/A
- Description: 1-Way M 280 Series Sealed (BK)

#### C105 Engine to Starter Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PU | 6 | Starter Solenoid Crank Voltage | A | PU | 6 | Starter Solenoid Crank Voltage

### C106 Engine to POA Jumper Harness (LY7)

#### Connector Part Information

- OEM: 12059472
- Service: 12101830
- Description: 7-Way F 150/280 Series GT (BK)

#### Connector Part Information

- OEM: 12052200
- Service: 12117321
- Description: 7-Way M 150/480 Series (BK)

#### C106 Engine to POA Jumper Harness (LY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/BK | 5291 | Engine Main Relay Fused Control (2) | A | PK/BK | 5291 | Engine Main Relay Fused Control (2)
B | -- | -- | Not Used | B | -- | -- | Not Used
C | D-GN | 59 | A/C Compressor Clutch Supply Voltage | C | D-GN | 59 | A/C Compressor Clutch Supply Voltage
D | PK/BK | 5292 | Engine Main Relay Fused Control (3) | D | PK/BK | 5292 | Engine Main Relay Fused Control (3)
E | PU | 6 | Starter Solenoid Crank Voltage | E | PU | 6 | Starter Solenoid Feed
F | PK/BK | 5293 | Engine Main Relay Fused Control (4) | F | PK/BK | 5293 | Engine Main Relay Fused Control (4)
G | BK/WH | 751 | Signal Ground | G | BK/WH | 1451 | Signal Ground

### C107 Left Repeater Lamp Harness to Forward Lamp

#### Connector Part Information

- OEM: 15426924
- Service: N/A
- Description: 2-Way F Weather Pack (BK)

#### Connector Part Information

- OEM: 15496066
- Service: N/A
- Description: 2-Way M Weather Pack (BK)

#### C107 Left Repeater Lamp Harness to Forward Lamp

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage | A | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
B | BK | 250 | Ground | B | BK | 250 | Ground

### C108 Right Repeater Lamp Harness to Forward Lamp

#### Connector Part Information

- OEM: 15426924
- Service: N/A
- Description: 2-Way F Weather Pack (BK)

#### Connector Part Information

- OEM: 15426924
- Service: N/A
- Description: 2-Way M Weather Pack (BK)

#### C108 Right Repeater Lamp Harness to Forward Lamp

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage | A | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
B | BK | 250 | Ground | B | BK | 250 | Ground

### C109 A/C Jumper Harness (LY7)

#### Connector Part Information

- OEM: 12052641
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12162000
- Service: N/A
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### C109 A/C Jumper Harness (LY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN | 59 | A/C Compressor Clutch Supply Voltage | A | D-GN | 59 | A/C Compressor Clutch Supply Voltage
B | BK | 750 | Ground | B | BK | 1450 | Ground

### C110 Engine Harness to Transmission

#### Connector Part Information

- OEM: 9432001
- Service: N/A
- Description: 20-Way F (BK)

#### Connector Part Information

- OEM: 9332001
- Service: N/A
- Description: 20-Way M (BK)

#### C110 Engine Harness to Transmission

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 400 | OSS High Signal | 1 | YE | 400 | OSS High Signal
2 | OG/BK | 1786 | Park/Neutral Signal | 2 | OG/BK | 1786 | Park/Neutral Signal
3 | PU | 401 | OSS Low Signal | 3 | PU | 401 | OSS Low Signal
4 | BK/WH | 751 | Ground (w/LY7) | 4 | BK/WH | 751 | Ground (w/LY7)
5 | PU | 898 | Shift Solenoid Valve 3 High Control | 5 | PU | 898 | Shift Solenoid Valve 3 High Control
6 | TN | 2762 | Low Reference | 6 | TN | 2762 | Low Reference
7 | YE | 772 | Transmission Range Switch Signal B | 7 | YE | 772 | Transmission Range Switch Signal B
8 | L-BU/WH | 1229 | PC Solenoid Valve Low Control | 8 | L-BU/WH | 1229 | PC Solenoid Valve Low Control
9 | YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | 9 | YE/BK | 1223 | 2-3 Shift Solenoid Valve Control
10 | YE/BK | 1227 | TFT Sensor Signal | 10 | YE/BK | 1227 | TFT Sensor Signal
11 | WH | 776 | Transmission Range Switch Signal P | 11 | WH | 776 | Transmission Range Switch Signal P
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | OG/BK | 1228 | PC Solenoid Valve High Control | 13 | OG/BK | 1228 | PC Solenoid Valve High Control
14 | L-GN | 1222 | 1-2 Shift Solenoid Valve Control | 14 | L-GN | 1222 | 1-2 Shift Solenoid Valve Control
15 | D-BU/WH | 1231 | AT ISS Low Signal | 15 | D-BU/WH | 1231 | AT ISS Low Signal
16 | TN/WH | 771 | Transmission Range Switch Signal A | 16 | TN/WH | 771 | Transmission Range Switch Signal A
17 | OG | 1525 | Solenoid Supply Voltage | 17 | OG | 1525 | Solenoid Supply Voltage
18 | OG/BK | 1230 | AT ISS High Signal | 18 | OG/BK | 1230 | AT ISS High Signal
19 | GY | 773 | Transmission Range Switch Signal C | 19 | GY | 773 | Transmission Range Switch Signal C
20 | BN | 418 | TCC PWM Solenoid Valve Control | 20 | BN | 418 | TCC PWM Solenoid Valve Control

### C111 Forward Lamp to I/P Harness (K59, TT6)

#### Connector Part Information

- OEM: 7283-5553-30
- Service: NS
- Description: 6-Way F 3 Series YESC/USCAR Sealed (BK)

#### Connector Part Information

- OEM: 7282-5553-30
- Service: NS
- Description: 6-Way M 3 Series YESC/USCAR (BK)

#### C111 Forward Lamp to I/P Harness (K59, TT6)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-D | -- | -- | Not Used | A-D | -- | -- | Not Used
E | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) | E | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
F | TN | 2501 | High Speed GMLAN Serial Data (-) (1) | F | TN | 2501 | High Speed GMLAN Serial Data (-) (1)
G | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) | G | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
H | TN | 2501 | High Speed GMLAN Serial Data (-) 1 | H | TN | 2501 | High Speed GMLAN Serial Data (-) 1
J-P | -- | -- | Not Used | J-P | -- | -- | Not Used
R | YE | 5727 | High Speed GMLAN Serial Data Wake Up | R | YE | 5727 | High Speed GMLAN Serial Data Wake Up
S | -- | -- | Not Used | S | -- | -- | Not Used

### C112 I/P to Forward Lamp Harness

#### Connector Part Information

- OEM: 15326863
- Service: 15306410
- Description: 16-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326868
- Service: 15306364
- Description: 16-Way M 150 Series Sealed (BK)

#### C112 I/P to Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55) | A | L-BU/BK | 1206 | Left Front Strut Position Sensor Low Reference (w/TT7/TT8, w/o F55)
B | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55) | B | PU/WH | 1205 | Left Front Strut Position Sensor Voltage Reference (w/TT7/TT8, w/o F55)
C | TN/WH | 1207 | Left Front Strut Position Sensor Signal (w/TT7/TT8 w/o F55) | C | TN/WH | 1207 | Left Front Strut Position Sensor Signal (w/TT7/TT8, w/o F55)
D | L-GN/BK | 1209 | Left Rear Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55) | D | L-GN/BK | 1209 | Left Rear Strut Position Sensor Low Reference (w/T7/TT8, w/o F55)
E | OG/BK | 1208 | Left Rear Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55) | E | OG/BK | 1208 | Left Rear Strut Position Sensor Voltage Reference (w/TT7/TT8, w/o F55)
F | L-GN/WH | 1210 | Left Rear Strut Position Sensor Signal (w/TT7/TT8 w/o F55) | F | L-GN/WH | 1210 | Left Rear Strut Position Sensor Signal (w/TT7/TT8, w/o F55)
G | YE | 5727 | High Speed GMLAN Serial Data Wake Up (TT7/TT8/ K59) | G | YE | 5727 | High Speed GMLAN Serial Data Wake Up (TT7/TT8/K59)
H-M | -- | -- | Not Used | H-M | -- | -- | Not Used
N | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (TT7/TT8) | N | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (TT7/TT8)
P | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (w/o TT7/TT8) | P | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (w/o TT7/TT8)
R | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (TT7/TT8) | R | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (TT7/TT8)
S | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (w/o TT7/TT8) | S | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (w/o TT7/TT8)

### C113 Engine to Forward Lamp Harness (LH2)

#### Connector Part Information

- OEM: 10734474
- Service: NS
- Description: 2-Way F (D-GY)

#### Connector Part Information

- OEM: 15425573
- Service: NS
- Description: 2-Way M (D-GY)

#### C113 Engine to Forward Lamp Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 1150 | Ground | 1 | BK | 1150 | Ground
2 | BK | 1150 | Ground | 2 | BK | 1150 | Ground

### C115 Fuel Injector Harness (LY7)

#### Connector Part Information

- OEM: 19632141
- Service: NS
- Description: 10-Way F Amp (BK)

#### Connector Part Information

- OEM: 19623521
- Service: NS
- Description: 10-Way M Amp (BK)

#### C115 Fuel Injector Harness (LY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | 5291 | Engine Main Relay Fused Control (2) | 1 | WH | 5291 | Engine Main Relay Fused Control (2)
2 | PK/BK | 5292 | Engine Main Relay Fused Control (3) | 2 | WH | 5292 | Engine Main Relay Fused Control (3)
3 | TN | 1744 | Fuel Injector Control (1) | 3 | TN | 1744 | Fuel Injector Control (1)
4 | PK/BK | 1746 | Fuel Injector Control (3) | 4 | WH | 1746 | Fuel Injector Control (3)
5 | TN/WH | 845 | Fuel Injector Control (5) | 5 | TN/WH | 845 | Fuel Injector Control (5)
6 | L-GN/BK | 1745 | Fuel Injector Control (2) | 6 | L-GN/BK | 1745 | Fuel Injector Control (2)
7 | L-BU/BK | 844 | Fuel Injector Control (4) | 7 | L-BU/BK | 844 | Fuel Injector Control (4)
8 | YE/BK | 846 | Fuel Injector Control (6) | 8 | YE/BK | 846 | Fuel Injector Control (6)
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used

### C139 Engine to Even Bank Coil/Module Harness (LH2)

#### Connector Part Information

- OEM: 15317367
- Service: N/A
- Description: 7-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15326553
- Service: N/A
- Description: 7-Way M GT 150 Series (BK)

#### C139 Engine to Even Bank Coil/Module Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/BK | 5292 | Ignition 1 Voltage | A | PK/BK | 5292 | Ignition 1 Voltage
B | BK/WH | 1451 | Ground | B | BK/WH | 1451 | Ground
C | BN/WH | 2130 | Low Reference | C | BN | 2130 | Low Reference
D | D-GN/WH | 2124 | IC 4 Control | D | D-BU | 2124 | IC 4 Control
E | L-BU/WH | 2126 | IC 6 Control | E | L-GN | 2126 | IC 6 Control
F | PU/WH | 2128 | IC 8 Control | F | RD | 2128 | IC 8 Control
G | OG/WH | 2122 | IC 2 Control | G | PU | 2122 | IC 2 Control

### C140 Engine to Odd Bank Coil/Module Harness (LH2)

#### Connector Part Information

- OEM: 15317367
- Service: N/A
- Description: 7-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15326553
- Service: N/A
- Description: 7-Way M GT 150 Series (BK)

#### C140 Engine to Odd Bank Coil/Module Harness (LH2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/BK | 5291 | Ignition 1 Voltage | A | PK | 5291 | Ignition 1 Voltage
B | BK/WH | 1451 | Ground | B | BK | 1451 | Ground
C | BN | 2129 | Low Reference | C | BN | 2129 | Low Reference
D | D-GN | 2125 | IC 5 Control | D | D-BU | 2125 | IC 5 Control
E | L-BU | 2123 | IC 3 Control | E | D-GN | 2123 | IC 3 Control
F | PU | 2121 | IC 1 Control | F | RD | 2121 | IC 1 Control
G | OG | 2127 | IC 7 Control | G | PU | 2127 | IC 7 Control

### C200 Body to I/P Harness Right

#### Connector Part Information

- OEM: 15448129
- Service: 15359287
- Description: 40-Way F (BK)

#### Connector Part Information

- OEM: 15475869
- Service: 15359284
- Description: 40-Way M (BK)

#### C200 Body to I/P Harness Right

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 6817 | Backlight Lamps Control | A1 | YE | 6817 | Backlight Lamps Control
A2-A3 | -- | -- | Not Used | A2-A3 | -- | -- | Not Used
A4 | BK/WH | 451 | Ground | A4 | BK/WH | 451 | Ground
A5 | BK | 450 | Ground | A5 | BK | 450 | Ground
A6 | YE | 1491 | Backlight Lamps Control | A6 | YE | 1491 | Backlight Lamps Control
A7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | A7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
A8 | GY | 157 | Interior Lamp Control | A8 | GY | 157 | Interior Lamp Control
GY | 157 | Interior Lamp Control
B1 | D-GN | 6975 | Front Passenger Seat Headrest Display Video Signal (+) | B1 | D-GN | 6975 | Front Passenger Seat Headrest Display Video Signal (+)
B2 | WH/BK | 5335 | Front Passenger Seat Headrest Display Video Signal (-) | B2 | WH/BK | 5335 | Front Passenger Seat Headrest Display Video Signal (-)
B3 | BARE | 6976 | Drain Wire | B3 | BARE | 6976 | Drain Wire
B4 | D-GN/WH | 5845 | Front Passenger Seat Headrest Display Video Mode Signal | B4 | D-GN/WH | 5845 | Front Passenger Seat Headrest Display Video Mode Signal
B5 | PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal | B5 | PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal
B6 | PU | 5526 | Tap Up/Tap Down Switch Signal | B6 | PU | 5526 | Tap Up/Tap Down Switch Signal
B7-B10 | -- | -- | Not Used | B7 | -- | -- | Not Used
B11 | BN | 818 | Vehicle Speed Signal | B11 | BN | 818 | Vehicle Speed Signal
BN | 818 | Vehicle Speed Signal (w/YQ4/YQ6/YQ7)
B12 | OG | 300 | Run Ignition 3 Voltage | B12 | OG | 300 | Run Ignition 3 Voltage
C1 | TN/OG | 5045 | Left Front Discriminating Sensor Low Reference | C1 | TN/OG | 5045 | Left Front Discriminating Sensor Low Reference
C2 | YE | 1834 | SIR Forward Sensor Signal (1) | C2 | YE | 1834 | SIR Forward Sensor Signal (1)
C3 | D-GN | 1409 | Right Front Discriminating Sensor Signal | C3 | D-GN | 1409 | Right Front Discriminating Sensor Signal
C4 | GY | 5600 | Right Front Discriminating Sensor Low Reference | C4 | GY | 5600 | Right Front Discriminating Sensor Low Reference
C5 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (UE1, TT7/TT8) | C5 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (UE1, TT7/TT8)
C6 | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (UE1, TT7/TT8) | C6 | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (UE1, TT7/TT8)
C7 | TN/WH | 1975 | Right Front Speaker (-) (2) (YQ3/YQ4/YQ6/YQ7) | C7 | TN/WH | 1975 | Right Front Speaker (-) (2) (YQ3/YQ4/YQ6/YQ7)
C8 | TN | 1875 | Right Front Speaker (+) (2) (YQ3/YQ4/YQ6/YQ7) | C8 | TN | 1875 | Right Front Speaker (+) (2) (YQ3/YQ4/YQ6/YQ7)
C9 | L-GN/BK | 1338 | Low Reference | C9 | L-GN/BK | 1338 | Low Reference
C10 | GY/BK | 1337 | High Reference | C10 | GY/BK | 1337 | High Reference
C11 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (K59, UE1, TT7/TT8) | C11 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) 1 (K59, UE1, TT7/TT8)
C12 | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (K59, UE1, TT7/TT8) | C12 | TN | 2501 | High Speed GMLAN Serial Data (-) 1 (K59, UE1, TT7/TT8)
D1 | PU | 5531 | Hood Closed Switch Signal | D1 | PU | 5531 | Hood Closed Switch Signal
D2 | YE | 5530 | Hood Open Switch Signal | D2 | YE | 5530 | Hood Open Switch Signal
D3 | YE | 32 | I/P Lamp Fuse Supply Voltage - 1 | D3 | YE | 32 | I/P Lamp Fuse Supply Voltage - 1
YE | 32 | I/P Lamp Fuse Supply Voltage - 1
D4 | BN/WH | 309 | Right Park Lamp Supply Voltage (w/UE1, TT7/TT8) | D4 | BN/WH | 309 | Right Park Lamp Supply Voltage
D5 | -- | -- | Not Used | D5 | -- | -- | Not Used
D6 | PK | 1639 | Run/Crank Ignition 1 Voltage | D6 | PK | 1639 | Run/Crank Ignition 1 Voltage
D7-D8 | -- | -- | Not Used | D7-D8 | -- | -- | Not Used

### C201 Body to I/P Harness Right Center

#### Connector Part Information

- OEM: 10864191
- Service: NS
- Description: 26-Way F

#### Connector Part Information

- OEM: 13536441
- Service: NS
- Description: 26-Way M (GY)

#### C201 Body to I/P Harness Right Center

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 2240 | Battery Positive Voltage | 1 | RD/WH | 2240 | Battery Positive Voltage
2 | BK/WH | 851 | Signal Ground | 2 | BK/WH | 851 | Signal Ground
3 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage | 3 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
4 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage | 4 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
5 | D-GN/WH | 1932 | Shift Select Switch Park Signal | 5 | D-GN/WH | 1932 | Shift Select Switch Park Signal
6 | D-GN | 5525 | Tap Up/Tap Down Enable Signal | 6 | D-GN | 5525 | Tap Up/Tap Down Enable Signal
7 | L-GN/YE | 6847 | Shift Select Switch Park Supply Voltage | 7 | L-GN/YE | 6847 | Shift Select Switch Park Supply Voltage
8 | PK | 3 | Run/Crank Ignition 1 Voltage | 8 | PK | 3 | Run/Crank Ignition 1 Voltage
9 | PU | 5234 | Passenger Seat Belt Indicator | 9 | PU | 5234 | Passenger Seat Belt Indicator
10 | BN/WH | 1947 | Left Front Low Level Audio (-) (YQ2, YQ3/YQ4/YQ6/YQ7) | 10 | BN/WH | 1947 | Left Front Low Level Audio (-)
11 | BN | 511 | Left Front Low Level Audio Signal (YQ2, YQ3/YQ4/YQ6/YQ7) | 11 | BN | 511 | Left Front Low Level Audio Signal
12 | L-BU/WH | 5725 | Ignition Mode Switch Mode Voltage Backup | 12 | L-BU/WH | 5725 | Ignition Mode Switch Mode Voltage Backup
13 | L-BU | 5726 | Ignition Mode Switch Mode Control Backup | 13 | L-BU | 5726 | Ignition Mode Switch Mode Control Backup
14 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage | 14 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage
15 | L-BU | 1960 | Right Center Speaker (-) (YQ2, YQ3/YQ4/YQ6I/YQ7) | 15 | L-BU | 1960 | Front Center Speaker (-)
16 | YE | 1860 | Front Center Speaker (+) (w/YQ2, YQ3/YQ4/YQ6I/YQ7) | 16 | YE | 1860 | Front Center Speaker (+)
17 | BARE | 2012 | Right Front Audio Drain Wire | 17 | BARE | 2012 | Right Front Audio Drain Wire
18 | D-BU | 512 | Right Front Low Level Audio Signal | 18 | D-BU | 512 | Right Front Low Level Audio Signal
19 | D-BU/WH | 1948 | Right Front Low Level Audio (-) | 19 | D-BU/WH | 1948 | Right Front Low Level Audio (-)
20-21 | -- | -- | Not Used | 20-21 | -- | -- | Not Used
22 | OG/BK | 5831 | Audio Remote Control Signal | 22 | OG/BK | 5831 | Audio Remote Control Signal
23 | GY | 655 | Cellular Microphone Signal (TT7/TT8) | 23 | GY | 655 | Cellular Microphone Signal (TT7/TT8)
24 | BARE | 1782 | Drain Wire (TT7/TT8) | 24 | BARE | 1782 | Drain Wire (TT7/TT8)
25-26 | -- | -- | Not Used | 25-26 | -- | -- | Not Used

### C202 I/P to Steering Column Harness

#### Connector Part Information

- OEM: 15448129
- Service: 15359287
- Description: 40-Way F (BK)

#### Connector Part Information

- OEM: 15359284
- Service: 15359284
- Description: 40-Way M (BK)

#### C202 I/P to Steering Column Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-BU | 187 | Rear Fog Lamp Switch Signal (T79) | A1 | L-BU | 187 | Rear Fog Lamp Switch Signal (T79)
A2 | OG | 192 | Front Fog Lamp Switch Signal | A2 | OG | 192 | Front Fog Lamp Switch Signal
A3 | L-BU | 283 | Driver Power Seat Rear Vertical Motor Down Control | A3 | BN | 283 | Driver Power Seat Rear Vertical Motor Down Control
A4 | PK | 2111 | Steering Column Tilt Motor Up Control | A4 | PK | 2111 | Steering Column Tilt Motor Up Control
A5 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45) | A5 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45)
A5 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45)
A6 | BK | 350 | Ground | A6 | BK | 350 | Ground
A7 | BN/WH | 301 | Park Lamp Switch On Signal | A7 | BN/WH | 301 | Park Lamp Switch On Signal
A8 | PU | 1783 | Twilight Sentinel Delay Signal | A8 | PU | 1783 | Twilight Sentinel Delay Signal
B1 | WH | 103 | Headlamp Switch On Signal | B1 | WH | 103 | Headlamp Switch On Signal
B2 | L-BU | 1485 | Flash-To-Pass Switch Supply Voltage | B2 | L-BU/WH | 1485 | Flash-To-Pass Switch Supply Voltage
B3 | BN | 1356 | Flash-To-Pass Switch Signal | B3 | BN | 1356 | Flash-To-Pass Switch Signal
B4 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal | B4 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal
B5 | D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal | B5 | D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
B6 | YE | 43 | Accessory Voltage | B6 | YE | 43 | Accessory Voltage
B7 | D-BU/WH | 1415 | Right Front Turn Signal Switch Signal | B7 | D-BU/WH | 1415 | Right Front Turn Signal Switch Signal
B8 | L-BU/WH | 1414 | Left Front Turn Signal Switch Signal | B8 | L-BU/WH | 1414 | Left Front Turn Signal Switch Signal
B9 | GY | 478 | Windshield Wiper Switch Signal (2) | B9 | GY | 478 | Windshield Wiper Switch Signal (2)
GY | 478 | Windshield Wiper Switch Signal (2)
B10 | -- | -- | Not Used | B10 | -- | -- | Not Used
B11 | TN | 28 | Horn Relay Control | B11 | TN | 28 | Horn Relay Control
B12 | WH | 1538 | Headlamp On With Wipers Signal | B12 | WH | 1538 | Headlamp On With Wipers Signal
C1 | PU | 1375 | Remote Radio Control Panel Accessory Supply Voltage | C1 | PK | 1375 | Remote Radio Control Panel Accessory Supply Voltage
C2 | YE | 1491 | Backlight Lamps Control | C2 | YE | 1491 | Backlight Lamps Control
C3 | D-BU | 1796 | Steering Column Radio Control Signal | C3 | D-BU | 1796 | Steering Column Radio Control Signal
C4 | D-BU | 477 | Windshield Wiper Switch Signal (1) | C4 | D-BU | 477 | Windshield Wiper Switch Signal (1)
C5 | GY | 1884 | Cruise Control Set/Coast/Resume/Accelerate Switch Signal | C5 | L-BU/WH | 1884 | Cruise Control Set/Coast/Resume/Accelerate Switch Signal
C6 | PU | 92 | Windshield Wiper Motor High Speed Control | C6 | PU | 92 | Windshield Wiper Motor High Speed Control
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal | C8 | YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal
C9 | PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal | C9 | PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal
C10 | GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal | C10 | GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal
C11 | PK | 1239 | Run/Crank Ignition 1 Voltage | C11 | PK | 1239 | Run/Crank Ignition 1 Voltage
C12 | OG | 2154 | Steering Column Tilt Motor Signal (A45) | C12 | OG | 2154 | Steering Column Tilt Motor Signal (A45)
D1 | OG | 2153 | Steering Column Telescope Motor Signal (A45) | D1 | OG | 2153 | Steering Column Telescope Motor Signal (A45)
D2 | RD/WH | 1640 | Battery Positive Voltage | D2 | RD | 1640 | Battery Positive Voltage
D3 | D-BU | 287 | Driver Power Seat Front Vertical Motor Down Control | D3 | TN | 287 | Driver Power Seat Front Vertical Motor Down Control
D4 | OG | 2098 | Steering Column Telescope Motor Forward | D4 | OG | 2098 | Steering Column Telescope Motor Forward
D5 | OG | 2095 | Steering Column Tilt and Telescope Rearward Switch Signal | D5 | OG | 2095 | Steering Column Tilt and Telescope Rearward Switch Signal
D6 | -- | -- | Not Used | D6 | -- | -- | Not Used
D7 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45) | D7 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45)
D8 | PK | 6170 | Steering Wheel Accessory Voltage | D8 | PK | 6170 | Steering Wheel Accessory Voltage

### C204 Body to I/P Harness Left Center

#### Connector Part Information

- OEM: 10864191
- Service: NS
- Description: 26-Way F

#### Connector Part Information

- OEM: 13536441
- Service: NS
- Description: 26-Way M (GY)

#### C204 Body to I/P Harness Left Center

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BARE | 814 | Drain Wire (YQ7) | 2 | BARE | 814 | Drain Wire (YQ7)
3 | BARE | 814 | Drain Wire | 3 | BARE | 814 | Drain Wire
4 | D-BU/WH | 5338 | Right TV Audio Signal (U2K, YQ6/YQ7) | 4 | D-BU/WH | 5338 | Right TV Audio Signal (U2K, YQ6/YQ7)
5 | GY/BK | 5339 | Right TV Audio Low Reference (U2K, YQ6/YQ7) | 5 | GY/BK | 5339 | Right TV Audio Low Reference (U2K, YQ6/YQ7)
6 | L-GN/WH | 5337 | Left TV Audio Signal (U2K, YQ6/YQ7) | 6 | L-GN/WH | 5337 | Left TV Audio Signal (U2K, YQ6/YQ7)
7 | D-BU/BK | 5345 | Auxiliary Audio Screen (1) (U2K, YQ6/YQ7) | 7 | D-BU/BK | 5345 | Auxiliary Audio Screen (1) (U2K, YQ6/YQ7)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | GY | 5836 | Amplifier Audio Prompt Signal (-) (w/YQ4/YQ6/YQ7) | 9 | GY | 5836 | Amplifier Audio Prompt Signal (-) (w/YQ4/YQ6/YQ7)
10 | PU | 5837 | Amplifier Audio Prompt Signal (+) (w/YQ4/YQ6/YQ7) | 10 | PU | 5837 | Amplifier Audio Prompt Signal (+) (w/YQ4/YQ6/YQ7)
11 | BARE | 5838 | Amplifier Audio Prompt Drain Wire (YQ3/YQ4/YQ6/YQ7) | 11 | BARE | 5838 | Amplifier Audio Prompt Drain Wire (YQ3/YQ4/YQ6/YQ7)
12 | BARE | 6759 | Drain Wire | 12 | BARE | 6759 | Drain Wire
13 | YE | 599 | Left Rear Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7) | 13 | YE | 599 | Left Rear Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7)
14 | BN | 1999 | Left Rear Low Level Audio (-) (YQ3/YQ4/YQ6/YQ7) | 14 | BN | 1999 | Left Rear Low Level Audio (-) (YQ3/YQ4/YQ6/YQ7)
15 | GY | 546 | Right Rear Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7) | 15 | GY | 546 | Right Rear Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7)
16 | L-GN | 1946 | Right Rear Low Level Audio (-) (YQ3/YQ4/YQ6/YQ7) | 16 | L-GN | 1946 | Right Rear Low Level Audio (-) (YQ3/YQ4/YQ6/YQ7)
17 | D-BU | 6760 | Center Channel Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7) | 17 | D-BU | 6760 | Center Channel Low Level Audio Signal (YQ3YQ4/YQ6/YQ7)
18 | OG | 6761 | Center Channel (-) Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7) | 18 | OG | 6761 | Center Channel (-) Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7)
19 | WH | 6765 | Subwoofer Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7) (+) | 19 | WH | 6765 | Subwoofer Low Level Audio Signal (YQ3/YQ4/YQ6/YQ7)
20 | OG/BK | 6162 | Subwoofer Low Level Audio Signal (-) | 20 | OG/BK | 6162 | Subwoofer Low Level Audio Signal (-)
21 | RD | 2057 | Auxiliary Video Signal (Low) | 21 | RD | 2057 | Auxiliary Video Signal (Low)
22 | PU | 2056 | Auxiliary Video Signal (High) | 22 | PU | 2056 | Auxiliary Video Signal (High)
23 | YE | 2059 | Left Auxiliary Audio Signal | 23 | YE | 2059 | Left Auxiliary Audio Signal
24 | WH | 2058 | Right Auxiliary Audio Signal | 24 | WH | 2058 | Right Auxiliary Audio Signal
25 | BARE | 814 | Drain Wire | 25 | BARE | 814 | Drain Wire
26 | BARE | 2099 | Left Rear Audio Drain Wire (YQ3/YQ4/YQ6/YQ7) | 26 | BARE | 2099 | Left Rear Audio Drain Wire (YQ3/YQ4/YQ6/YQ7)

### C205 Body to I/P Harness Left

#### Connector Part Information

- OEM: 15448129
- Service: 15359287
- Description: 40-Way F (BK)

#### Connector Part Information

- OEM: 15475869
- Service: 15359284
- Description: 40-Way M (BK)

#### C205 Body to I/P Harness Left

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 6817 | Backlight Lamps Control | A1 | YE | 6817 | Backlight Lamps Control
A2 | -- | -- | Not Used | A2 | -- | -- | Not Used
A3 | D-BU | 287 | Driver Power Seat Front Vertical Motor Down Control | A3 | D-BU | 287 | Driver Power Seat Front Vertical Motor Down Control
A4 | OG | 2098 | Steering Column Telescope Motor Forward | A4 | OG | 2098 | Steering Column Telescope Motor Forward
A5 | PK | 2111 | Steering Column Tilt Motor Up Control | A5 | PK | 2111 | Steering Column Tilt Motor Up Control
A6 | L-BU | 283 | Driver Power Seat Rear Vertical Motor Down Control | A6 | L-BU | 283 | Driver Power Seat Rear Vertical Motor Down Control
A7 | -- | -- | Not Used | A7 | -- | -- | Not Used
A8 | YE | 6817 | Backlight Lamps Control | A8 | YE | 6817 | Backlight Lamps Control
B1 | BARE | 1705 | Drain Wire | B1 | BARE | 1705 | Drain Wire
B2 | GY | 5231 | Video RGB Low Reference | B2 | GY | 5231 | Video RGB Low Reference
B3 | WH | 17 | Stop Lamp Switch Signal | B3 | WH | 17 | Stop Lamp Switch Signal
WH | 17 | Stop Lamp Switch Signal | WH | 17 | Stop Lamp Switch Signal
B4 | PU | 1472 | Left Front Park Lamp Signal | B4 | PU | 1472 | Left Front Park Lamp Signal
B5 | PU | 709 | Left Park Lamp Supply Voltage (w/UE1, TT7/TT8) | B5 | PU | 709 | Left Park Lamp Supply Voltage (w/UE1, TT7/TT8)
B6 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal | B6 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal
B7 | D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal | B7 | D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
B8 | BN/WH | 1473 | Right Front Park Lamp Signal | B8 | BN/WH | 1473 | Right Front Park Lamp Signal
B9 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45) | B9 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45)
B10 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45) | B10 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45)
B11 | OG | 2154 | Steering Column Tilt Motor Signal (A45) | B11 | OG | 2154 | Steering Column Tilt Motor Signal (A45)
B12 | OG | 2153 | Steering Column Telescope Motor Signal (A45) | B12 | OG | 2153 | Steering Column Telescope Motor Signal (A45)
C1 | L-GN | 7396 | Driver Seat Headrest Display Video Signal (+) | C1 | L-GN | 7396 | Driver Seat Headrest Display Video Signal (+)
C2 | WH | 7394 | Driver Seat Headrest Display Video Signal (-) | C2 | WH | 394 | Driver Seat Headrest Display Video Signal (-)
C3 | BARE | 2099 | Drain Wire | C3 | BARE | 2099 | Drain Wire
C4 | D-GN/WH | 7395 | Driver Seat Headrest Display Video Mode Signal | C4 | D-GN/WH | 7395 | Driver Seat Headrest Display Video Mode Signal
C5 | PK | 6170 | Accessory Supply Voltage | C5 | PK | 6170 | Accessory Supply Voltage
C6 | TN | 6171 | Signal Input | C6 | TN | 6171 | Signal Input
C7 | TN/WH | 1974 | Left Front Speaker (-) (2) (YQ3/YQ4/YQ6/YQ7) | C7 | TN/WH | 1974 | Left Front Speaker (-) (2) (YQ3/YQ4/YQ6/YQ7)
C8 | L-BU | 1874 | Left Front Speaker (+) (2) (YQ3/YQ4/YQ6/YQ7) | C8 | L-BU | 1874 | Left Front Speaker (+) (2) (YQ3/YQ4/YQ6/YQ7)
C9 | D-GN | 5060 | Low Speed GMLAN Serial Data | C9 | D-GN | 5060 | Low Speed GMLAN Serial Data
C10 | L-GN/BK | 1209 | Left Rear Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55) | C10 | L-GN/BK | 1209 | Left Rear Strut Position Sensor Low Reference (w/TT7/TT8 w/o F55)
C11 | OG/BK | 1208 | Left Rear Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55) | C11 | OG/BK | 1208 | Left Rear Strut Position Sensor Voltage Reference (w/TT7/TT8 w/o F55)
C12 | L-GN/WH | 1210 | Left Rear Strut Position Sensor Signal (w/TT7/TT8 w/o F55) | C12 | L-GN/WH | 1210 | Left Rear Strut Position Sensor Signal (w/TT7/TT8 w/o F55)
D1 | RD/WH | 3640 | Battery Positive Voltage | D1 | RD/WH | 3640 | Battery Positive Voltage
D2 | BK/WH | 351 | Ground | D2 | BK/WH | 351 | Ground
D3 | PK | 1239 | Run/Crank Ignition 1 Voltage | D3 | PK | 1239 | Run/Crank Ignition 1 Voltage
D4 | BK | 350 | Ground | D4 | BK | 350 | Ground
BK | 350 | Ground
D5 | RD/WH | 2040 | Battery Positive Voltage | D5 | RD/WH | 2040 | Battery Positive Voltage
D6 | RD/WH | 1440 | Battery Positive Voltage | D6 | RD/WH | 1440 | Battery Positive Voltage
D7 | PK | 3 | Run/Crank Ignition 1 Voltage | D7 | PK | 3 | Run/Crank Ignition 1 Voltage
D8 | YE | 5727 | High Speed GMLAN Serial Data Wake Up (F55) | D8 | YE | 5727 | High Speed GMLAN Serial Data Wake Up (F55)

### C212 Body to Console Harness

#### Connector Part Information

- OEM: 13507762
- Service: NS
- Description: 12-Way F

#### Connector Part Information

- OEM: 13507705
- Service: NS
- Description: 12-Way M

#### C212 Body to Console Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 5756 | Front Center Speaker (+) (w/YQ2, YQ3/YQ4/YQ6/YQ7) | 1 | OG | 5756 | Front Center Speaker (+) (w/YQ2, YQ3/YQ4/YQ6/YQ7)
2 | PU/WH | 5715 | Keyless Entry Active Antenna Supply Voltage | 2 | PU/WH | 5715 | Keyless Entry Active Antenna Supply Voltage
3 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | 3 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
4 | OG/BK | 5718 | Keyless Entry Active Antenna Low Reference | 4 | OG/BK | 5718 | Keyless Entry Active Antenna Low Reference
5 | GY | 5717 | Keyless Entry Active Antenna Data Signal | 5 | GY | 5717 | Keyless Entry Active Antenna Data Signal
6 | L-BU | 5716 | Keyless Entry Active Antenna Clock Signal | 6 | L-BU | 5716 | Keyless Entry Active Antenna Clock Signal
7 | OG/BK | 5766 | Front Center Speaker (-) (YQ2, YQ3/YQ4/YQ6/YQ7) | 7 | OG/BK | 5766 | Front Center Speaker (-) (YQ2, YQ3/YQ4/YQ6/YQ7)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | TN | 219 | Keyless Entry Antenna Low Reference (1) | 9 | TN | 219 | Keyless Entry Antenna Low Reference (1)
10 | BK | 450 | Ground | 10 | BK | 450 | Ground
11 | PU | 218 | Keyless Entry Antenna Signal (1) | 11 | PU | 218 | Keyless Entry Antenna Signal (1)
12 | RD/WH | 2240 | Battery Positive Voltage | 12 | RD/WH | 2240 | Battery Positive Voltage

### C213 Rear Console to Rear Seat Harness

#### Connector Part Information

- OEM: 13534928
- Service: NS
- Description: 20-Way F (GY)

#### Connector Part Information

- OEM: 7282-5683-60
- Service: NS
- Description: 20-Way M 1.5 Series (GN)

#### C213 Rear Console to Rear Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 1634 | Right Rear A/C Seat Switch Signal | 1 | BN | 1634 | Right Rear A/C Seat Switch Signal
2 | YE | 9174 | Left Rear A/C Seat Switch Signal | 2 | YE | 9174 | Left Rear A/C Seat Switch Signal
3 | TN | 9170 | Rear A/C Seat Switch Signal | 3 | TN | 9170 | Rear A/C Seat Switch Signal
4 | L-BU | 9330 | Left Rear A/C Seat High Indicator Control | 4 | L-BU | 9330 | Left Rear A/C Seat High Indicator Control
5 | TN | 9170 | Rear A/C Seat Switch Signal | 5 | TN | 9170 | Rear A/C Seat Switch Signal
6 | YE | 9174 | Left Rear A/C Seat Switch Signal | 6 | YE | 9174 | Left Rear A/C Seat Switch Signal
7 | BN | 1634 | Right Rear A/C Seat Switch Signal | 7 | BN | 1634 | Right Rear A/C Seat Switch Signal
8 | GY | 9177 | Left Rear A/C Seat Medium Indicator Control | 8 | GY | 9177 | Left Rear A/C Seat Medium Indicator Control
9 | TN/WH | 1635 | Right Rear A/C Seat High Indicator Control | 9 | TN/WH | 1635 | Right Rear A/C Seat High Indicator Control
10 | D-BU/WH | 6586 | Right Rear A/C Seat Medium Indicator Control | 10 | D-BU/WH | 6586 | Right Rear A/C Seat Medium Indicator Control
11 | PK | 1636 | Right Rear A/C Seat Low Indicator Control | 11 | PK | 1636 | Right Rear A/C Seat Low Indicator Control
12 | L-GN/BK | 9337 | Rear A/C Seat Indicator Control | 12 | L-GN/BK | 9337 | Rear A/C Seat Indicator Control
13 | L-GN/BK | 9337 | Rear A/C Seat Indicator Control | 13 | L-GN/BK | 9337 | Rear A/C Seat Indicator Control
14 | PK | 1636 | Right Rear A/C Seat Low Indicator Control | 14 | PK | 1636 | Right Rear A/C Seat Low Indicator Control
15 | D-BU/WH | 6586 | Right Rear A/C Seat Medium Indicator Control | 15 | D-BU/WH | 6586 | Right Rear A/C Seat Medium Indicator Control
16 | TN/WH | 1635 | Right Rear A/C Seat High Indicator Control | 16 | TN/WH | 1635 | Right Rear A/C Seat High Indicator Control
17 | D-GN/WH | 9176 | Left Rear A/C Seat Low Indicator Control | 17 | D-GN/WH | 9176 | Right Rear A/C Seat Low Indicator Control
18 | L-BU | 9330 | Left Rear A/C Seat High Indicator Control | 18 | L-BU | 9330 | Left Rear A/C Seat High Indicator Control
19 | GY | 9177 | Left Rear A/C Seat Medium Indicator Control | 19 | GY | 9177 | Left Rear A/C Seat Medium Indicator Control
20 | D-GN/WH | 9176 | Left Rear A/C Seat Low Indicator Control | 20 | D-GN/WH | 9176 | Left Rear A/C Seat Low Indicator Control

### C214 HVAC Motor Assembly

#### Connector Part Information

- OEM: 10847013
- Service: NS
- Description: 16-Way F (GN)

#### Connector Part Information

- OEM: 7282-5683-60
- Service: NS
- Description: 16-Way M YESC 1.5 (GY)

#### C214 HVAC Motor Assembly

Pin | Wire | Circuit No | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GY/BK | 2778 | Passenger Air Temperature Motor Control | 1 | GY/BK | 2778 | Passenger Air Temperature Motor Control
2 | WH/BK | 1236 | Passenger Air Temperature Door Control | 2 | WH/BK | 1236 | Passenger Air Temperature Door Control
3 | D-BU | 1646 | Passenger Air Temperature Door Position Signal | 3 | D-BU | 1646 | Passenger Air Temperature Door Position Signal
4 | YE | 1318 | Lower Mode Door Control | 4 | YE/GN | 1318 | Lower Mode Door Control
5 | TN | 2273 | Mode Door Control | 5 | TN | 2273 | Mode Door Control
6 | YE/BK | 1814 | Lower Mode Door Position Signal | 6 | YE/BK | 1814 | Lower Mode Door Position Signal
7 | D-GN | 5518 | Passenger Compartment Rear Air Temperature Sensor Signal | 7 | D-GN | 5518 | Passenger Compartment Rear Air Temperature Sensor Signal
8 | L-BU | 5517 | Passenger Compartment Rear Air Temperature Sensor Low Reference | 8 | L-BU | 5517 | Passenger Compartment Rear Air Temperature Sensor Low Reference
9 | BN | 5516 | Passenger Compartment Rear Air Temperature Motor Control | 9 | BN | 5516 | Passenger Compartment Rear Air Temperature Motor Control
10 | GY | 705 | 5-Volt Reference | 10 | GY | 705 | 5-Volt Reference
11 | YE | 1791 | Air Temperature Door Control Low Reference | 11 | TN/RD | 1791 | Air Temperature Door Control Low Reference
12 | L-BU | 733 | Air Temperature Door Position Signal | 12 | L-BU | 733 | Air Temperature Door Position Signal
13 | D-BU | 1199 | Air Temperature Door Control | 13 | D-BU | 1199 | Air Temperature Door Control
14 | YE | 61 | Outside Ambient Temperature Sensor Low Reference | 14 | YE | 61 | Outside Ambient Temperature Sensor Low Reference
15 | GY | 731 | A/C Refrigerant Low Temperature Sensor Signal | 15 | GY | 731 | A/C Refrigerant Low Temperature Sensor Signal
16 | -- | -- | Not Used | 16 | -- | -- | Not Used

### C217 Inflatable Restraint Module to Body Harness (Passenger)

#### Connector Part Information

- OEM: 15336478
- Service: N/A
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: N/A
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### C217 Inflatable Restraint Module to Body Harness (Passenger)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 1403 | Passenger I/P Module High Control | A1 | WH/BK | 1403 | Passenger I/P Module High Control
A2 | OG | 1404 | Passenger I/P Module Low Control | A2 | D-GN/WH | 1404 | Passenger I/P Module Low Control
B1 | GY | 3027 | Passenger I/P Module Stage 2 High Control | B1 | GY | 3027 | Passenger I/P Module Stage 2 High Control
B2 | PU | 3026 | Passenger I/P Module Stage 2 Low Control | B2 | PU | 3026 | Passenger I/P Module Stage 2 Low Control

### C218 Inflatable Restraint Steering Wheel Module to Body Harness (Driver)

#### Connector Part Information

- OEM: 15336478
- Service: N/A
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: N/A
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### C218 Inflatable Restraint Steering Wheel Module to Body Harness (Driver)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | TN | 3021 | Steering Wheel Module Stage 1 High Control | A1 | TN | 3021 | Steering Wheel Module Stage 1 High Control
A2 | BN | 3020 | Steering Wheel Module Stage 1 Low Control | A2 | BN | 3020 | Steering Wheel Module Stage 1 Low Control
B1 | WH | 3023 | Steering Wheel Module Stage 2 High Control | B1 | WH | 3023 | Steering Wheel Module Stage 2 High Control
B2 | PK | 3022 | Steering Wheel Module Stage 2 Low Control | B2 | PK | 3022 | Steering Wheel Module Stage 2 Low Control

### C276 Steering Column Harness

#### Connector Part Information

- OEM: 12064769
- Service: NS
- Description: 10-Way F Metri-Pack 150 Series (NA)

#### Connector Part Information

- OEM: 12064770
- Service: NS
- Description: 10-Way M Metri-Pack 150 Series (NA)

#### C276 Steering Column Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 28 | Horn Relay Control | A | TN | 28 | Horn Relay Control
B | BK | 350 | Ground | B | BK | 350 | Ground
C | D-BU | -- | Internal Wiring | C | -- | -- | Not Used
D | WH | 1239 | Run/Crank Ignition 1 Voltage | D | WH | 1239 | Run/Crank Ignition 1 Voltage
E | PU | 350 | Ground | E | BK | 350 | Ground
F | OG | 1491 | Backlight Lamps Control | F | YE | 1491 | Backlight Lamps Control
G | L-GN | 1796 | ACC Gap Adjustment/Radio Control Signal | G | D-BU | 1796 | ACC Gap Adjustment/Radio Control Signal
H | PK | 1375 | Remote Radio Control Head Accessory Voltage Supply Voltage | H | PK | 1375 | Remote Radio Control Head Accessory Voltage Supply Voltage
J | YE | -- | Internal Wiring | J-K | -- | -- | Not Used
K | L-BU | -- | Internal Wiring

### C277 Steering Column Harness

#### Connector Part Information

- OEM: 12064769
- Service: NS
- Description: 10-Way F Metri-Pack 150 Series (NA)

#### Connector Part Information

- OEM: 12064770
- Service: NS
- Description: 10-Way M Metri-Pack 150 Series (NA)

#### C277 Steering Column Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK | 28 | Horn Relay Control | A | -- | -- | Not Used
B | PU | 350 | Ground | B | D-GN/WH | 350 | Ground
C | -- | -- | Not Used | C | GY | -- | Internal Wire
D | BN | 1239 | Run/Start Ignition 1 Voltage | D | BN | 1239 | Run/Start Ignition 1 Voltage
E | BK | 350 | Ground | E | PU | 350 | Ground
F | YE | 1491 | Backlight Control | F | PU/WH | 1491 | Backlight Control
G | D-BU | 1796 | ACC DIstance Adjustment/Radio Control Signal | G | L-GN | 1796 | ACC Distance Adjustment/Radio Control Signal
H | BK | 1375 | Remote Radio Control Panel Accessory Supply Voltage | H | BK | 1375 | Remote Radio Control Panel Accessory Supply Voltage
J | TN | 6170 | Voltage Reference Signal | J | GY | 6170 | Voltage Reference Signal
K | GY | 6171 | Signal Input | K | BK | 6171 | Signal Input

### C300 Body to Driver Seat Harness

#### Connector Part Information

- OEM: 10864191
- Service: NS
- Description: 26-Way F (BK)

#### Connector Part Information

- OEM: 7282-6376-30
- Service: NS
- Description: 26-Way M Hybrid (GY)

#### C300 Body to Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Battery Positive Voltage | 1 | RD/WH | 3740 | Battery Positive Voltage
2 | RD/WH | 2840 | Battery Positive Voltage | 2 | RD/WH | 2840 | Battery Positive Voltage
3 | OG | 5919 | Driver Seat Fan Speed Control | 3 | OG | 5919 | Driver Seat Fan Speed Control
4-5 | -- | -- | Not Used | 4-5 | -- | -- | Not Used
6 | BK/WH | 551 | Signal Ground | 6 | BK/WH | 551 | Signal Ground
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | BK | 550 | Ground | 8 | BK | 550 | Ground
9 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45) | 9 | TN | 782 | Memory Seat/Mirror Sensor Low Reference (A45)
10 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45) | 10 | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference (A45)
11 | OG | 2154 | Steering Column Tilt Motor Signal (A45) | 11 | OG | 2154 | Steering Column Tilt Motor Signal (A45)
12 | OG | 2153 | Steering Column Telescope Motor Signal (A45) | 12 | OG | 2153 | Steering Column Telescope Motor Signal (A45)
13 | PU | 5611 | Passenger Set Belt Tension Sensor Signal | 13 | PU | 5611 | Passenger Set Belt Tension Sensor Signal
14 | TN/WH | 238 | Driver Seat Belt Switch Signal | 14 | TN/WH | 238 | Driver Seat Belt Switch Signal
15 | PK | 5017 | Driver Seat Belt Switch Low Reference | 15 | PK | 5017 | Driver Seat Belt Switch Low Reference
16 | BK/WH | 551 | Signal Ground | 16 | BK/WH | 551 | Signal Ground
17 | D-GN | 5757 | Driver Seat Left Speaker (+) | 17 | D-GN | 5757 | Driver Seat Left Speaker (+)
18 | D-GN/WH | 5767 | Driver Seat Left Speaker (-) | 18 | D-GN/WH | 5767 | Driver Seat Left Speaker (-)
19 | GY | 5758 | Driver Seat Right Speaker (+) | 19 | GY | 5758 | Driver Seat Right Speaker (+)
20 | GY/BK | 5768 | Driver Seat Right Speaker (-) | 20 | GY/BK | 5768 | Driver Seat Right Speaker (-)
21 | D-GN | 5060 | Low Speed GMLAN Serial Data | 21 | D-GN | 5060 | Low Speed GMLAN Serial Data
22 | PK | 2077 | Driver Heated Seat Element Supply Voltage (KA1/KB6) | 22 | PK | 2077 | Driver Heated Seat Element Supply Voltage (KA1/KB6)
23 | GY | 791 | PWM Serial Data (KA1/KB6) | 23 | GY | 791 | PWM Serial Data (KA1/KB6)
24 | WH | 790 | PWM Serial Data (KA1/KB6) | 24 | WH | 790 | PWM Serial Data (KA1/KB6)
25 | YE/BK | 2079 | Driver Heated Seat NTC Signal (KA1/KB6) | 25 | YE/BK | 2079 | Driver Heated Seat NTC Signal (KA1/KB6)
26 | YE | 2080 | Driver Heated Seat NTC Low Reference (KA1/KB6) | 26 | YE | 2080 | Driver Heated Seat NTC Low Reference (KA1/KB6)

### C301 Body to Driver Seat Harness

#### Connector Part Information

- OEM: 10847017
- Service: NS
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 7282-5622-40
- Service: NS
- Description: 14-Way M YESC Hybrid (GY)

#### C301 Body to Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | 2111 | Steering Column Tilt Motor Up Control | 1 | PK | 2111 | Steering Column Tilt Motor Up Control
2 | RD/WH | 3240 | Battery Positive Voltage | 2 | RD/WH | 3240 | Battery Positive Voltage
3 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage | 3 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage
4 | D-GN | 7396 | Driver Seat Headrest Display Video Signal (+) | 4 | D-GN | 7.96 | Driver Seat Headrest Display Video Signal (+)
5 | D-GN/WH | 7395 | Driver Seat Headrest Display Video Mode Signal | 5 | D-GN/WH | 7395 | Driver Seat Headrest Display Video Mode Signal
6 | D-BU/WH | 149 | Left Front Seat Indicator Power Supply | 6 | D-BU/WH | 149 | Left Front Seat Indicator Power Supply
7 | OG | 2098 | Steering Column Telescope Motor Forward | 7 | OG | 2098 | Steering Column Telescope Motor Forward
8 | L-BU | 283 | Driver Power Seat Rear Vertical Motor Down Control | 8 | L-BU | 283 | Driver Power Seat Rear Vertical Motor Down Control
9 | BK/WH | 551 | Ground | 9 | BK/WH | 551 | Ground
10 | BARE | 2099 | Drain Wire | 10 | BARE | 2099 | Drain Wire
11 | WH | 7394 | Driver Seat Headrest Display Video Signal (-) | 11 | WH | 7394 | Driver Seat Headrest Display Video Signal (-)
12 | PK/BK | 5844 | Seat Headrest Display Height Adjusting Signal | 12 | PK/BK | 5844 | Seat Headrest Display Height Adjusting Signal
13 | GY | 157 | Left Front Seat Indicator Ground | 13 | GY | 157 | Left Front Seat Indicator Ground
14 | D-BU | 287 | Driver Power Seat Front Vertical Motor Down Control | 14 | D-BU | 287 | Driver Power Seat Front Vertical Motor Down Control

### C302 Body to Rear Seat Harness

#### Connector Part Information

- OEM: 10726722
- Service: NS
- Description: 6-Way F (GY)

#### Connector Part Information

- OEM: 7282-5536-40
- Service: NS
- Description: 16-Way M (GY)

#### C302 Body to Rear Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Battery Positive Voltage | 1 | RD/WH | 3740 | Battery Positive Voltage
2 | BN | 341 | Ignition 3 Voltage | 2 | BN | 341 | Ignition 3 Voltage
3 | BK | 550 | Ground | 3 | BK | 550 | Ground
4 | BK | 650 | Ground | 4 | BK | 650 | Ground
5 | BN | 2341 | Right Rear A/C Seat Module Power Supply | 5 | BN | 2341 | Right Rear A/C Seat Module Power Supply
6 | BN | 1341 | Left Rear A/C Seat Cooling Motor Positive | 6 | BN | 1341 | Left Rear A/C Seat Cooling Motor Positive

### C302 Body to Rear Seat Harness (w/o Heated Seats)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Power Supply | 1 | RD/WH | 3740 | Power Supply
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | BK | 550 | Ground | 3 | BK | 550 | Ground
4 | BK | 650 | Ground | 4 | BK | 650 | Ground
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used

### C304 Console to I/P Harness

#### Connector Part Information

- OEM: 13506916
- Service: NS
- Description: 16-Way F (BU)

#### Connector Part Information

- OEM: 13507436
- Service: NS
- Description: 16-Way M (BU)

#### C304 Console to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | GY | 705 | 5-Volt Reference | 2 | GY | 705 | 5-Volt Reference
3-4 | -- | -- | Not Used | 3 | -- | -- | Not Used
5 | YE | 61 | Outside Ambient Temperature Sensor Low Reference | 5 | YE | 61 | Outside Ambient Temperature Sensor Low Reference
6 | BN/WH | 1571 | Traction Control Switch Signal (2) | 6 | BN/WH | 1571 | Traction Control Switch Signal (2)
7 | PK | 111 | Hazard Switch Signal | 7 | WH | 111 | Hazard Switch Signal
8 | YE | 6817 | Backlight Lamps Control | 8 | YE | 6817 | Backlight Lamps Control
YE | 6817 | Backlight Lamps Control | YE | 6817 | Backlight Lamps Control
9 | L-GN/BK | 5730 | Rear Mode Door Control B | 9 | L-GN/BK | 5730 | Rear Mode Door Control B
10 | L-GN/WH | 5729 | Rear Mode Door Control A | 10 | L-GN/WH | 5729 | Rear Mode Door Control A
11 | GY | 2599 | Rear Mode Door Position Signal | 11 | GY | 2599 | Rear Mode Door Position Signal
12-16 | -- | -- | Not Used | 12 | -- | -- | Not Used

### C305 Headliner to Body Harness

#### Connector Part Information

- OEM: 7283-6388-40
- Service: NS
- Description: 16-Way F Yazaki (GY)

#### Connector Part Information

- OEM: 13507436
- Service: NS
- Description: 16-Way M Yazaki (GY)

#### C305 Headliner to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage | 1 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage
2 | BK | 1489 | Noise Reduction Microphone Drain Wire (YQ3/YQ4/YQ6/YQ7) | 2 | BK | 1489 | Noise Reduction Microphone Drain Wire (YQ3/YQ4/YQ6/YQ7)
3 | D-GN | 1488 | Noise Reduction Microphone (+) (YQ3/YQ4/YQ6/YQ7) | 3 | D-GN | 1488 | Noise Reduction Microphone (+) (YQ3/YQ4/YQ6/YQ7)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | OG/BK | 5851 | Audio Remote Control Signal | 5 | OG/BK | 5831 | Audio Remote Control Signal
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BK/WH | 851 | Ground | 7 | BK/WH | 851 | Ground
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | WH | 2370 | Rear Park Lamp Display Supply Voltage | 9 | WH | 2370 | Rear Park Lamp Display Supply Voltage
10 | OG | 2371 | Left Amber Indicator Control | 10 | OG | 2371 | Left Amber Indicator Control
11 | D-BU | 2372 | Center Amber Indicator Control | 11 | D-BU | 2372 | Center Amber Indicator Control
12 | GY | 2373 | Rear Parking Assist Red Indicator Control | 12 | GY | 2373 | Rear Parking Assist Red Indicator Control
13-14 | -- | -- | Not Used | 13 | -- | -- | Not Used
15 | BK | 580 | Ground | 15 | BK | 850 | Ground
16 | YE | 1491 | Backlight Lamp Control (CF5) | 16 | YE | 1491 | Backlight Lamp Control (CF5)

### C306 Body to Front Passenger Seat

#### Connector Part Information

- OEM: 10847017
- Service: N/A
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 7283-6447-40
- Service: NS
- Description: 14-Way M (GY)

#### C306 Body to Front Passenger Seat

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BK/WH | 651 | Ground | 2 | BK/WH | 651 | Ground
3 | D-GN | 6975 | Front Passenger Seat Headrest Display Video Signal (+) | 3 | D-GN | 6975 | Front Passenger Seat Headrest Display Video Signal (+)
4 | D-GN/WH | 5845 | Front Passenger Seat Headrest Display Video Analog Signal | 4 | D-GN/WH | 5845 | Front Passenger Seat Headrest Display Video Analog Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | 6 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
7-9 | -- | -- | Not Used | 8 | -- | -- | Not Used
10 | BARE | 6976 | Drain Wire | 10 | BARE | 6976 | Drain Wire
11 | WH/BK | 5335 | Front Passenger Seat Headrest Display Video Signal (-) | 11 | WH/BK | 5335 | Front Passenger Seat Headrest Display Video Signal (-)
12 | PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal | 12 | PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal
PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal | PK/BK | 5844 | Seat Headrest Display Brightness Adjusting Signal
13 | GY | 157 | Door Lighting Control | 13 | GY | 157 | Door Lighting Control
14 | -- | -- | Not Used | 14 | -- | -- | Not Used

### C307 Body to Front Passenger Seat

#### Connector Part Information

- OEM: 10864191
- Service: NS
- Description: 26-Way F (BK)

#### Connector Part Information

- OEM: 7282-6376-30
- Service: NS
- Description: 26-Way M (GY)

#### C307 Body to Front Passenger Seat

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Battery Positive Voltage | 1 | RD/WH | 3740 | Battery Positive Voltage
2 | RD/WH | 2540 | Battery Positive Voltage (w/KA1/KB6) | 2 | RD/WH | 2540 | Battery Positive Voltage (w/KA1/KB6)
3 | PK | 1139 | Ignition 1 Voltage | 3 | PK | 1139 | Ignition 1 Voltage
4 | BN | 41 | Run Ignition 3 Voltage (KB1/KA6) | 4 | BN | 41 | Run Ignition 3 Voltage (KB1/KA6)
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | RD/WH | 3240 | Battery Positive Voltage | 6 | RD/WH | 3240 | Battery Positive Voltage
7 | OG | 5919 | Driver Seat Fan Speed Control (KB6) | 7 | OG | 5919 | Driver Seat Fan Speed Control (KB6)
8 | BK | 650 | Ground | 8 | BK | 650 | Ground
9 | D-BU | 2307 | Airbag ON Signal | 9 | D-BU | 2307 | Airbag ON Signal
10 | D-GN | 2308 | Airbag OFF Signal | 10 | D-GN | 2308 | Airbag OFF Signal
11 | PK | 5018 | Passenger Seat Pressure Sensor Serial Data | 11 | PK | 5018 | Passenger Seat Pressure Sensor Serial Data
12 | BK/WH | 1751 | Ground | 12 | BK/WH | 1751 | Ground
13 | PU | 5611 | Passenger Seat Belt Tension Sensor Signal | 13 | PU | 5611 | Passenger Seat Belt Tension Sensor Signal
14 | TN/WH | 238 | Driver Seat Belt Switch Signal | 14 | TN/WH | 238 | Driver Seat Belt Switch Signal
15 | PK | 5017 | Driver Seat Belt Switch Low Reference | 15 | PK | 5017 | Driver Seat Belt Switch Low Reference
16 | BK/WH | 651 | Ground | 16 | BK/WH | 651 | Ground
17 | YE | 5759 | Right Front Seat Left Speaker (+) (YQ3/YQ4/YQ6/YQ7) | 17 | YE | 5759 | Right Front Seat Left Speaker (+) (YQ3/YQ4/YQ6/YQ7)
18 | YE/BK | 5769 | Right Front Seat Left Speaker (-) (YQ3/YQ4/YQ6/YQ7) | 18 | YE/BK | 5769 | Right Front Seat Left Speaker (-) (YQ3/YQ4/YQ6/YQ7)
19 | L-GN | 5760 | Right Front Seat Right Speaker (+) (YQ3/YQ4/YQ6/YQ7) | 19 | L-GN | 5760 | Right Front Seat Left Speaker (+) (YQ3/YQ4/YQ6/YQ7)
20 | L-GN/BK | 5770 | Right Front Seat Right Speaker (-) (YQ3/YQ4/YQ6/YQ7) | 20 | L-GN/BK | 5770 | Right Front Seat Right Speaker (-) (YQ3/YQ4/YQ6/YQ7)
21 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage | 21 | PK | 5165 | Antenna 14-Volt Switched Supply Voltage
22 | PK | 2077 | Driver Heated Seat Element Supply voltage (KA1/KB6) | 22 | PK | 2270 | Driver Heated Seat Element Supply voltage (KA1/KB6)
23 | GY | 791 | PWM Serial Data (KA1/KB6) | 23 | GY | 791 | PWM Serial Data (KA1/KB6)
24 | WH | 790 | PWM Serial Data (KA1/KB6) | 24 | WH | 790 | PWM Serial Data (KA1/KB6)
25 | YE/BK | 2079 | Driver Heated Seat NTC Signal (KA1/KB6) | 25 | YE/BK | 2079 | Driver Heated Seat NTC Signal (KA1/KB6)
26 | YE | 2080 | Driver Heated Seat NTC Low Reference (KA1/KB6) | 26 | YE | 2080 | Driver Heated Seat NTC Low Reference (KA1/KB6)

### C308 Headliner to Body

#### Connector Part Information

- OEM: 7283-6456-90
- Service: NS
- Description: 16-Way F YESC Yazaki (BU)

#### Connector Part Information

- OEM: 7282-6456-90
- Service: NS
- Description: 16-Way M YESC Yazaki (BU)

#### C308 Headliner to Body

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | PK | 1339 | Run/Crank Ignition 1 Voltage | 3 | PK | 1339 | Run/Crank Ignition 1 Voltage
4 | YE | 6817 | Backlight Lamps Control | 4 | YE | 6817 | Backlight Lamps Control
5 | GY | 655 | Cellular Telephone Microphone Signal | 5 | GY | 655 | Cellular Telephone Microphone Signal
6 | BARE | 1782 | Drain Wire | 6 | BARE | 1782 | Drain Wire
7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | 7 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
8 | GY | 157 | Interior Lamp Control | 8 | GY | 157 | Interior Lamp Control
9 | L-GN/BK | 5711 | Keyless Entry Antenna Low Reference (2) | 9 | L-GN/BK | 5711 | Keyless Entry Antenna Low Reference (2)
10 | L-GN | 5707 | Keyless Entry Antenna Signal (2) | 10 | L-GN | 5707 | Keyless Entry Antenna Signal (2)
11 | PK | 1691 | Automatic Day/Night Mirror Low Reference | 11 | PK | 1691 | Automatic Day/Night Mirror Low Reference
12 | GY | 1690 | Automatic Day/Night Mirror Signal | 12 | GY | 1690 | Automatic Day/Night Mirror Signal
13 | PK | 1339 | Run/Crank Ignition 1 Voltage | 13 | PK | 1339 | Run/Crank Ignition 1 Voltage
14 | L-GN | 24 | Backup Lamp Supply Voltage | 14 | L-GN | 24 | Backup Lamp Supply Voltage
15 | -- | -- | Not Used | 15 | -- | -- | Not Used
16 | OG/BK | 2332 | Switch Signal | 16 | OG/BK | 2332 | Switch Signal
17 | D-GN | 2308 | Air Bag OFF Signal | 17 | D-GN | 2308 | Air Bag OFF Signal
18 | D-BU | 2307 | Air Bag ON Signal | 18 | D-BU | 2307 | Air Bag ON Signal
19 | PU | 5234 | Passenger Seat Belt Indicator Signal | 19 | PU | 5234 | Passenger Seat Belt Indicator Signal
20 | PK | 1139 | Ignition 1 Voltage | 20 | PK | 1139 | Ignition 1 Voltage

### C309 Sunroof Jumper (CF5) to Headliner

#### Connector Part Information

- OEM: 7283-6456-90
- Service: NS
- Description: 10-Way F YESC 1.5 (L-GY)

#### Connector Part Information

- OEM: 10846817
- Service: NS
- Description: 10-Way M (GY)

#### C309 Sunroof Jumper (CF5) to Headliner

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | L-BU | 5027 | Sunroof Switch - Data (1) | 2 | L-BU | 5027 | Sunroof Switch - Data (1)
3 | BN | 5028 | Sunroof Switch - Data (2) | 3 | BN | 5028 | Sunroof Switch - Data (2)
4 | OG | 5029 | Sunroof Switch - Data (3) | 4 | OG | 5029 | Sunroof Switch - Data (3)
5 | PK | 5031 | Sunroof Switch - Data (5) | 5 | PK | 5031 | Sunroof Switch - Data (5)
6 | PU | 5032 | Sunroof Switch - Data (6) | 6 | PU | 5032 | Sunroof Switch - Data (6)
7 | TN | 5030 | Sunroof Switch - Data (4) | 7 | TN | 5030 | Sunroof Switch - Data (4)
8-10 | -- | -- | Not Used | 8-10 | -- | -- | Not Used

### C310 Sunroof (CF5) to Body

#### Connector Part Information

- OEM: 7283-5628-40
- Service: NS
- Description: 3-Way F YESC Class 3 (L-GY)

#### Connector Part Information

- OEM: 15342668
- Service: NS
- Description: 3-Way M (L-GY)

#### C310 Sunroof (CF5) to Body

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 1050 | Ground | 1 | BK | 1050 | Ground
2 | BK | 755 | Sunroof Enable Signal | 2 | TN | 755 | Sunroof Enable Signal
3 | D-BU | 2640 | Battery Positive Voltage | 3 | RD/WH | 2640 | Battery Positive Voltage

### C312 Driver Lumbar to Driver Seat (AL2 w/o A45)

#### Connector Part Information

- OEM: 12129136
- Service: N/A
- Description: 4-Way F Metri-Pack 280 Series, Flexlock (BK)

#### Connector Part Information

- OEM: 12129135
- Service: N/A
- Description: 4-Way M Metri-Pack 280 Series (BK)

#### C312 Driver Lumbar to Driver Seat (AL2 w/o A45)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 768 | Driver Seat Lumbar Motor Up Control | A | L-GN | 768 | Driver Seat Lumbar Motor Up Control
B | L-GN | 284 | Driver Seat Horizontal Motor Rearward Control | B | BN | 284 | Driver Seat Horizontal Motor Rearward Control
C | D-BU | 611 | Driver Seat Lumbar Motor Forward Control | C | D-BU | 611 | Driver Seat Lumbar Motor Forward Control
D | PK | 610 | Driver Seat Lumbar Motor Rearward Control | D | PK | 610 | Driver Seat Lumbar Motor Rearward Control

### C313 Passenger Lumbar to Passenger Seat (AL2)

#### Connector Part Information

- OEM: 12129136
- Service: N/A
- Description: 4-Way F Metri-Pack 280 Series, Flexlock (BK)

#### Connector Part Information

- OEM: 12129135
- Service: N/A
- Description: 4-Way M Metri-Pack 280 Series (BK)

#### C313 Passenger Lumbar to Passenger Seat (AL2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 768 | Driver Seat Lumbar Motor Up Control | A | L-GN | 768 | Driver Seat Lumbar Motor Up Control
B | L-GN | 284 | Driver Seat Horizontal Motor Rearward Control | B | L-GN | 284 | Driver Seat Horizontal Motor Rearward Control
C | D-BU | 611 | Driver Seat Lumbar Motor Forward Control | C | D-BU | 611 | Driver Seat Lumbar Motor Forward Control
D | PK | 610 | Driver Seat Lumbar Motor Rearward Control | D | PK | 610 | Driver Seat Lumbar Motor Rearward Control

### C317 Driver Seat Harness to Body Harness

#### Connector Part Information

- OEM: 15304656
- Service: N/A
- Description: 2-Way F 280 Series (YE)

- OEM: 15304653
- Service: N/A
- Description: 4-Way F GT 150/280 Series (YE)

#### Connector Part Information

- OEM: 15304649
- Service: 15306061
- Description: 6-Way M GT 150/280 Series (YE)

#### C317 Driver Seat Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 2118 | Driver Seat Belt Pretensioner High Control | A | TN/WH | 2118 | Driver Seat Belt Pretensioner High Control
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BN | 2105 | Left Side Impact Module High Control | C | D-GN | 2105 | Left Side Impact Module High Control
D | D-GN | 2106 | Side Impact Module - Left Low Control | D | BN | 2106 | Side Impact Module - Left Low Control
E | -- | -- | Not Used | E | -- | -- | Not Used
F | WH | 2119 | Driver Seat Belt Pretensioner Low Control | F | OG/BK | 2119 | Driver Seat Belt Pretensioner Low Control

### C318 Passenger Seat Harness to Body Harness

#### Connector Part Information

- OEM: 15304656
- Service: N/A
- Description: 2-Way F 280 Series (YE)

- OEM: 15304653
- Service: N/A
- Description: 4-Way F GT 150/280 Series (YE)

#### Connector Part Information

- OEM: 15304649
- Service: 15306061
- Description: 6-Way M GT 150/280 Series (YE)

#### C318 Passenger Seat Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 2116 | Passenger Seat Belt Pretensioner High Control | A | L-GN | 2116 | Passenger Seat Belt Pretensioner High Control
B | -- | -- | Not Used | B | -- | -- | Not Used
C | WH | 2104 | Side Impact Module - Right Low Control | C | GY | 2104 | Side Impact Module - Right Low Control
D | D-GN | 2103 | Side Impact Module - Right High Control | D | D-BU | 2103 | Side Impact Module - Right High Control
E | -- | -- | Not Used | E | -- | -- | Not Used
F | WH | 2117 | Passenger Seat Belt Pretensioner Low Control | F | OG | 2117 | Passenger Seat Belt Pretensioner Low Control

### C319 Lumbar Motor Position Sensor - Driver to Driver Seat Harness (A45)

#### Connector Part Information

- OEM: 12047785
- Service: N/A
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: N/A
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### C319 Lumbar Motor Position Sensor - Driver to Driver Seat Harness (A45)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 782 | Memory Seat/Mirror Sensor Low Reference | A | TN | 782 | Memory Seat/Mirror Sensor Low Reference
B | TN | 1062 | Driver Memory Seat Lumbar Vertical Position Sensor Signal | B | TN | 1062 | Driver Memory Seat Lumbar Vertical Position Sensor Signal
C | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference | C | GY | 788 | Memory Mirror Position Sensor 5-Volt Reference
D | YE | 1063 | Driver Memory Seat Lumbar Horizontal Position Sensor Signal | D | YE | 1063 | Driver Memory Seat Lumbar Horizontal Position Sensor Signal

### C320 Body to Rear I/P Harness

#### Connector Part Information

- OEM: 10864191
- Service: N/A
- Description: 26-Way F

#### Connector Part Information

- OEM: 15386268
- Service: N/A
- Description: 26-Way M (BK)

#### C320 Body to Body Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3240 | Battery Positive Voltage | 1 | RD/WH | 3240 | Left Rear Fuse
2 | BN | 41 | Run Ignition 3 Voltage | 2 | BN | 41 | Left Rear Fuse
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | PU | 2056 | Auxiliary Video High Signal (+) | 4 | PU | 2056 | Auxiliary Video High Signal (+)
5 | RD | 2057 | Auxiliary Video High Signal (-) | 5 | RD | 2057 | Auxiliary Video High Signal (-)
6 | BARE | 814 | Drain Wire | 6 | BARE | 814 | Drain Wire
7 | YE | 6817 | Backlight Lamps Control | 7 | YE | 6817 | I/P Backlight Lamp Control Output
8 | BK/WH | 851 | Ground | 8 | BK/WH | 851 | Ground
9 | D-BU/BK | 5314 | LR Low Level Audio (-) | 9 | D-BU/BK | 5314 | Left Rear Audio Input (-)
10 | D-BU/WH | 5312 | LR Row Level Audio Signal | 10 | D-BU/WH | 5312 | Left Rear Audio Input (+)
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used
13 | YE | 2059 | Left Auxiliary Amplifier Audio Prompt Signal (+) | 13 | YE | 2059 | Left Auxiliary Amplifier Audio Prompt Signal (+)
14 | WH | 2058 | Right Auxiliary Amplifier Audio Prompt Signal (+) | 14 | WH | 2058 | Right Auxiliary Amplifier Audio Prompt Signal (+)
15 | YE | 599 | LR Low Level Audio Signal | 15 | YE | 599 | LR Low Level Audio Signal
16 | BN | 1999 | LR Low Level Audio (-) | 16 | BN | 1999 | LR Low Level Audio (-)
17 | BARE | 2099 | Drain Wire | 17 | BARE | 2099 | Drain Wire
18 | GY/BK | 5830 | RR Low Level Audio (-) | 18 | GY/BK | 5830 | Right Rear Audio Output (-)
19 | D-GN/WH | 5313 | RR Low Level Audio Signal | 19 | D-GN/WH | 5313 | Right Rear Audio Output (+)
20-21 | -- | -- | Not Used | 20-21 | -- | -- | Not Used
22 | D-GN | 5060 | Low Speed GMLAN Serial Data | 22 | D-GN | 5060 | Low Speed GMLAN Serial Data
23 | BARE | 814 | Drain Wire | 23 | BARE | 814 | Drain Wire
24 | GY | 546 | RR Low Level Audio Signal | 24 | GY | 546 | RR Low Level Audio Signal
25 | D-GN | 1946 | RR Low Level Audio (-) | 25 | D-GN | 1946 | RR Low Level Audio (-)
26 | BARE | 2099 | Drain Wire | 26 | BARE | 2099 | Drain Wire

### C321 Left Rear Seat Cushion to Left Rear Seat Harness C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Left Rear Heated Seat Supply Voltage | 1 | RD/WH | 3740 | Left Rear Heated Seat Supply Voltage
2 | BK | 550 | Left Rear Heated Seat Ground | 2 | BK | 550 | Left Rear Heated Seat Ground
3 | L-GN | 276 | Control Signal Rearward | 3 | L-GN | 276 | Control Signal Rearward
4 | L-BU | 277 | Control Signal Forward | 4 | L-BU | 277 | Control Signal Forward
5 | PU | 9336 | Control Signal Downward | 5 | PU | 9336 | Control Signal Downward
6 | WH | 9338 | Control Signal Inward | 6 | WH | 9338 | Control Signal Inward
7 | GY | 9337 | Control Signal Outward | 7 | GY | 9337 | Control Signal Outward
8 | BK | 550 | Ground | 5 | BK | 550 | Ground
9 | D-BU | 9335 | Control Signal Upward | 9 | D-BU | 9335 | Control Signal Upward
10 | BN | 341 | Power Supply | 10 | BN | 341 | Power Supply

### C321 Left Rear Seat Cushion to Left Rear Seat Harness (w/o Heated Seat)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Power Supply | 1 | RD/WH | 3740 | Power Supply
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | L-BU | 276 | Rearward Control Signal | 3 | L-BU | 276 | Rearward Control Signal
4 | L-GN | 277 | Forward Control Signal | 4 | L-GN | 277 | Forward Control Signal
5-10 | -- | -- | Not Used | 5-10 | -- | -- | Not Used

### C322 Right Rear Seat Cushion to Right Rear Seat Harness (w/o Heated Seat)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Power Supply | 1 | RD/WH | 3740 | Power Supply
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | L-BU | 277 | Forward Control Signal | 3 | L-BU | 277 | Forward Control Signal
4 | L-GN | 276 | Rearward Control Signal | 4 | L-GN | 276 | Rearward Control Signal

### C322 Right Rear Seat Cushion to Right Rear Seat Harness C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Right Rear Heated Seat Supply Voltage | 1 | RD/WH | 3740 | Right Rear Heated Seat Supply Voltage
2 | BK | 650 | Ground | 2 | BK | 650 | Ground
3 | L-BU | 277 | Control Signal Forward | 3 | L-BU | 277 | Control Signal Forward
4 | L-GN | 276 | Control Signal Rearward | 4 | L-GN | 276 | Control Signal Rearward
5 | PU | 9336 | Control Signal Downward | 5 | PU | 9336 | Control Signal Downward
6 | WH | 9338 | Control Signal Inward | 6 | WH | 9338 | Control Signal Inward
7 | GY | 9337 | Control Signal Outward | 7 | GY | 9337 | Control Signal Outward
8 | D-BU | 9335 | Control Signal Upward | 5 | D-BU | 9335 | Control Signal Upward
9 | BN | 341 | Power Supply | 9 | BN | 341 | Power Supply

### C323 Left Rear Seat Cushion to Left Rear Seat Harness C2

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK | 2077 | Left Rear Heating Element Supply Voltage | 1 | PK | 2077 | Left Rear Heating Element Supply Voltage
2 | BK | 550 | Ground | 2 | BK | 550 | Ground
3 | PK | 2079 | Left Rear Heated Seat Temperature Sensor Signal | 3 | PK | 2079 | Left Rear Heated Seat Temperature Sensor Signal
4 | YE | 2080 | Left Rear Heated Seat Temperature Sensor Low Reference | 4 | YE | 2080 | Left Rear Heated Seat Temperature Sensor Low Reference
5 | OG | 5919 | Left Rear Seat Fan Speed Control | 5 | OG | 5919 | Left Rear Seat Fan Speed Control
6 | BK | 550 | Left Rear Heated Seat Heating Element Control | 6 | BK | 550 | Left Rear Heated Seat Heating Element Control
7 | BN | 1341 | Battery Positive Voltage | 7 | BN | 1341 | Battery Positive Voltage

### C324 Right Rear Seat Cushion to Right Rear Seat Harness C2

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-BU | 2479 | Right Rear Heated Seat Element Supply Voltage | 1 | D-BU | 2479 | Right Rear Heated Seat Element Supply Voltage
2 | GY | 2434 | Right Rear Heated Seat Temperature Sensor Signal | 2 | GY | 2434 | Right Rear Heated Seat Temperature Sensor Signal
3 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference | 3 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference
4 | WH | 5915 | Right Rear Seat Fan Speed Control | 4 | WH | 5915 | Right Rear Seat Fan Speed Control
5 | BN | 2341 | Battery Positive Voltage | 5 | BN | 2341 | Battery Positive Voltage

### C325 Rear Seat Harness to Rear Seatback C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 5150 | Ground | 1 | BK | 5150 | Ground
2 | BK | 650 | Ground | 2 | BK | 650 | Ground
3 | BN | 2341 | Battery Positive Voltage | 3 | BN | 2341 | Battery Positive Voltage
4 | GY | 9337 | Left Rear Heated Seat Outward Control Signal | 4 | GY | 9337 | Left Rear Heated Seat Outward Control Signal
5 | WH | 9338 | Left Rear Heated Seat Inward Control Signal | 5 | WH | 9338 | Left Rear Heated Seat Inward Control Signal
6 | PU | 9336 | Left Rear Heated Seat Downward Control Signal | 6 | PU | 9336 | Left Rear Heated Seat Downward Control Signal
7 | D-BU | 9335 | Left Rear Heated Seat Upward Control Signal | 7 | D-BU | 9335 | Left Rear Heated Seat Upward Control Signal
8 | BN | 341 | Power Supply | 8 | BN | 341 | Power Supply
9 | D-BU | 9335 | Right Rear Heated Seat Upward Control Signal | 9 | D-BU | 9335 | Right Rear Heated Seat Upward Control Signal
10 | PU | 9336 | Right Rear Heated Seat Downward Control Signal | 10 | PU | 9336 | Right Rear Heated Seat Downward Control Signal
11 | WH | 9338 | Right Rear Heated Seat Inward Control Signal | 11 | WH | 9338 | Right Rear Heated Seat Inward Control Signal
12 | GY | 9337 | Right Rear Heated Seat Outward Control Signal | 12 | GY | 9337 | Right Rear Heated Seat Outward Control Signal

### C326 Rear Seat Harness to Rear Seatback C2

#### C325 Rear Seat Harness to Rear Seatback C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | WH | 5915 | Right Rear Seat Fan Speed Control | 1 | WH | 5915 | Right Rear Seat Fan Speed Control
2 | D-BU | 2479 | Right Rear Seat Fan Heating Element Supply Voltage | 2 | D-BU | 2479 | Right Rear Seat Fan Heating Element Supply Voltage
3 | GY | 2434 | Right Rear Seat Fan Temperature Sensor Signal | 3 | GY | 2434 | Right Rear Seat Fan Temperature Sensor Signal
4 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference | 4 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference
5 | OG | 5919 | Left Rear Seat Fan Speed Control | 5 | OG | 5919 | Left Rear Seat Fan Speed Control
6 | BN | 1341 | Battery Positive Voltage | 6 | BN | 1341 | Battery Positive Voltage
7 | PK | 2079 | Left Rear Heated Seat Temperature Sensor Signal | 7 | YE/BK | 2079 | Left Rear Heated Seat Temperature Sensor Signal
8 | PK | 2077 | Left Rear Heated Seat Heating Element Supply Voltage | 8 | PK | 2077 | Left Rear Heated Seat Heating Element Supply Voltage
9 | YE | 2080 | Left Rear Heated Seat Temperature Sensor Signal | 9 | YE | 2080 | Left Rear Heated Seat Temperature Sensor Signal

### C327 Left, Right Rear Seat Harness Connection

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 3740 | Power Supply | 1 | RD/WH | 3740 | Power Supply
2 | BN | 2341 | Battery Positive Voltage | 2 | BN | 2341 | Battery Positive Voltage
3 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference | 3 | PK | 2435 | Right Rear Heated Seat Temperature Sensor Low Reference
4 | GY | 3424 | Right Rear Heated Seat Temperature Sensor Signal | 4 | GY | 3424 | Right Rear Heated Seat Temperature Sensor Signal
5 | D-BU | 2479 | Right Rear Heated Seat Heating Element Supply Voltage | 5 | D-BU | 2479 | Right Rear Heated Seat Heating Element Supply Voltage
6 | WH | 5915 | Right Rear Seat Fan Speed Control | 6 | WH | 5919 | Right Rear Seat Fan Speed Control
7 | GY | 9337 | Right Rear Seat Outward Control Signal | 7 | GY | 9337 | Right Rear Seat Outward Control Signal
8 | WH | 9338 | Right Rear Seat Inward Control Signal | 8 | WH | 9338 | Right Rear Seat Inward Control Signal
9 | PU | 9336 | Right Rear Seat Downward Control Signal | 9 | PU | 9336 | Right Rear Seat Downward Control Signal
10 | D-BU | 9335 | Right Rear Seat Upward Control Signal | 10 | D-BU | 9335 | Right Rear Seat Upward Control Signal
11 | BK | 650 | Ground | 11 | BK | 650 | Ground
12 | BN | 341 | Power Supply | 12 | BN | 341 | Power Supply

### C327 Left, Right Rear Seat Harness Connection

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-5 | -- | -- | Not Used | 1-5 | -- | -- | Not Used
6 | RD/WH | 3740 | Power Supply | 6 | RD/WH | 3740 | Power Supply
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | BK | 550 | Ground | 8 | BK | 550 | Ground

### C329 Rear Seatback Harness to Left Rear Massage Motor Sensor

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 9330 | 5-Volt Power Supply | A | WH | 9330 | 5-Volt Power Supply
B | L-GN | 9177 | Left Rear Massage Sensor INP | B | L-GN | 9177 | Left Rear Massage Sensor INP
C | GY | 9176 | Sensor Low Reference | C | BK | 9176 | Sensor Low Reference
D | D-BU | 9334 | Left Rear Lumbar (UP/DOWN) Low Reference | D | PK | 9334 | Left Rear Lumbar (UP/DOWN) Low Reference
E | PU | 9333 | Left Rear Lumbar (UP/DOWN) Supply Voltage | E | L-BU | 9333 | Left Rear Lumbar (UP/DOWN) Supply Voltage
F | WH | 9338 | Left Rear Lumbar (INWARD/OUTWARD) Motor Low Reference | F | D-GN | 9338 | Left Rear Lumbar (INWARD/OUTWARD) Motor Low Reference
G | GY | 9337 | Left Rear Lumbar (INWARD/OUTWARD) Motor Supply Voltage | G | L-GN | 9337 | Left Rear Lumbar (INWARD/OUTWARD) Motor Supply Voltage
H | -- | -- | Not Used | H | -- | -- | Not Used

### C330 Rear Seatback Harness to Massage Module C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN/BK | 9337 | Right Rear Massage IND | A | RD | 9337 | Right Rear Massage IND
B | L-GN/BK | 9337 | Left Rear Massage IND | B | TN | 9337 | Left Rear Massage IND
C | BN | 341 | Power Supply | C | WH | 341 | Power Supply
D | BK | 550 | Ground | D | BN | 550 | Ground
E | TN | 9170 | Right Rear Massage INP | E | PU | 9170 | Right Rear Massage INP
F | TN | 9170 | Left Rear Massage INP | F | WH | 9170 | Left Rear Massage INP
G | D-BU | 9335 | Right Rear Lumbar Motor Upward Control | G | L-BU | 9335 | Right Rear Lumbar Motor Upward Control
H | PU | 9336 | Right Rear Lumbar Motor Downward Control | H | D-BU | 9336 | Right Rear Lumbar Motor Downward Control
J | D-BU | 9335 | Right Rear Lumbar Motor Upward Control | J | D-GN | 9335 | Right Rear Lumbar Motor Upward Control
K | PU | 9336 | Right Rear Lumbar Motor Downward Control | K | GY | 9336 | Right Rear Lumbar Motor Downward Control
L | WH | 9338 | Right Rear Lumbar (INWARD/OUTWARD) Motor Supply Voltage | L | RD | 9338 | Right Rear Lumbar (INWARD/OUTWARD) Motor Supply Voltage
M | GY | 9337 | Right Rear Lumbar (INWARD/OUTWARD) Motor Low Reference | M | OG | 9337 | Right Rear Lumbar (INWARD/OUTWARD) Motor Low Reference

### C331 Rear Seatback Harness to Massage Module C2

#### C330 Rear Seatback Harness to Massage Module C1

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 9330 | 5V Power Output | A | WH | 9330 | 5V Power Output
B | L-GN | 9177 | Left Rear Massage Sensor INP | B | L-GN | 9177 | Left Rear Massage Sensor INP
C | GY | 9176 | Sensor Low Reference | C | BK | 9176 | Sensor Low Reference
D | D-BU | 9334 | Left Rear Lumbar Motor (UP/DOWN) Low Reference | D | PK | 9334 | Left Rear Lumbar Motor (UP/DOWN) Low Reference
E | PU | 9333 | Left Rear Lumbar Motor (UP/DOWN) Supply Voltage | E | L-BU | 9333 | Left Rear Lumbar Motor (UP/DOWN) Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### C400 Body Harness to Rear Fascia

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series (BK)

#### C400 Body Harness to Rear Fascia

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG | 122 | Rear Fog Lamp Supply Voltage (w/TT7/TT8) | A | OG | 122 | Rear Fog Lamp Supply Voltage (w/TT7/TT8)
B | BK | 1050 | Ground | B | BK | 1050 | Ground
C | PU | 1472 | Left Park Lamp Relay Control (TT7/TT8) | C | PU | 709 | Left Park Lamp Supply Voltage
D | BN/WH | 1473 | Right Park Lamp Supply Voltage (w/TT7/TT8) | D | BN/WH | 309 | Right Park Lamp Supply Voltage

### C401 Body Harness to Rear Fascia (UD7)

#### Connector Part Information

- OEM: 15326835
- Service: 88986452
- Description: 8-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326840
- Service: NS
- Description: 8-Way M GT 150 Series Sealed 4.0 (BK)

#### C401 Body Harness to Rear Fascia (UD7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | YE | 2375 | Left Rear Corner Object Sensor Signal | B | YE | 2375 | Left Rear Corner Object Sensor Signal
C | GY | 2379 | Object Sensor Low Reference | C | GY | 2379 | Object Sensor Low Reference
D | OG | 2376 | Left Rear Middle Object Sensor Signal | D | OG | 2376 | Left Rear Middle Object Sensor Signal
E | D-GN | 2377 | Right Rear Middle Object Sensor Signal | E | D-GN | 2377 | Right Rear Middle Object Sensor Signal
F | PU | 2378 | Right Rear Corner Object Sensor Signal | F | PU | 2378 | Right Rear Corner Object Sensor Signal
G | OG | 5708 | Keyless Entry Antenna Signal (3) | G | OG | 5708 | Keyless Entry Antenna Signal (3)
H | OG/BK | 5712 | Keyless Entry Antenna Low Reference (3) | H | OG/BK | 5712 | Keyless Entry Antenna Low Reference (3)

### C420 Fuel Tank Jumper to Body

#### Connector Part Information

- OEM: 15326660
- Service: 15326907
- Description: 10-Way F GT 280 Series Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 15326661
- Service: 88986245
- Description: 10-Way M GT 280 Series Sealed 5.8 (BK)

#### C420 Fuel Tank Jumper to Body

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 120 | Fuel Pump Supply Voltage | A | GY | 120 | Fuel Pump Supply Voltage
B | D-GN | 890 | Fuel Tank Pressure Sensor Signal | B | D-GN | 890 | Fuel Tank Pressure Sensor Signal
C | GY | 596 | 5-Volt Reference | C | GY | 596 | 5-Volt Reference
D | WH | 1310 | EVAP Canister Vent Solenoid Control | D | WH | 1310 | EVAP Canister Vent Solenoid Control
E | BK | 452 | Low Reference | E | BK | 452 | Low Reference
F | D-BU | 1936 | Fuel Level Sensor Signal Left - Secondary | F | D-BU | 1936 | Fuel Level Sensor Signal Left - Secondary
G | L-BU | 1937 | Fuel Level Sensor Signal Right - Secondary | G | L-BU | 1937 | Fuel Level Sensor Signal Right - Secondary
H | -- | -- | Not Used | H | -- | -- | Not Used
J | RD/WH | 1540 | Battery Positive Voltage | J | RD/WH | 1540 | Battery Positive Voltage
K | BK | 1050 | Ground | K | BK | 1050 | Ground

#### C421 Fuel Tank Filler Door Lock to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 120 | Fuel Tank Filler Door Lock Actuator Unlock Control | A | TN | 120 | Fuel Tank Filler Door Lock Actuator Unlock Control
B | GY | 890 | Fuel Tank Filler Door Lock Actuator Lock Control | B | GY | 890 | Fuel Tank Filler Door Lock Actuator Lock Control

### C500 Body to Left Front Door Harness

#### Connector Part Information

- OEM: 10847017
- Service: NS
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 13510971
- Service: NS
- Description: 14-Way M

#### C500 Body to Left Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 1040 | Battery Positive Voltage | 1 | RD/WH | 1040 | Battery Positive Voltage
2 | RD/WH | 640 | Battery Positive Voltage | 2 | RD/WH | 640 | Battery Positive Voltage
3 | GY | 1690 | Automatic Day/Night Mirror Signal | 3 | GY | 1690 | Automatic Day/Night Mirror Signal
4 | D-BU | 5882 | Left Front Door Handle Switch Signal (2) | 4 | D-BU | 5882 | Left Front Door Handle Switch Signal (2)
5 | PK | 5709 | Keyless Entry Antenna Signal (4) | 5 | PK | 5709 | Keyless Entry Antenna Signal (4)
6 | YE | 1956 | Left Front Tweeter Speaker (-) | 6 | YE | 1956 | Left Front Tweeter Speaker (-)
7 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) (YQ3/YQ4/YQ6/YQ7) | 7 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) (YQ3/YQ4/YQ6/YQ7)
8 | BK | 350 | Ground | 8 | BK | 350 | Ground
9 | BK/WH | 351 | Signal Ground | 9 | BK/WH | 351 | Signal Ground
10 | PK | 1691 | Automatic Day/Night Mirror Low Reference | 10 | PK | 1691 | Automatic Day/Night Mirror Low Reference
11 | D-GN | 5060 | Low Speed GMLAN Serial Data | 11 | D-GN | 5060 | Low Speed GMLAN Serial Data
12 | PK/BK | 5713 | Keyless Entry Antenna Low Reference (4) | 12 | PK/BK | 5713 | Keyless Entry Antenna Low Reference (4)
13 | TN | 1856 | Left Front Tweeter Speaker (+) | 13 | TN | 1856 | Left Front Tweeter Speaker (+)
14 | BK | 850 | Ground (YQ3/YQ4/YQ6/YQ7) | 14 | BK | 850 | Ground (YQ3/YQ4/YQ6/YQ7)

### C501 Left Front Door to Left Front Door Trim Harness

#### Connector Part Information

- OEM: 13530230
- Service: NS
- Description: 12-Way F (BK)

#### Connector Part Information

- OEM: 15448869
- Service: NS
- Description: 12-Way M (BK)

#### C501 Left Front Door to Left Front Door Trim Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | D-GN | 5060 | Low Speed GMLAN Serial Data | 1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | BK/WH | 640 | Battery Positive Voltage | 2 | BK/WH | 640 | Battery Positive Voltage
BK/WH | 640 | Battery Positive Voltage
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) | 4 | PU/WH | 5754 | Amplifier Powered Woofer Control (1)
5 | L-BU/WH | 6576 | Driver Door Courtesy Lamp Control Low | 5 | L-BU/WH | 6576 | Driver Door Courtesy Lamp Control Low
6 | YE | 1491 | Backlight Lamps Control | 6 | YE | 1491 | Backlight Lamps Control
7-8 | -- | -- | Not Used | 7 | -- | -- | Not Used
9 | BK/WH | 351 | Signal Ground | 9 | BK/WH | 351 | Signal Ground
10-12 | -- | -- | Not Used | 10-12 | -- | -- | Not Used

### C600 Body to Right Front Door Harness

#### Connector Part Information

- OEM: 10847017
- Service: NS
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 13510971
- Service: NS
- Description: 14-Way M

#### C600 Body to Right Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 1040 | Battery Positive Voltage | 1 | RD/WH | 1040 | Battery Positive Voltage
2 | RD/WH | 740 | Battery Positive Voltage | 2 | RD/WH | 740 | Battery Positive Voltage
3 | YE | 6817 | Backlight Lamps Control | 3 | YE | 6817 | Backlight Lamps Control
4 | PK | 5879 | Right Front Door Handle Switch Signal (2) | 4 | PK | 5879 | Right Front Door Handle Switch Signal (2)
5 | YE | 5710 | Keyless Entry Antenna Signal (5) | 5 | YE | 5710 | Keyless Entry Antenna Signal (5)
6 | PU | 1952 | Right Front Tweeter Speaker (-) | 6 | PU | 1952 | Right Front Tweeter Speaker (-)
7 | PK/BK | 5755 | Amplifier Powered Woofer (YQ3/YQ4/YQ6/YQ7) | 7 | PK/BK | 5755 | Amplifier Powered Woofer (YQ3/YQ4/YQ6/YQ7)
8 | BK | 450 | Ground | 8 | BK | 450 | Ground
9 | BK/WH | 451 | Signal Ground | 9 | BK/WH | 451 | Signal Ground
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | D-GN | 5060 | Low Speed GMLAN Serial Data | 11 | D-GN | 5060 | Low Speed GMLAN Serial Data
12 | YE/BK | 5714 | Keyless Entry Antenna Low Reference (5) | 12 | YE/BK | 5714 | Keyless Entry Antenna Low Reference (5)
13 | L-GN | 1852 | Right Front Tweeter Speaker (+) | 13 | L-GN | 1852 | Right Front Tweeter Speaker (+)
14 | BK | 850 | Ground (YQ3/YQ4/YQ6/YQ7) | 14 | BK | 850 | Ground (YQ3/YQ4/YQ6/YQ7)

### C601 Right Front Door to Right Front Door Trim Harness

#### Connector Part Information

- OEM: 13530230
- Service: NS
- Description: 12-Way F (BK)

#### Connector Part Information

- OEM: 15448869
- Service: NS
- Description: 12-Way M (BK)

#### C601 Right Front Door to Right Front Door Trim Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU/WH | 5754 | Amplifier Powered Woofer Control (1) | 1 | PU/WH | 5754 | Amplifier Powered Woofer Control (1)
2 | L-BU/WH | 6576 | Driver Door Courtesy Lamp Control Low | 2 | L-BU/WH | 6576 | Driver Door Courtesy Lamp Control Low
3 | YE | 1491 | Backlight Lamps Control | 3 | YE | 1491 | Backlight Lamps Control
3 | YE | 1491 | Backlight Lamps Control
4 | OG | 1189 | Power Window Switch Right Front Low Reference | 4 | OG | 1189 | Power Window Switch Right Front Low Reference
5 | WH | 1185 | Power Window Switch Left Rear Up Signal | 5 | WH | 1185 | Power Window Switch Left Rear Up Signal
6 | L-BU | 244 | Passenger Door Lock Switch Lock Control | 6 | L-BU | 244 | Passenger Door Lock Switch Lock Control
7 | D-BU | 245 | Passenger Door Lock Switch Unlock Control | 7 | D-BU | 245 | Passenger Door Lock Switch Unlock Control
8 | PU | 2765 | Power Window Switch Right Front Express Signal | 8 | PU | 2765 | Power Window Switch Right Front Express Signal
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used
11 | YE | 6817 | Backlight Lamps Control | 11 | YE | 6817 | Backlight Lamps Control
12 | BK/WH | 451 | Ground | 12 | BK/WH | 451 | Ground

### C700 Body to Left Front Door Harness

#### Connector Part Information

- OEM: 10847017
- Service: NS
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 13510971
- Service: NS
- Description: 14-Way M

#### C700 Body to Left Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 1040 | Battery Positive Voltage | 1 | RD/WH | 1040 | Battery Positive Voltage
2 | RD/WH | 840 | Battery Positive Voltage | 2 | RD/WH | 840 | Battery Positive Voltage
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BK/WH | 351 | Ground | 4 | BK/WH | 351 | Signal Ground
5 | WH | 1959 | Left Rear Midrange Speaker Output (-) | 5 | WH | 1959 | Left Rear Midrange Speaker Output (-)
6 | TN | 1859 | Left Rear Midrange Speaker Output (+) | 6 | TN | 1859 | Left Rear Midrange Speaker Output (+)
7 | BK | 350 | Ground | 7 | BK | 350 | Ground
8 | YE | 6817 | Backlight Lamps Control | 8 | YE | 6817 | Backlight Lamps Control
9 | RD/WH | 2040 | Battery Positive Voltage | 9 | RD/WH | 2040 | Battery Positive Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | 11 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
12 | GY | 157 | Interior Lamp Control | 12 | GY | 157 | Interior Lamp Control
13 | D-GN | 5060 | Low Speed GMLAN Serial Data | 13 | D-GN | 5060 | Low Speed GMLAN Serial Data
14 | -- | -- | Not Used | 14 | -- | -- | Not Used

### C701 Left Rear Door to Left Rear Door Trim Harness

#### Connector Part Information

- OEM: 15326110
- Service: NS
- Description: 12-Way F (BK)

#### Connector Part Information

- OEM: 15326942
- Service: NS
- Description: 12-Way M (BK)

#### C701 Left Rear Door to Left Rear Door Trim Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
B | GY | 157 | Interior Lamp Control | B | GY | 157 | Interior Lamp Control
C | YE | 1491 | Backlight Lamps Control | C | YE | 1491 | Backlight Lamps Control
D | BK/WH | 351 | Ground | D | BK/WH | 351 | Ground
E | YE | 1187 | Power Window Switch Left Rear Down Signal | E | YE | 1187 | Power Window Switch Left Rear Down Signal
F | TN | 1859 | Left Rear Midrange Speaker Output (+) | F | TN | 1859 | Left Rear Midrange Speaker Output (+)
G | WH | 1959 | Left Rear Midrange Speaker Output (-) | G | WH | 1959 | Left Rear Midrange Speaker Output (-)
H | D-GN | 1184 | Power Window Switch Right Front Up Signal | H | D-GN | 1184 | Power Window Switch Right Front Up Signal
J | D-GN | 5048 | Power Window Switch Left Rear Express Signal | J | D-GN | 5048 | Power Window Switch Left Rear Express Signal
K | YE | 6817 | Backlight Lamps Control | K | YE | 6817 | Backlight Lamps Control
L | RD/WH | 2040 | Battery Positive Voltage | L | RD/WH | 2040 | Battery Positive Voltage
M | -- | -- | Not Used | M | -- | -- | Not Used

### C800 Body to Right Rear Door Harness

#### Connector Part Information

- OEM: 10847017
- Service: NS
- Description: 14-Way F (L-GY)

#### Connector Part Information

- OEM: 13510971
- Service: NS
- Description: 14-Way M

#### C800 Body to Right Rear Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 1040 | Battery Positive Voltage | 1 | RD/WH | 1040 | Battery Positive Voltage
2 | RD/WH | 840 | Battery Positive Voltage | 2 | RD/WH | 840 | Battery Positive Voltage
3 | TN | 294 | Fuel Tank Cap Unlock Signal | 3 | TN | 294 | Fuel Tank Cap Unlock Signal
4 | BK/WH | 451 | Ground | 4 | BK/WH | 451 | Signal Ground
5 | OG | 1955 | Right Rear Midrange Speaker Output (-) | 5 | OG | 1955 | Right Rear Midrange Speaker Output (-)
6 | TN | 1855 | Right Rear Midrange Speaker Output (+) | 6 | TN | 1855 | Right Rear Midrange Speaker Output (+)
7 | BK | 450 | Ground | 7 | BK | 450 | Ground
8 | YE | 6817 | Backlight Lamps Control | 8 | YE | 6817 | Backlight Lamps Control
9 | RD/WH | 2140 | Battery Positive Voltage | 9 | RD/WH | 2140 | Battery Positive Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | 11 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
12 | GY | 157 | Interior Lamp Control | 12 | GY | 157 | Interior Lamp Control
13 | D-GN | 5060 | Low Speed GMLAN Serial Data | 13 | D-GN | 5060 | Low Speed GMLAN Serial Data
14 | -- | -- | Not Used | 14 | -- | -- | Not Used

### C801 Right Front Door to Right Front Door Trim Harness

#### Connector Part Information

- OEM: 15326110
- Service: NS
- Description: 12-Way F Dock and Lock (BK)

#### Connector Part Information

- OEM: 15326942
- Service: NS
- Description: 12-Way M Dock and Lock (BK)

#### C801 Right Front Door to Right Front Door Trim Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | A | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
B | GY | 157 | Interior Lamp Control | B | GY | 157 | Interior Lamp Control
C | YE | 1491 | Backlight Lamps Control | C | YE | 1491 | Backlight Lamps Control
D | BK/WH | 451 | Ground | D | BK/WH | 451 | Ground
E | OG | 1189 | Power Window Switch Left Rear Down Signal | E | OG | 1189 | Power Window Switch Left Rear Down Signal
F | TN | 1855 | Right Rear Midrange Speaker Output (+) | F | TN | 1855 | Right Rear Midrange Speaker Output (+)
G | OG | 1955 | Right Rear Midrange Speaker Output (-) | G | OG/WH | 1955 | Right Rear Midrange Speaker Output (-)
H | WH | 1185 | Power Window Switch Right Rear Up Signal | H | WH | 1185 | Power Window Switch Right Rear Up Signal
J | D-GN | 5049 | Power Window Switch Right Rear Express Signal | J | D-GN | 5049 | Power Window Switch Right Rear Express Signal
K | YE | 6817 | Backlight Lamps Control | K | YE | 6817 | Backlight Lamps Control
L | RD/WH | 2140 | Battery Positive Voltage | L | RD/WH | 2140 | Battery Positive Voltage
M | -- | -- | Not Used | M | -- | -- | Not Used