For 1990-2009 cars

Connector 1: | Fuse Block - Underhood Label
Connector 2: | Fuse Block - Underhood Top View
Connector 3: | Fuse Block - Underhood Bottom View
Connector 4: | Fuse Block - Underhood C1
Connector 5: | Fuse Block - Underhood C2
Connector 6: | Fuse Block - Underhood C3
Connector 7: | Fuse Block - Underhood C4
Connector 8: | Fuse Block - Underhood C5
Connector 9: | Fuse Block - Left Rear Label
Connector 10: | Fuse Block - Left Rear Top View
Connector 11: | Fuse Block - Left Rear Bottom View
Connector 12: | Fuse Block - C1
Connector 13: | Fuse Block - C2
Connector 14: | Fuse Block C3
Connector 15: | Fuse Block C4
Connector 16: | Fuse Block C5
Connector 17: | Fuse Block C6
Connector 18: | Fuse Block - Right Rear Label
Connector 19: | Fuse Block - Right Rear Top View
Connector 20: | Fuse Block - Right Rear Bottom View
Connector 21: | Fuse Block - Right Rear C1
Connector 22: | Fuse Block - Right Rear C2
Connector 23: | Fuse Block - Right Rear C3
Connector 24: | Fuse Block - Right Rear C5
Connector 25: | Fuse Block - Right Rear C6
Connector 26: | Fuse Block - Right Rear C7
Connector 27: | Fuse Block - Steering Column Fuse Box or Holder

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

Device | Rating | Description
--- | --- | ---
ABS Fuse | 50A | Electronic Brake Control Module (EBCM)
ACCESSORY Relay | -- | RAIN SSR/HDLP WASH , WPR MOD, and WPR SW Fuses
BLOWER Fuse | 40A | BLOWER Relay
BLOWER Relay | -- | Blower Motor Control Module
A/C Control Head Fuse | 10A | HVAC Control Module, Headlamp Level Controller - Export, Adaptive Cruise Control Module w/K59
COMP CLTCH Fuse | 10A | Compressor Clutch
CMP CLU Relay | -- | Compressor Clutch
HDLP WASH Relay C/B | -- | Headlamp Washer Relay
MAF Sensor Fuse | 10A | MAF Sensor
Engine Main Relay | -- | ACCESSORY Relay, Starter Relay, etc.
IPM/Diagnostic Interface Fuse | 10A | IPM and Data Link Connector
ODD COILS Fuse | 15A | Odd Ignition Coils and Odd Fuel Injectors
A/C Control Head Fuse | 10A | HVAC Control Module
ECM/TCM Fuse | 10A | ECM, IPC, RCDLR and TCM
Steering wheel Adjuster Switch | 10A | Tilt/Telescope Switch
V8 ECM Fuse | 10A | Evaporative Emission (EVAP) Canister Purge Solenoid, Electronic Control Module (ECM)
WPR SW Fuse | 7.5A | Wiper Switch
FOG LAMP Fuse | 15A | FOG LAMP Relay
FOG LAMP Relay | -- | Fog Lamps
HDLP WASH C/B | 30A | Headlamp Washer Relay
HFV6 ECM Fuse | 15A | Electronic Control Module (ECM) Ignition 1 Power (LY7)
HIGH BEAM Relay | -- | LT HI BEAM and RT HIGH BEAM Fuses
HIGH FAN Fuse | 30A | HIGH SPEED FAN Relay
HIGH SPEED FAN Relay | -- | Cooling Fan - Right
HORN Fuse | 15A | HORN Relay
HORN Relay | -- | Horns
STARTER Fuse | 30A | Starter Relay
STR RLY Fuse | 10A | Starter Relay
ABS Fuse | 15A | Electronic Brake Control Module (EBCM) Ignition 1 Power Feed
Front Ashtray Fuse | 15A | Front Cigar Lighter
LR Door Cigar Lighter Fuse | 20A | Cigar Lighter - Left Rear
Left Rear Seat Fuse Block Fuse | 60A | Fuse Block - Left Rear Seat
Left Rear Seat Fuse Block Fuse | 60A | Fuse Block - Left Rear Seat
LOW BEAM Relay | -- | LT Low BEAM and RT LOW BEAM Fuses
LOW FAN Fuse | 30A | LOW SPEED FAN Relay
LOW SPEED FAN Relay | -- | Cooling Fan - Left
LT HI BEAM Fuse | 10A | Headlamps - Left
LT LOW BEAM Fuse | 20A | Headlamps - Left
LT PARK LAMP Fuse | 10A | Headlamp - Left, Cornering/Side Marker Lamp - LF, LR and Tail Lamp - Left (Domestic)
RUN/CRANK Relay | -- | Low Speed Fan Relay, High Speed Fan Relay and PRE O2/CAM, POST O2 and Coil (V8 and V6) Fuses
Park Lamp Relay | -- | RT Park Lamp and LIC/IPM Fuses
POST O2 Fuse | 15A | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2, Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2
EVEN COILS Fuse | 15A | Even Ignition Coils/Even Fuel Injectors
PRE O2/CAM Fuse | 15A | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1/Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LH2), Camshaft Position (CMP) Solenoid Exhaust Actuators Bank 1 and Bank 2, Camshaft Position (CMP) Solenoid Intake Actuators Bank 1 and Bank 2 Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1/Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1, Intake Manifold Runner Control (IMRC) Valve, EVAP Canister Purge Valve (LY7)
Headlamp Washer RelayFuse | 7.5A | Headlamp Washer Relay, Rain Sensor and Tire Pressure Monitor Module
Engine Harness Interface | -- | Engine Wiring Harness
Body Harness Interface | -- | Body Harness
Body Harness Interface | -- | Body Harness
Right Rear Seat Fuse Block Fuse | 60A | Fuse Block - Right Rear Seat
Right Rear Seat Fuse Block Fuse | 60A | Fuse Block - Right Rear Seat
RT HIGH BEAM Fuse | 10A | Headlamps - Right
RT LOW BEAM Fuse | 20A | Headlamps - Right
RT PARK LAMP Fuse | 10A | Headlamp - Right, Right Position Lamp Relay (Export), Cornering/Side Marker Lamp - RF, Tail Lamp - Right (Domestic)
Fan Series/Parallel Relay | -- | Cooling Fan
SPARE Fuse | -- | Not Used
SPARE Fuse | -- | Not Used
SPARE Fuse | -- | Not Used
SPARE Fuse | -- | Not Used
TCM/IPC Fuse | 15A | ECM, IPC, and TCM
EXT LIGHTS Fuse | 10A | PARK LAMP, LOW BEAM, HIGH BEAM Relays
VOLT CHECK Fuse | 10A | IPM
Air Quality Sensor Fuse | 10A | Air Quality Sensor
WPR MOD Fuse | 30A | Windshield Wiper/Washer Module
Spare Relay | -- | Not Used
Spare Relay | -- | Not Used

### Fuse Block - Underhood Top View

### Fuse Block - Underhood Bottom View

### Fuse Block - Underhood C1

#### Connector Part Information

- OEM: 135364420
- Service: N/A
- Description: 36-Way F (BK)

#### Fuse Block - Underhood C1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 504 | Cooling Fan Low Reference
2 | GY | 532 | Cooling Fan Motor Supply Voltage
3 | L-BU | 409 | Cooling Fan Motor Supply Voltage
4 | D-GN | 29 | Horn Control - Left
D-GN | 29 | Horn Control - Right
5 | D-GN/WH | 711 | Left Headlamp Integrated Power Supply Voltage
6-7 | -- | -- | Not Used
8 | TN/WH | 312 | Right Headlamp Integrated Power Supply Voltage
9 | YE | 5530 | Hood Open Switch Signal
10 | BN/WH | 309 | Right Side Marker Lamp Supply Voltage
11 | L-BU/WH | 1314 | Left Front Turn Signal/Fog Lamp Supply Voltage
12 | L-BU/WH | 1314 | LH Turn Signal Lamp Supply Voltage
13-16 | -- | -- | Not Used
17 | L-GN/BK | 311 | Right Headlamp Integrated Power Supply Voltage (w/TR7)
18 | L-GN/WH | 6845 | Air Quality NOX Sensor Signal (K14)
19 | PK | 1439 | Ignition 1 Voltage (w/K14)
20 | PU | 1472 | Left Park Lamp Supply Voltage (TT7/TT8)
21 | PU/WH | 5203 | Air Quality Sensor Signal (K14)
22 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
D-BU/WH | 1315 | RH Turn Signal Lamp Supply Voltage
23 | -- | -- | Not Used
24 | PU | 709 | Left Side Marker Lamp Supply Voltage
25-26 | -- | -- | Not Used
27 | PU | 2234 | Front Fog Lamp Supply Voltage
28 | PU | 2234 | Front Fog Lamp Supply Voltage
29 | BK | 250 | Ground
30 | BN/WH | 1473 | Right Park Lamp Supply Voltage (w/TT7/TT8)
31 | RD/WH | 340 | Battery Positive Voltage (w/TR7)
32 | YE | 61 | Low Reference
YE | 61 | Low Reference (K14)
33 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
34 | -- | -- | Not Used
35 | PU | 5531 | Hood Closed Switch Signal
36 | YE | 712 | Left Headlamp Integrated Power Supply Voltage

### Fuse Block - Underhood C2

#### Connector Part Information

- OEM: 10721337
- Service: N/A
- Description: 2-Way F (BK)

#### Fuse Block - Underhood C2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | 2 | Battery Positive Voltage
2 | RD/BK | 2 | Battery Positive Voltage

### Fuse Block - Underhood C3

#### Connector Part Information

- OEM: 10721337
- Service: N/A
- Description: 2-Way F (BK)

#### Fuse Block - Underhood C3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | 2 | Battery Positive Voltage
2 | RD/BK | 2 | Battery Positive Voltage

### Fuse Block - Underhood C4

#### Connector Part Information

- OEM: 13536445
- Service: N/A
- Description: 68-Way F (BK)

#### Fuse Block - Underhood C4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Supply Voltage
2 | -- | -- | Not Used
3 | YE | 32 | Instrument Panel Lamp Fuse Supply Voltage - 1
4 | -- | -- | Not Used
5 | YE | 32 | Rear License Lamp Supply Voltage
6 | RD/WH | 1140 | Battery Positive Voltage
7 | RD/WH | 1140 | Battery Positive Voltage
8 | BN/WH | 1473 | Right Park Lamp Supply Voltage (w/TT7/TT8)
9 | -- | -- | Not Used
10 | RD/WH | 340 | Battery Positive Voltage
11 | YE | 61 | Low Reference
12 | PK | 2039 | ABS Supply Voltage
13 | L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
14 | PU/WH | 5203 | Air Quality Sensor Signal
15 | PU | 5531 | Hood Closed Switch Signal
16 | -- | -- | Not Used
17 | RD/WH | 3540 | Battery Positive Voltage
18 | BN | 247 | Blower Motor Relay Control
19 | -- | -- | Not Used
20 | RD/WH | 1640 | Battery Positive Voltage
21 | WH | 1080 | Park Lamp Relay Control
22 | D-GN/WH | 1317 | Fog Lamp Relay Control
23 | RD/WH | 340 | Battery Positive Voltage
RD/WH | 340 | Battery Positive Voltage (w/TT7/TT8)
24 | -- | -- | Not Used
25 | RD/WH | 2040 | Battery Positive Voltage
26 | RD/BK | 4042 | Battery Positive Voltage (w/TT6/TT7/TT8)
27-29 | -- | -- | Not Used
30 | PK | 1539 | Run/Crank Ignition 1 Voltage
31 | RD/WH | 3340 | Battery Positive Voltage
32 | RD/WH | 1440 | Battery Positive Voltage
33 | RD/WH | 1440 | Battery Positive Voltage
34 | -- | -- | Not Used
35 | YE | 5530 | Hood Open Switch Signal
36 | PK/WH | 1970 | Headlamp Low Beam Relay Control
37 | BN | 4 | Accessory Voltage
38 | -- | -- | Not Used
39 | TN | 28 | Horn Relay Control
40 | -- | -- | Not Used
41 | YE | 43 | Accessory Voltage
42 | PU | 709 | Left Park Lamp Supply Voltage
43 | RD/WH | 1840 | Battery Positive Voltage
44 | PK | 1639 | Run/Crank Ignition 1 Voltage
45 | PK | 839 | Ignition 1 Voltage
46-47 | -- | -- | Not Used
48 | PK | 839 | Ignition 1 Voltage
49-50 | -- | -- | Not Used
51 | L-GN/WH | 6845 | Air Quality NOX Sensor Signal (K14)
52 | RD/WH | 1840 | Battery Positive Voltage
53 | PK | 239 | I/P Supply Voltage
54 | -- | -- | Not Used
55 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
56 | PU | 1472 | Left Park Lamp Supply Voltage (w/TT7/TT8)
57 | L-BU | 188 | Blower Motor Control Processor Supply Voltage
58 | BN/WH | 309 | Right Park Lamp Supply Voltage
59 | YE | 243 | Accessory Voltage (w/TT6/TT7/TT8/CE1)
60-61 | -- | -- | Not Used
62 | YE | 143 | Accessory Voltage
63-66 | -- | -- | Not Used
67 | TN/WH | 1969 | Headlamp High Beam Relay Control (w/o TT6/TT7/TT8)
68 | -- | -- | Not Used

### Fuse Block - Underhood C5

#### Connector Part Information

- OEM: 10864191
- Service: N/A
- Description: 26-Way F (BK)

#### Fuse Block - Underhood C5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | 342 | Battery Positive Voltage
2 | PK/BK | 5290 | Ignition 1 Voltage (w/LY7)
3 | PK/BK | 5294 | Ignition 1 Voltage
4 | D-GN/WH | 459 | A/C Compressor Clutch Relay Control
5 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
6 | PK | 439 | Ignition 1 Voltage (w/LY7)
7 | -- | -- | Not Used
8 | PU | 6 | Starter Solenoid Crank Voltage
9 | PK/BK | 5291 | Ignition 1 Voltage
10 | PK/BK | 5291 | Ignition 1 Voltage (w/LH2/LH1)
11 | PK | 239 | ECM Supply Voltage
12 | PK | 239 | TCM Voltage
13 | PK/BK | 5293 | Ignition 1 Voltage
14 | -- | -- | Not Used
15 | PK/BK | 5290 | Ignition 1 Voltage (w/LH2)
16 | PK/BK | 5290 | Ignition 1 Voltage (w/LH2)
17 | D-BU | 473 | High Speed Cooling Fan Relay Control
18-20 | -- | -- | Not Used
21 | D-GN | 335 | Low Speed Cooling Fan Relay Control
22 | PK/BK | 5292 | Ignition 1 Voltage (w/LH2)
23 | PK/BK | 5292 | Ignition 1 Voltage
24 | YE | 447 | Starter Relay Coil Control
25 | BN | 5069 | MAIN Relay Control
26 | RD/WH | 1440 | Battery Positive Voltage
RD/WH | 1440 | Battery Positive Voltage

### Fuse Block - Left Rear Label

#### Fuse Block - Left Rear Label Usage

Device | Rating | Description
--- | --- | ---
AIRBAG Fuse | 10A | Sensing and Diagnostic Module
Suspension Motor Fuse | 30A | Suspension Relay
Suspension Relay | -- | Suspension Compressor
Suspension Solenoid Fuse | 10A | Suspension Solenoid
AMP Fuse | 30A | Audio Amplifier
Driver Door Module (DDM) Fuse | 15A | Driver Door Module, Speaker - LF Door Subwoofer
Joint Connector | -- | Connector
L Position Relay Micro | -- | Fuse Block Underhood, Cornering/Side Marker Lamp - LR, Turn Signal/Multifunction Switch
Suspension Control Module Fuse | 25A | Suspension Control Module
POSITION LAMPS Fuse | 10A | R POS LP Relay (Export) and L POS LP Relay (Export)
R Position Relay Micro | -- | Fuse Block Underhood, Cornering/Side Marker Lamp - RR, Turn Signal/Multifunction Switch
RR/LR Door Module Fuse | 15A | Left Rear Door Module (LRDM) and Right Rear Door Module (RRDM)
RR Heated Seats Fuse | 20A | Heated Seat Module - RR
Rear Shelf Speaker Fuse | 15A | Speaker - Rear Subwoofer
Backup Lamp Relay | -- | Back Up Lamp
Backup Lamp Fuse | 10A | Backup Lamp Relay
Ignition 3 Relay | -- | Ignition 3 Fuse
Power Seats C/B | 30A | Memory Seat Module - Driver, Seat Adjuster Switch - Passenger, Lumbar Switch - Passenger (AL2)
Park Lamp Relay Micro | -- | R POS LP Relay (Export) and L POS LP Relay (Export)
Automatic Gear Shift Fuse | 10A | Automatic Transmission Shift Lever
Trunk Relay | -- | Not Used
Trunk Compartment Lock Fuse | 7.5A | Trunk Door Release Relay
Rear Seat Entertainment Video Tuner Fuse | 15A | TV Antenna Module (YQ6/YQ7)
LR Heated Seats Fuse | 10A | Heated Seat Module - LR
Rear Seat Massage Fuse | 20A | Rear Seat Massage Module
Rear Seat Heated Switch Fuse | 10A | Rear Seat Heated Module
Driver Seat Module Fuse | 15A | Driver Seat Module
Sun Visor Fuse | 10A | Sun Visor
Spare Relay | -- | Not Used

#### Left Side of the I/P Carrier

(1) | I/P Carrier
(2) | I/P Side Panel - Left
(3) | Data Link Connector (DLC)
(4) | Courtesy Lamp - Left Footwell
(5) | Steering Column Fuse Box or Holder

### Fuse Block - Left Rear Top View

### Fuse Block - Left Rear Bottom View

### Fuse Block - C1

#### Connector Part Information

- OEM: 10721337
- Service: N/A
- Description: 2-Way F (BK)

#### Fuse Block - C1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | 2 | Battery Positive Voltage
2 | RD/BK | 2 | Battery Positive Voltage

### Fuse Block - C2

#### Connector Part Information

- OEM: 13536438
- Service: N/A
- Description: Black Joint Connector

#### Fuse Block - C2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
S1 | BN | 41 | Internal Lines
S2 | BN | 41 | Run Ignition 3 Voltage
S3 | BN | 41 | Run Ignition 3 Voltage
S4 | -- | -- | Not Used
S5 | BN | 41 | Run Ignition 3 Voltage
S6 | BN | 41 | Run Ignition 3 Voltage
S7 | BN | 41 | Run Ignition 3 Voltage
S8-S11 | -- | -- | Not Used
S12 | RD/WH | 840 | Internal Lines
S13 | RD/WH | 840 | Battery Positive Voltage
S14 | RD/WH | 840 | Battery Positive Voltage
S15-S19 | -- | -- | Not Used
S20 | RD/WH | 3640 | Internal Lines
S21 | RD/WH | 3640 | Internal Lines
S22 | RD/WH | 3640 | Battery Positive Voltage
S23 | RD/WH | 3640 | Internal Lines
S24 | L-GN | 24 | Internal Lines
S25 | L-GN | 24 | Backup Lamp Supply Voltage
S26 | L-GN | 24 | Backup Lamp Supply Voltage
S27 | L-GN | 24 | Backup Lamp Supply Voltage
S28 | L-GN | 24 | Backup Lamp Supply Voltage

### Fuse Block C3

#### Fuse Block - C3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
CB1 | RD/WH | 3740 | Battery Positive Voltage
CB2 | -- | -- | Internal Lines

### Fuse Block C4

#### Fuse Block - C4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
FL1 | RD/BK | 1242 | Battery Positive Voltage
FL2 | -- | -- | Internal Lines
FL3 | -- | -- | Internal Lines
FL4 | -- | -- | Internal Lines

### Fuse Block C5

#### Fuse Block - C5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
FU1 | YE | 643 | Battery Positive Voltage
FU2 | -- | -- | Internal Lines
FU3 | RD/WH | 3940 | Battery Positive Voltage
FU4 | -- | -- | Internal Lines
FU5 | RD/WH | 2340 | Battery Positive Voltage
FU6 | -- | -- | Internal Lines
FU7 | RD/WH | 840 | Internal Lines
FU8 | -- | -- | Internal Lines
FU9 | RD/BK | 1342 | Battery Positive Voltage
FU10 | -- | -- | Internal Lines
FU11 | RD/WH | 640 | Battery Positive Voltage
FU12 | -- | -- | Internal Lines
FU13 | RD/WH | 3240 | Battery Positive Voltage
FU14 | -- | -- | Internal Lines
FU15 | BN | 900 | Internal Lines
FU16 | BN | 2341 | Run Ignition 3 Voltage
FU17 | BN | 900 | Internal Lines
FU18 | BN | 341 | Run Ignition 3 Voltage
FU19 | BN | 900 | Internal Lines
FU20 | BN | 1342 | Run Ignition 3 Voltage
FU21 | BN | 900 | Internal Lines
FU22 | BN | 41 | Internal Lines
FU23 | -- | -- | Internal Lines
FU24 | RD/WH | 2440 | Battery Positive Voltage
FU25 | -- | -- | Internal Lines
FU26 | RD/WH | 2840 | Battery Positive Voltage
FU27 | -- | -- | Internal Lines
FU28 | RD/WH | 3640 | Internal Lines
FU29 | -- | -- | Internal Lines
FU30 | D-GN | 901 | Internal Lines
FU31 | -- | -- | Internal Lines
FU32 | RD/WH | 940 | Battery Positive Voltage
FU33 | -- | -- | Internal Lines
FU34 | RD/WH | 905 | Internal Lines

### Fuse Block C6

#### Fuse Block - C6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
R1-R5 | -- | -- | Not Used
R6 | GY | 921 | Internal Lines
R7 | GY | 926 | Internal Lines
R8 | D-GN | 322 | Automatic Level Control Compressor Motor Supply Voltage
R9 | -- | -- | Internal Lines
R10 | YE | 321 | Automatic Level Control Relay Coil Control
R11 | YE/BK | 1418 | Left Rear Turn Signal Switch Signal
R12 | PU | 1472 | Left Park Lamp Relay Control
PU | 1472 | Left Park Lamp Relay Control
R13 | D-GN/WH | 905 | Internal Lines
D-GN/WH | 905 | Internal Lines
R14 | PU | 709 | Left Park Lamp Supply Voltage
R15 | D-GN/WH | 905 | Internal Lines
R16 | D-GN/WH | 1419 | Left Rear Turn Signal Switch Signal
R17 | BN/WH | 1473 | Left Park Lamp Supply Voltage
BN/WH | 1473 | Left Park Lamp Supply Voltage
R18 | D-GN/WH | 905 | Internal Lines
R19 | BN/WH | 309 | Right Park Lamp Supply Voltage
R20 | D-GN/WH | 903 | Internal Lines
D-GN/WH | 904 | Internal Lines
R21 | BK | 850 | Ground
R22 | -- | -- | Internal Lines
R23 | BN/WH | 900 | Internal Lines
R24 | -- | -- | Not Used
R25 | OG | 300 | Run Ignition 3 Voltage
OG | 921 | Run Ignition 3 Voltage
R26 | -- | -- | Internal Lines
R27 | D-GN/WH | 903 | Internal Lines
R28 | -- | -- | Internal Lines
R29 | -- | -- | Internal Lines
R30 | BN/WH | 1429 | Standing Lamp Relay Control
R31 | RD/WH | 3640 | Internal Lines
R32 | RD/WH | 3640 | Internal Lines
R33 | TN/WH | 56 | Trunk Release Motor Supply Voltage
R34 | -- | -- | Not Used
R35 | L-BU | 1344 | Trunk Release Relay Control
R36 | D-GN | 901 | Internal Lines
R37 | D-GN | 901 | Internal Lines
D-GN | 901 | Internal Lines
R38 | L-GN | 24 | Internal Lines
R39 | -- | -- | Not Used
R40 | D-GN | 646 | Reverse Relay Control

### Fuse Block - Right Rear Label

#### Fuse Block - Right Rear Label Usage

Device | Rating | Description
--- | --- | ---
AIRBAG Fuse | 10A | Inflatable Restraint Sensing and Diagnostic Module (SDM)
CANISTER VENT Fuse | 10A | Canister Vent Solenoid
Fuel Pump Fuse | 20A | Fuel Pump Relay
Fuel Pump Relay Micro | -- | Fuel Pump Motor
HTD STG/CLM Fuse | 15A | Heated Steering Wheel Control Module (KA9), Steering Column Lock Control Module (UA2)
INTERIOR LAMP Fuse | 10A | INT LAMP Relay
INT Lamp Relay Micro | -- | RIM, I/P Compartment Lamp, Courtesy Lamp Left and Right Footwells, Courtesy Lamps Left and Right Rear Doors, Overhead Courtesy Lamps Front and Rear and Rear Compartment Lamp
Joint Connector | -- | Connector
LT TURN - RIM Fuse | 10A | Rear Integration Module (RIM)
PSGR DR MOD Fuse | 15A | --
Radio/Clock Fuse | 10A | Radio Module, Clock Module
Cigar Lighter - RR Sear | 15A | Cigar Lighter - RR Seat
Rear Fog Lamp, A/C Compressor Fuse | 10A | Rear Fog Lamp, A/C Compressor
Co-Driver Seat Heated Module Fuse | 20A | Passenger Climate Control Seat Module
Rear Defogger Fuse | 40A | Rear Window Defogger Relay
Rear Defroster Relay Micro | -- | Rear Defogger Element
REAR FOG LAMP Fuse | 10A | REAR FOG LAMP Relay
REAR FOG LAMP Relay Micro | -- | Rear Fog Lamps
RIM Fuse | 10A | Rear Integration Module (RIM), Rear Object Sensor Control Module (UD7), Theft Deterrent Alarm Siren (UA2), Inside Rearview Mirror (ISRVM) and Inflatable Restraint Sensing and Diagnostic Module
RUN/CRANK Relay Micro | -- | RUN/CRANK Elements
Spare Fuse | -- | Not Used
Spare Relay | -- | Not Used
Spare Relay | -- | Not Used
Stop Lamp Fuse | 10A | Stop Lamp Relay
Stop Lamp Relay Micro | -- | Left and Right Tail Lamps
Sunroof Fuse | 20A | Sunroof Control Module
Trunk Diode | -- | Rear Compartment Lamp, Rear Compartment Lid Release Actuator
WINDOW MTRS C/B | 30A | LF, RF, LR, RR Window Regulators
Inside Rearview Mirror, Backup Radar Fuse | 10A | Inside Rearview Mirror, Backup Radar Module

### Fuse Block - Right Rear Top View

### Fuse Block - Right Rear Bottom View

### Fuse Block - Right Rear C1

#### Connector Part Information

- OEM: 10721337
- Service: N/A
- Description: 2-Way F (BK)

#### Fuse Block - Right Rear C1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/BK | 2 | Battery Positive Voltage
2 | RD/BK | 2 | Battery Positive Voltage

### Fuse Block - Right Rear C2

#### Connector Part Information

- OEM: 13536437
- Service: See Catalog
- Description: Black Joint Connector

#### Fuse Block - Right Rear C2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
S1 | PK | 1639 | Internal Lines
S2 | PK | 1639 | Run/Crank Ignition 1 Voltage
S3 | -- | -- | Internal Lines
S4 | BK | 1050 | Internal Lines
S5 | BK | 1050 | Internal Lines
S6 | BK | 1050 | Internal Lines
S7 | BK | 1050 | Ground
S8 | PK | 1339 | Internal Lines
S9 | PK | 1339 | Run/Crank Ignition 1 Voltage
S10 | -- | -- | Not Used
S11 | PK | 1339 | Run/Crank Ignition 1 Voltage
S12 | L-BU | 20 | Internal Lines
S13 | L-BU | 20 | Backup Lamp Supply Voltage
S14 | L-BU | 20 | Backup Lamp Supply Voltage
S15 | RD/WH | 2240 | Internal Lines
S16 | RD/WH | 2240 | Battery Positive Voltage
S17 | RD/WH | 2240 | Battery Positive Voltage
S18 | PK | 1139 | Internal Lines
S19 | PK | 1139 | Run/Crank Ignition 1 Voltage
S20 | PK | 1139 | Run/Crank Ignition 1 Voltage
S21 | PK | 1139 | Run/Crank Ignition 1 Voltage
S22 | PK | 1339 | Internal Lines
S23 | PK | 1339 | Run/Crank Ignition 1 Voltage
S24 | -- | -- | Not Used
S25 | PK | 1339 | Run/Crank Ignition 1 Voltage
S26-S28 | -- | -- | Not Used

### Fuse Block - Right Rear C3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
CB1 | RD/WH | 1040 | Battery Positive Voltage
CB2 | -- | -- | Internal Lines

#### Fuse Block - Right Rear C4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
FD1 | OG/BK | 737 | Trunk Lamp Control
FD2 | OG/BK | 744 | Trunk Ajar Switch Signal
OG/BK | 744 | Trunk Ajar Switch Signal

### Fuse Block - Right Rear C5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
FL1-FL2 | -- | -- | Not Used
FL3 | -- | -- | Internal Lines
FL4 | GY | 911 | Internal Lines

### Fuse Block - Right Rear C6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
FU1 | RD/WH | 1540 | Battery Positive Voltage
FU2 | -- | -- | Internal Lines
FU3 | RD/WH | 540 | Battery Positive Voltage
FU4 | -- | -- | Internal Lines
FU5 | RD/WH | 3640 | Battery Positive Voltage
FU6 | -- | -- | Internal Lines
FU7 | L-BU | 20 | Internal Lines
FU8 | -- | -- | Internal Lines
FU9 | L-GN | 908 | Battery Positive Voltage
FU10 | -- | -- | Internal Lines
FU11 | RD/WH | 2540 | Run/Crank Ignition 1 Voltage
FU12 | -- | -- | Internal Lines
FU13 | RD/WH | 2260 | Internal Lines
FU14 | -- | -- | Internal Lines
FU15 | -- | -- | Internal Lines
FU16 | PK | 1139 | Run/Crank Ignition 1 Voltage
FU17 | GY | 2000 | Internal Lines
FU18 | PK | 1339 | Internal Lines
PK | 1339 | Internal Lines
FU19 | -- | -- | Internal Lines
FU20 | PK | 1639 | Internal Lines
FU21 | -- | -- | Internal Lines
FU22 | PK | 1239 | Run/Crank Ignition 1 Voltage
FU23 | -- | -- | Internal Lines
FU24 | D-BU | 910 | Internal Lines
FU25 | -- | -- | Internal Lines
FU26 | RD/WH | 740 | Battery Positive Voltage
FU27 | -- | -- | Internal Lines
FU28 | RD/WH | 442 | Battery Positive Voltage
FU29 | -- | -- | Internal Lines
FU30 | YE | 909 | Internal Lines
FU31 | -- | -- | Internal Lines
FU32 | RD/WH | 2140 | Battery Positive Voltage
FU33 | -- | -- | Internal Lines
FU34 | RD/WH | 542 | Battery Positive Voltage

### Fuse Block - Right Rear C7

Pin | Wire | Circuit | Function
--- | --- | --- | ---
R1-R5 | -- | -- | Not Used
R6 | OG | 300 | Run/Crank Ignition 3 Voltage
R7 | GY | 911 | Internal Lines
R8 | PU | 293 | Rear Defog Element Supply Voltage
R9 | -- | -- | Not Used
R10 | WH | 193 | Rear Defog Relay Control
R11 | BK | 1050 | Internal Lines
R12 | L-GN | 908 | Internal Lines
R13 | GY | 120 | Fuel Pump Supply Voltage
R14 | -- | -- | Not Used
R15 | D-GN/WH | 465 | Fuel Pump Primary Relay Control
R16 | D-BU | 910 | Internal Lines
R17 | D-BU | 910 | Internal Lines
D-BU | 910 | Internal Lines
R18 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
R19 | -- | -- | Not Used
R20 | D-BU | 1393 | Courtesy Lamp Relay Coil Control
R21 | PK | 3 | Run/Crank Ignition 1 Voltage
R22 | -- | -- | Internal Lines
R23 | GY | 2000 | Internal Lines
R24 | -- | -- | Not Used
R25 | BK | 1050 | Internal Lines
R26-R30 | -- | -- | Not Used
R31 | PK | 1639 | Internal Lines
R32 | YE | 909 | Internal Lines
R33 | OG | 122 | Rear Fog Lamp Supply Voltage
R34 | -- | -- | Not Used
R35 | YE | 1977 | RIM Supply Voltage
R36 | BK | 1050 | Internal Lines
R37 | L-BU | 20 | Internal Lines
R38 | L-BU | 20 | Internal Lines
R39 | -- | -- | Not Used
R40 | WH | 17 | Stop Lamp Switch Signal

### Fuse Block - Steering Column Fuse Box or Holder

#### Fuse Block - Inline Steering Column Usage

No. | Device | Rating | Description
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | Instrument Panel Module | 2A | Remote Radio Control Supply Voltage
3 | Backlight Lamps | 2A | Backlight Lamps Control
4 | Horn | 2A | Horn Relay Control