For 1990-2009 cars

Application | Ref No. | Quantity | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Auxiliary Transmission Oil Cooler Quick Connect Fittings | -- | -- | -- | 25 N·m | 18 lb ft
Auxiliary Transmission Oil Cooler Brace to Skid Bar Bolt | -- | -- | -- | 25 N·m | 18 lb ft
Auxiliary Transmission Oil Cooler Bracket to Body Nuts | -- | -- | -- | 8 N·m | 71 lb in
Auxiliary Transmission Oil Cooler to Bracket Mounting Bolts | -- | -- | -- | 22 N·m | 16 lb ft
Case Extension to Case Assembly | 16 | 6 | M10x1.5x40 | 50 N·m | 37 lb ft
Control Solenoid Valve Assembly and Control Valve Lower Body Assembly to Control Valve Upper Body Assembly | 310 | 6 | M5x0.8x55 | 8 N·m | 71 lb in
Control Solenoid Valve Assembly and Control Valve Lower Body Assembly to Control Valve Upper Body Assembly | 309 | 10 | M5x0.8x45 | 8 N·m | 71 lb in
Control Solenoid Valve Heat Sink to Valve Body | 312 | 2 | M5x0.8x53 | 8 N·m | 71 lb in
Control Valve Upper Body Assembly to Control Valve Lower Body Assembly | 301 | 12 | M5x0.8x36 | 8 N·m | 71 lb in
Control (w/ Body and Valve) Valve Assembly to Case Assembly | 22 | 6 | M5x0.8x73 | 8 N·m | 71 lb in
Fluid Pan Assembly to Case Assembly | 30 | 18 | M6x1.0x20 | 9 N·m | 80 lb in
Fluid Pump Cover Assembly to Torque Converter Housing | 231 | 13 | M6 1.0x40 | 11 N·m | 97 lb in
Input and Output Speed Sensor Assembly to Control Valve Upper Body Assembly | 302 | 2 | M6x1.0x20 | 12 N·m | 106 lb in
Line Pressure Test Hole Plug to Torque Converter Housing | 202 | 1 | 1/8-27 NPTF | 11 N·m | 97 lb in
Manual Shaft Detent Assembly to Valve Body | 23 | 1 | M6x1.0x14.5 | 12 N·m | 106 lb in
Prop Shaft Trans Flange to Output Shaft | 39 | 1 | M22x1.5x14 | 105 N·m | 77 lb ft
Shift Control Assembly to Body Nuts | -- | 4 | -- | 12 N·m | 106 lb in
Shift Control Knob Screw | -- | 1 | -- | 2 N·m | 18 lb in
Shift Control Linkage to Manual Shift Shaft Nut | -- | 1 | -- | 16 N·m | 142 lb in
Shift Control Linkage to Shift Control Assembly Nut | -- | 1 | -- | 16 N·m | 11 lb in
Torque Converter Housing Assembly to Case Assembly | 3 | 9 | M10x1.5x50 | 72 N·m | 53 lb ft
Torque Converter to Flywheel Bolts | -- | 3 | -- | 63 N·m | 46 lb ft
Trans Oil Level Check Plug to Fluid Pan Assembly | 31 | 1 | M12x1.75 | 25 N·m | 18 lb ft
Transmission Oil Cooler Pipe Clip to Oil Pan Nuts | -- | -- | -- | 25 N·m | 18 lb in
Transmission Oil Cooler Pipe Clip to Torque Tube Bolts | -- | -- | -- | 12 N·m | 106 lb in
Transmission Oil Cooler Pipes to Transmission Bolt | -- | -- | -- | 25 N·m | 18 lb ft
Transmission to Engine Block Bolts | -- | 10 | -- | 50 N·m | 37 lb ft
Transmission Support Assembly to Body Bolts | -- | 2 | -- | 58 N·m | 43 lb ft
Transmission Support Assembly to Transmission Bolts | -- | 2 | -- | 63 N·m | 46 lb ft
*Reference number refers to the component callout number in Disassembled Views