For 1990-2009 cars

#### Repair Materials - Flexible Plastic Part

Thermoset Plastic Type | Repair Type | Recommended Repair Material | Availability
--- | --- | --- | ---
Most flexible and semi flexible plastics* | Most repairs* | GM Goodwrench Compoxy repair materials (GM P/N 12377980* or equivalent) | Shanghai general Motors ASCs/Dealers
GM-8 Compoxy repair materials (GM P/N 82091* or equivalent) | Consult the local paint supplier
* TPO, TEO (Polyolefin Plastics) require the application of GM P/N 1052364 polyolefin adhesive primer before the GM P/N 12377980 repair compound is applied.