For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the transmission. Refer to Transmission Replacement .

1 | Torque Converter Assembly Tip

• | Place a drain pan under the front of the transmission.

• | Use care not to damage the torque converter seal during the installation procedure.

• | Rotate the torque converter assembly in order to engage the input shaft, the stator shaft, and the lugs onto the oil pump drive gear.