For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Pump Rotor Cavity Tip Measure the distance from the bottom of the gage bar to the bottom of the pump rotor cavity. Refer to Fluid Pump Selective Specifications .
2 | A/Trans Fluid Pump Rotor Tip Refer to Fluid Pump Selective Specifications to select the correct rotor.
3 | A/Trans Fluid Pump Slide Tip Refer to Fluid Pump Selective Specifications to select the correct slide.