For 1990-2009 cars

Table 1: | Driver Door Module (DDM) Scan Tool Output Controls
Table 2: | Left Rear Door Module (LRDM) Scan Tool Output Controls
Table 3: | Passenger Door Module (PDM) Scan Tool Output Controls
Table 4: | Right Rear Door Module (RRDM) Scan Tool Output Controls

The Scan Tool Output Controls for the following control modules is located in the Special Functions section of the Scan Tool Menu.

#### Driver Door Module (DDM) Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Special Functions | Door Deadbolt Lock/Unlock | When Lock Deadbolt is selected, the DDM momentarily pulses the driver door deadbolt motor, locking the driver door. When Unlock Deadbolt is selected, the DDM momentarily pulses the driver door deadbolt motor, unlocking the driver door.
Special Functions | Door Switch Backlight | When On is selected, the DDM turns the backlighting on the switches on the drivers door ON.
Special Functions | Driver Mirror Horizontal Motor | When Left is selected, the DDM powers the driver mirror in the Left direction for approximately 5 seconds. When Right is selected, the DDM powers the driver mirror in the Right direction for approximately 5 seconds.
Special Functions | Driver Mirror Vertical Motor | When Up is selected, the DDM powers the driver mirror in the Up direction for approximately 5 seconds. When Down is selected, the DDM powers the driver mirror in the Down direction for approximately 5 seconds.
Special Functions | Driver Window Motor | When Up is selected, the DDM commands the driver door window motor in the Up direction for approximately 5 seconds. When Down is selected, the DDM commands the driver door window motor in the Down direction for approximately 5 seconds.
Special Functions | Exterior Courtesy Lamp | When On is selected, the DDM turns the exterior courtesy lamp located on the bottom edge of the drivers door ON.
Special Functions | LF Latch Solenoid Switch | When On is selected, the DDM momentarily pulses the driver door latch motor. When Off is selected, the DDM momentarily pulses the driver door latch motor.
Special Functions | Door Lock Switch Indicator | When On is selected, the DDM turns the driver door lock switch indicator On.
Special Functions | Mirror Fold | When In is selected, the DDM powers the driver mirror to fold to the In position. When Out is selected, the DDM powers the driver mirror to fold to the Out position.
Special Functions | Mirror Heater | When On is selected, the DDM turns On the driver mirror heating element for approximately 5 seconds.

#### Left Rear Door Module (LRDM) Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Special Functions | Door Deadbolt Lock/Unlock | When Lock Deadbolt is selected, the LRDM momentarily pulses the left rear deadbolt motor, locking the left rear door. When Unlock Deadbolt is selected, the LRDM momentarily pulses the left rear deadbolt motor, unlocking the left rear door.
Special Functions | Door Lock/Unlock | When Lock is selected, the LRDM momentarily pulses the left rear door lock motor, locking the left rear door. When Unlock is selected, the LRDM momentarily pulses the left rear door lock motor, unlocking the left rear door.
Special Functions | Door Switch Backlight | When On is selected, the LRDM turns the backlighting on the left rear door switches On.
Special Functions | Window Up/Down | When Up is selected, the LRDM commands the driver door window motor in the Up direction for approximately 5 seconds. When Down is selected, the LRDM commands the driver door window motor in the Down direction for approximately 5 seconds.

#### Passenger Door Module (PDM) Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Special Functions | Door Deadbolt Lock/Unlock | When Lock Deadbolt is selected, the PDM momentarily pulses the passenger door deadbolt motor, locking the passenger door. When Unlock Deadbolt is selected, the PDM momentarily pulses the passenger door deadbolt motor, unlocking the passenger door.
Special Functions | Door Switch Backlight | When On is selected, the PDM turns the backlighting on the switches on the passenger door ON.
Special Functions | Exterior Courtesy Lamp | When On is selected, the PDM turns the exterior courtesy lamp located on the bottom edge of the passenger door ON.
Special Functions | Front Passenger Window Motor | When Up is selected, the PDM commands the passenger door window motor in the Up direction for approximately 5 seconds. When Down is selected, the PDM commands the passenger door window motor in the Down direction for approximately 5 seconds.
Special Functions | Door Lock Switch Indicator | When On is selected, the PDM turns the passenger door lock switch indicator On.
Special Functions | Mirror Fold | When In is selected, the PDM powers the passenger mirror to fold to the In position. When Out is selected, the PDM powers the passenger mirror to fold to the Out position.
Special Functions | Mirror Heater | When On is selected, the PDM turns On the driver mirror heating element for approximately 5 seconds.
Special Functions | Psgr. Mirror Horizontal Motor | When Left is selected, the PDM powers the passenger mirror in the Left direction for approximately 5 seconds. When Right is selected, the PDM powers the passenger mirror in the Right direction for approximately 5 seconds.
Special Functions | Psgr. Mirror Vertical Motor | When Up is selected, the PDM powers the passenger mirror in the Up direction for approximately 5 seconds. When Down is selected, the PDM powers the passenger mirror in the Down direction for approximately 5 seconds.
Special Functions | RF Latch Solenoid | When On is selected, the PDM momentarily pulses the passenger door latch motor. When Off is selected, the PDM momentarily pulses the passenger door latch motor.

#### Right Rear Door Module (RRDM) Scan Tool Output Controls

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Special Functions | Door Deadbolt Lock/Unlock | When Lock Deadbolt is selected, the RRDM momentarily pulses the right rear deadbolt motor, locking the right rear door. When Unlock Deadbolt is selected, the RRDM momentarily pulses the right rear deadbolt motor, unlocking the right rear door.
Special Functions | Door Lock/Unlock | When Lock is selected, the RRDM momentarily pulses the right rear door lock motor, locking the right rear door. When Unlock is selected, the RRDM momentarily pulses the right rear door lock motor, unlocking the right rear door.
Special Functions | Door Switch Backlight | Backlight When On is selected, the RRDM turns the backlighting on the right rear door switches On.
Special Functions | Window Up/Down | When Up is selected, the RRDM commands the right rear door window motor in the Up direction for approximately 5 seconds. When Down is selected, the RRDM commands the right rear door window motor in the Down direction for approximately 5 seconds.