For 1990-2009 cars

Callout | Component Name
--- | ---
1 | NEW Fluid Pump Seal Assembly
2 | NEW Fluid Pump Seal Assembly
3 | NEW Center Support Fluid Passage Seal Assembly
4 | Control Valve Body Assembly Tip Align the manual shift shaft position switch activator slide with the detent lever guide pin.
5 | Notice: Refer to Fastener Notice in the Preface section. Bolt M5 x 73 (Qty: 6)

#### Procedure

Tighten the bolts in the sequence shown

Tighten
8 N·m (71 lb in)