For 1990-2009 cars

### Removal Procedure

1. Remove the bridge console. Refer to Front Floor Console Extension Replacement - Center.
2. Remove the bolts securing the rear of the compartment to the bridge console.
3. Remove the bridge console compartment.

### Installation Procedure

1. Install the bridge console compartment.
2. Install the bolts securing the rear of compartment to the bridge console.
3. Install the bridge console. Refer to Front Floor Console Extension Replacement - Center.