For 1990-2009 cars

## Rear Seat Roof Illuminated Mirror Replacement Bulb

### Removal Procedure

1. Pry the courtesy lamp cover.
2. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Install the courtesy lamp cover.

## Rear Seat Roof Illuminated Mirror Replacement Mirror

### Removal Procedure

1. Pry the courtesy lamp cover.
2. Open the vanity mirror and remove the interior trim panel.
3. Remove the 4 nuts attaching the vanity mirror to the roof.
4. Pry the vanity mirror bezel frame and disconnect the connectors.

### Installation Procedure

1. Install the vanity mirror to the roof and connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Tighten the fastening nuts of the vanity mirror.

Tighten
Tighten to 3.5 N·m (32 lb in).

3. Install Trim Panel.
4. Install the courtesy lamp cover.