For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Interior Lights Schematics Connector End View Reference: Master Electrical Component List
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Inspect for poor connections at the harness connector of the vanity mirror lamp. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 4 | Go to Step 3
3 | Replace the sunshade. Refer to Sunshade Replacement . Did you complete the replacement? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2