For 1990-2009 cars

## Power Steering Fluid Cooler Replacement LY7

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Place a drain pan under the vehicle.
4. Remove the power steering cooler bolts from the power steering cooler brackets.
5. Disconnect the power steering lines from the power steering cooler.
6. Remove the power steering fluid cooler from the vehicle.

### Installation Procedure

1. Install the power steering cooler to the vehicle.
2. Connect the power steering lines to the power steering cooler.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the power steering cooler bolts to the power steering cooler brackets.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

4. Remove the drain pan from under the vehicle.
5. Install the front air deflector. Refer to Front Air Deflector Replacement.
6. Lower the vehicle.
7. Bleed the power steering system. Refer to Power Steering System Bleeding.

## Power Steering Fluid Cooler Replacement LH2

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.
3. Place a drain pan under the vehicle.
4. Remove the power steering cooler bolts from the power steering cooler brackets.
5. Disconnect the power steering lines from the power steering cooler.
6. Remove the power steering fluid cooler from the vehicle.

### Installation Procedure

1. Install the power steering cooler to the vehicle.
2. Connect the power steering lines to the power steering cooler.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the power steering cooler bolts to the power steering cooler brackets.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

4. Remove the drain pan from under the vehicle.
5. Install the front air deflector. Refer to Front Air Deflector Replacement.
6. Lower the vehicle.
7. Bleed the power steering system. Refer to Power Steering System Bleeding.