For 1990-2009 cars

Callout | Component Name
--- | ---
1 | NEW Fluid Pump Seal
2 | Torque Converter (with Fluid Pump) Housing Assembly Notice: Ensure the turbine shaft (O-ring) seal is not installed prior to installing the torque converter housing assembly. The seal may become cut or damaged during installation of the torque converter housing assembly.
3 | Bolts M10x 50 (Qty: 9) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Tighten the bolts in the sequence show.

Tighten
72 N·m (53 lb ft)

4 | NEW Turbine Shaft (O-Ring) Seal