For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AE5 | Lock Control, Remote Entry, Low Power, Start
AL2 | Control Seat with Power Lumbar
AQ9 | Front Seat, Buckle, Luxury
AU8 | Lock Control, Remote Entry, Specific Frequency
AX4 | Restraint Conversion Seat, MAN, European
AY0 | Seat Airbag System, Driver and Passenger, Front/Side/Roof
A26 | Window European Glazing, All
A45 | Memory Seat Adjuster Mirror, Power, Driver and Personalization
A82 | Restraint Head
BAG | Parts Package, Export
B19 | Ornamentation INTR, Customs
B20 | Ornamentation Intr, Luxury
B57 | Ornamentation Extra, Deluxe
CE1 | Wiper System Windshield, Pulse, Moisture Sensitive
CE4 | Washer Headlamp, High Pressure
CF5 | Sunroof Glass, Sliding Electric
CJ2 | HVAC Front Air Conditioner, Auto TEMP CONT, AUX TEMP CONT
DD7 | Mirror I/S R/V LT Sensitive, Compass
DD8 | Mirror I/S R/V LT Sensitive
DL7 | Mirror O/S LH and RH, Remote Control, Heated Power Folding, Color
DR2 | Mirror O/S LH and RH, Remote Control, Heated Light Sensitive, Manual Folding, Color
DT4 | Ashtray Cigarette Lighter
FE1 | Suspension System Soft Ride
FE3 | Suspension System Soft Ride
F55 | Chassis Continuously Variable Real Time Damping Magneto Rheological
GU2 | Rear Axle 2.73 Ratio
GU5 | Rear Axle 3.23 Ratio
GU6 | Rear Axle 3.42 Ratio
G80 | Axle Location Skid Prevention
JE2 | Braking Lining Driving Performance
JE5 | Brake System Power, Antilock, Front and Rear Wheel
JJA | PT Dress Subassembly Installed (Modular Optimization Method Only)
JL4 | Controllable Active Brake
JL9 | Brake System Power, Front and Rear Disc, Antilock, Front and Rear Wheel
JNG | Drive Shaft Painted
KA1 | Front Heated Seat
KA3 | Heater Engine Block, 220V
KA6 | Heated Seat, Rear
KB6 | Heated Seat, Cooling, Front
KG4 | Generator 150 AMP
K05 | Heater, Engine Cylinder Block
K14 | Air Filter, Auto Recirculating
K59 | Cruise Control Automatic Adaptive
LAL | Plant Code - Lansing, MI USA (Grand River)
LH2 | Engine Oil, 8 Cyl, 4.6L, SFI, V8, DOHC, HO, Alum, GM
LY7 | Engine Oil, 6 CYL, 3.6L, SFI, V6, Alum, 60 Degrees, GM
MTF | Provisions Fire Extinguisher Mounting
M22 | HMD 6L50-E PTU Transmission Auto 5 Speed, Electronic
M82 | HMD 5L40-E Transmission Auto 5 Speed, Electronic
NA3 | Emission System Japan
NC1 | Emission System California (LEV)
NF9 | Emission System General Unleaded
NP5 | Steering Wheel Leather Wrapped
NR7 | Steering Wheel Leather Wrapped, Heated
NT4 | Emission System EEC 05
NT7 | Emission System Federal, TIER 2
NT9 | Emission System Federal, TIER 2 Phase-Out
NU1 | Emission System California, LEV2
NU4 | Emission System California, LEV II Plus
NV7 | Steering Power, Variable Effort
N05 | Lock Control Fuel Filler Cap
N30 | Steering Wheel Deluxe
N31 | Steering Wheel Heated
N87 | Wheel 18 x 8, Aluminum
N88 | Wheel 17 x 7.5, Aluminum, Premium
QKP | Tire All P235/50R17_95S BW R/PE ST TL ALS
Q11 | Tire All P235/50R17 Front and P255/45R17 Rear
Q12 | Tire All P235/50R17 Front and P255/45R17 Rear
Q13 | Wheel 17 x 7.5 Front and 17 x 8.0 Rear (Polished)
Q14 | Wheel 17 x 7.5 Front and 17 x 8.0 Rear (Painted)
TQ5 | Control Intelligent High Beam
TR7 | Headlamps Control Leveling System, Automatic
TT6 | Headlamps High Intensity Discharge
TT7 | Headlamps High Intensity Discharge, LH Rule of Road
TT8 | Headlamps High Intensity Discharge, RH Rule of Road
T2H | Specific External Requirements, Export
T43 | Spoiler Rear
T62 | Lighting Daytime Running
T65 | Lamp System Daytime Running, Export
T79 | Rear Fog Lamps
T84 | Headlamps RH Rule of the Road, E Mark
T90 | Signal Lamp and Width Indicator, Export
UA2 | Theft Deterrent System Export Specific
UA6 | Theft Deterrent System
UD7 | Rear Parking Auxiliary System Sensor Indicator
UE1 | Communication System Vehicle, G. P. S. 1
UG1 | Garage Door Opener Universal
UH3 | Indicator Low Tire Pressure, Var 2
UJ6 | Indicator Low Tire Pressure
UJ9 | Indicator Low Tire Pressure, Var 1
UQ7 | Speaker System, Audio Performance Reinforced, Bose
UV6 | Display Head Up
UX8 | Speaker System 8 Deluxe
UY5 | Speaker System 15 Deluxe
U19 | Speedometer, INST, Kilo and Miles, KILO Odometer
U2K | Digital Audio System, S-Band
U2L | Digital Audio System, L-Band
U30 | Cluster INST, TACH, Clock
VBX | Language Label, Arabic
VB1 | Label Shipping, Japan
VC4 | Label Price/Fuel Econ, Puerto Rico and Virgin Islands
VC5 | Label Shipping, Except US, US Possessions, or Japan
VG8 | Label Vehicle Buyer Precautions
VH5 | Plate Vehicle Identification
VJ1 | License Plate - Rear Mounting Package, Japan
VJ2 | Label, Headlamp Adjust Export
VJ4 | Label Location Child Restraint, Export
VL2 | Label, Spare Caution, Compact Spare
VL4 | License Plate Front Mounting Package, EEC
VL6 | License Plate - Front Mounting PKG, Japan
VMA | License Plate - Front Mounting PKG, Korea
VP6 | Noise Control
VR5 | Provisions Slow Vehicle Warning Triangle Mounting
VU9 | Provisions Flasher Installed
VZ3 | Label Mercury Disposal Notification
V03 | Cooling System Extra Capacity
V08 | Cooling System High Duty
V73 | Vehicle Statement USA/Canada
V76 | Hook Tow
V78 | Vehicle Statement
V87 | Vehicle Statement, Gulf States Organization
V92 | Trailer Provisions
XA7 | Washer Nozzles, Heated, Windshield
YQ1 | Infotainment System 009
YQ2 | Infotainment System 010
YQ3 | Infotainment System 011
YQ4 | Infotainment System 012
YQ6 | Infotainment System 014
YQ7 | Infotainment System 015
Z49 | Positive Conversion Equipment Canada, Export
Z5X | Mirror Provisions Arabic Language
Z5Y | Mirror Provisions O/S Etched Warning