For 1990-2009 cars

## Generator Bracket Replacement LY7

### Removal Procedure

1. Turn OFF the ignition.
2. Remove the generator. Refer to Generator Replacement.
3. Remove the coolant inlet pipe lower bolt from the generator bracket.
4. Remove the belt tensioner. Refer to Drive Belt Tensioner Replacement - Generator.
5. Remove the generator bracket bolts.
6. Remove the generator bracket.

### Installation Procedure

1. Install the generator bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the generator bracket bolts and tighten in the sequence shown.

2.1. | Tighten the generator bracket bolts (1, 2) to 50 N·m (37 lb ft).

2.2. | Tighten the generator bracket bolt (3) to 23 N·m (17 lb ft).

3. Install the belt tensioner. Refer to Drive Belt Tensioner Replacement - Generator.
4. Install the coolant inlet pipe lower bolt from the generator bracket.
5. Install the generator. Refer to Generator Replacement.

## Generator Bracket Replacement LH2

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the generator. Refer to Generator Replacement.
3. Remove the generator drive belt tensioner. Refer to Drive Belt Tensioner Replacement - Generator.
4. Remove the right side engine mount bracket. Refer to Engine Mount Bracket Replacement - Right Side.
5. Remove the generator bracket bolts (1, 2 and 3).
6. Remove the generator bracket from the engine.

### Installation Procedure

1. Install the generator bracket to the engine.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the generator bracket bolts in the sequence shown and tighten to 50 N·m (37 lb ft).
3. Install the right side engine mount bracket. Refer to Engine Mount Bracket Replacement - Right Side.
4. Install the generator drive belt tensioner. Refer to Drive Belt Tensioner Replacement - Generator.
5. Install the generator. Refer to Generator Replacement.
6. connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.